(footprint "QFN-14-1EP_2.5x3mm_EP1.15x1.65mm_ONSemi_MLP14A"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.onsemi.cn/pub/Collateral/510CB.PDF")
	(property "Reference" "REF**"
		(at 0 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-14-1EP_2.5x3mm_EP1.15x1.65mm_ONSemi_MLP14A"
		(at 0 2.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.75 4.291 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.75 5.541 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.75 6.791 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.25 -1.46 90)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "2" smd roundrect
		(at -1.21 -1 180)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "3" smd roundrect
		(at -1.21 -0.501 180)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "4" smd roundrect
		(at -1.21 0 180)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "5" smd roundrect
		(at -1.21 0.499 180)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "6" smd roundrect
		(at -1.21 0.999 180)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "7" smd roundrect
		(at -0.25 1.459 270)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "8" smd roundrect
		(at 0.248 1.459 270)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "9" smd roundrect
		(at 1.209 0.999)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "10" smd roundrect
		(at 1.209 0.499)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "11" smd roundrect
		(at 1.209 0)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "12" smd roundrect
		(at 1.209 -0.501)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "13" smd roundrect
		(at 1.209 -1)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "14" smd roundrect
		(at 0.248 -1.46 90)
		(size 0.78 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07)
	)
	(pad "15" smd rect
		(at -0.002 0 90)
		(size 1.65 1.15)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_74lcx07bqx.glb"
		(offset
			(xyz 0.0005 -0.001 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
