(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC06ABQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC06ABQ"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC06ABQ"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74LVC06A.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Hex inverter with open-drain outputs"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC06ABQ"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, INVERTER, TRANSCEIVER, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC06ABQ_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "1A")
					(number "1")
				)
				(pin open_collector line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "1Y")
					(number "2")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "2A")
					(number "3")
				)
				(pin open_collector line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "2Y")
					(number "4")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "3A")
					(number "5")
				)
				(pin open_collector line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "3Y")
					(number "6")
				)
				(pin passive line
					(at 17.78 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin open_collector line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "4Y")
					(number "8")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "4A")
					(number "9")
				)
				(pin open_collector line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "5Y")
					(number "10")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "5A")
					(number "11")
				)
				(pin open_collector line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "6Y")
					(number "12")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "6A")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "14")
				)
				(pin power_in line
					(at 17.78 -21.59 180)
					(length 2.54)
					(name "GND")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
