(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC1G123DP,125"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC1G123DP,125"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC1G123DP,125"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/916/74LVC1G123-1388973.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Monostable Multivibrator, 74LVC1G123, 50 mA, 1.65 V to 5.5 V, TSSOP-8"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC1G123DP,125"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC1G123DP,125_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{A}")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{CLR}")
					(number "3")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin output line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "Q")
					(number "5")
				)
				(pin passive line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "C_{EXT}")
					(number "6")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "R_{EXT}/C_{EXT}")
					(number "7")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "V_{CC}")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
