(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC1G14FW4-7"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC1G14FW4-7"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC1G14FW4-7"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/115/DIOD_S_A0009369123_1-2543295.pdf"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Buffer, Schmitt-trigger inverter, 74LVC1G14, 1.65 V to 5.5 V, DFN1010-6"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC1G14FW4-7"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, BUFFER, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC1G14FW4-7_0_0"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
			)
			(symbol "74LVC1G14FW4-7_0_1")
			(symbol "74LVC1G14FW4-7_1_1"
				(pin no_connect line
					(at 15.24 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "Y")
					(number "4")
				)
				(pin no_connect line
					(at 15.24 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
