(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC1G175_SOT457"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC1G175_SOT457"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC1G175_SOT457"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/916/74LVC1G175-1480578.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Flip-Flop, Non Inverted, Positive Edge, 74LVC1G175, D, 300 MHz, 50 mA, SC-74"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC1G175GV,125"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, GATE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC1G175_SOT457_1_1"
				(pin input clock
					(at 0 -2.54 0)
					(length 2.54)
					(name "CLK")
					(number "1")
				)
				(pin power_in line
					(at 7.62 -10.16 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "D")
					(number "3")
				)
				(pin output line
					(at 15.24 0 180)
					(length 2.54)
					(name "Q")
					(number "4")
				)
				(pin power_in line
					(at 7.62 5.08 270)
					(length 2.54)
					(name "VCC")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{CLR}")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
