(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC1T45GM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC1T45GM"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC1T45GM"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn74lvc1t45"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Transceiver, Translating, 74LVC1T45, 74LVC Family, 1.2V to 5.5V Supply, XSON-6"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC1T45GM-Q100X"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC1T45GM_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCA")
					(number "1")
				)
				(pin power_in line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A")
					(number "3")
				)
				(pin bidirectional line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "B")
					(number "4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DIR")
					(number "5")
				)
				(pin power_in line
					(at 16.51 0 180)
					(length 2.54)
					(name "VCCB")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
