(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC2G07_SOT457"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 29.21 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC2G07_SOT457"
				(at 29.21 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC2G07_SOT457"
				(at 29.21 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.tme.eu/Document/2ad9356043a4952b9021ef50162f8c34/74LVC2G07.pdf"
				(at 29.21 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Buffer, Non-Inverting 2 Element 1 Bit per Element Open Drain Output 6-TSOP"
				(at 29.21 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Nexperia"
				(at 29.21 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC2G07GV,125"
				(at 29.21 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 29.21 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 29.21 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, BUFFER, TRANSCEIVER, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SG-74 SOT23-6 TSOP6 SOT457"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC2G07_SOT457_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin output line
					(at 12.7 -8.89 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin power_in line
					(at 0 1.27 0)
					(length 2.54)
					(name "V_{CC}")
					(number "5")
				)
				(pin output line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
