(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74LVC2G14_SOT457"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74LVC2G14_SOT457"
				(at 30.48 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74LVC2G14_SOT457"
				(at 30.48 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74LVC2G14.pdf"
				(at 30.48 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Logic IC, Inverter, Dual, 1 Inputs, 6 Pins, TSOP, 74LVC2G14"
				(at 30.48 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74LVC2G14GV,125"
				(at 30.48 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 30.48 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, BUFFER, TRANSCEIVER, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74LVC2G14_SOT457_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin power_in line
					(at 7.62 -16.51 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin output line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin power_in line
					(at 7.62 8.89 270)
					(length 2.54)
					(name "VCC")
					(number "5")
				)
				(pin output line
					(at 15.24 0 180)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
