(footprint "DHVQFN-20-1EP_2.5x4.5_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "DHVQFN-20-1EP_2.5x4.5_P0.5mm"
		(at 0 3.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -1.95 5.849 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.95 7.049 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.95 8.249 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.248 -2.261)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "2" smd rect
		(at -1.26 -1.75 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "3" smd rect
		(at -1.26 -1.25 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "4" smd rect
		(at -1.26 -0.75 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "5" smd rect
		(at -1.26 -0.25 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "6" smd rect
		(at -1.26 0.247 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "7" smd rect
		(at -1.26 0.747 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "8" smd rect
		(at -1.26 1.249 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "9" smd rect
		(at -1.26 1.749 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "10" smd rect
		(at -0.248 2.15)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "11" smd rect
		(at 0.249 2.15)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "12" smd rect
		(at 1.259 1.749 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "13" smd rect
		(at 1.259 1.249 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "14" smd rect
		(at 1.259 0.747 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "15" smd rect
		(at 1.259 0.247 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "16" smd rect
		(at 1.259 -0.25 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "17" smd rect
		(at 1.259 -0.75 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "18" smd rect
		(at 1.259 -1.25 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "19" smd rect
		(at 1.259 -1.75 90)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "20" smd rect
		(at 0.249 -2.261)
		(size 0.29 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "21" smd rect
		(at 0 0 180)
		(size 0.9 2.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.5)
	)
	(embedded_fonts no)
	(model "antmicro_74lvch244abq_115.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
