(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "74VHC153FT_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "74VHC153FT_TSSOP"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "74VHC153FT_TSSOP"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/408/74VHC153FT_datasheet_en_20160818-1153686.pdf"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual Interface 4-channel multiplexer"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Toshiba"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "74VHC153FT"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, MUX, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "74VHC153FT_TSSOP_1_1"
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "~{1G}")
					(number "1")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "1C3")
					(number "3")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "1C2")
					(number "4")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "1C1")
					(number "5")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "1C0")
					(number "6")
				)
				(pin output line
					(at 21.59 -8.89 180)
					(length 2.54)
					(name "1Y")
					(number "7")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin output line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "2Y")
					(number "9")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "2C0")
					(number "10")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "2C1")
					(number "11")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "2C2")
					(number "12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "2C3")
					(number "13")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "A")
					(number "14")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "~{2G}")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
