(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "88E1116R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "88E1116R"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "88E1116R"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://octopart.com/datasheet/88e1116ra0-nnc1c000-marvell-7878457"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Phy 1-CH 10MBPS/100MBPS/1GBPS 1.8V/2.5V/3.3V 64-PIN QFN Ep"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "88E1116RA0-NNC1C000"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Marvell Semiconductor"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, PHY, ETHERNET, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "88E1116R_1_1"
				(pin input line
					(at 0 -81.28 0)
					(length 2.54)
					(name "CONFIG[1]")
					(number "1")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 2.54)
					(name "CONFIG[2]")
					(number "2")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 2.54)
					(name "CONFIG[3]")
					(number "3")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 2.54)
					(name "COMAn")
					(number "4")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "5")
				)
				(pin output line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "LED[0]")
					(number "6")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "VDDO")
					(number "7")
				)
				(pin output line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "LED[1]")
					(number "8")
				)
				(pin output line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "LED[2]")
					(number "9")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RESETn")
					(number "10")
				)
				(pin input line
					(at 25.4 -80.01 180)
					(length 2.54)
					(name "TRSTn")
					(number "11")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "DIS_REG12")
					(number "12")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DVDD")
					(number "13")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVDDR")
					(number "14")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "AVDDR")
					(number "15")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "AVDDX")
					(number "16")
				)
				(pin output line
					(at 0 -21.59 0)
					(length 2.54)
					(name "CTRL18")
					(number "17")
				)
				(pin no_connect line
					(at 22.86 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "18")
				)
				(pin bidirectional line
					(at 25.4 -21.59 180)
					(length 2.54)
					(name "MDIN[3]")
					(number "19")
				)
				(pin bidirectional line
					(at 25.4 -19.05 180)
					(length 2.54)
					(name "MDIP[3]")
					(number "20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "AVDD")
					(number "21")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "22")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "MDIN[2]")
					(number "23")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "MDIP[2]")
					(number "24")
				)
				(pin bidirectional line
					(at 25.4 -8.89 180)
					(length 2.54)
					(name "MDIN[1]")
					(number "25")
				)
				(pin bidirectional line
					(at 25.4 -6.35 180)
					(length 2.54)
					(name "MDIP[1]")
					(number "26")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "27")
				)
				(pin no_connect line
					(at 22.86 -24.13 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "29")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "MDIN[0]")
					(number "30")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "MDIP[0]")
					(number "31")
				)
				(pin output line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "TSTPT")
					(number "32")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "RSET")
					(number "33")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDDC")
					(number "34")
				)
				(pin output line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "HSDACN")
					(number "35")
				)
				(pin output line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "HSDACP")
					(number "36")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "AVDDC")
					(number "37")
				)
				(pin input line
					(at 0 -87.63 0)
					(length 2.54)
					(name "XTAL_IN")
					(number "38")
				)
				(pin output line
					(at 0 -90.17 0)
					(length 2.54)
					(name "XTAL_OUT")
					(number "39")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "40")
				)
				(pin input line
					(at 25.4 -82.55 180)
					(length 2.54)
					(name "TMS")
					(number "41")
				)
				(pin input line
					(at 25.4 -85.09 180)
					(length 2.54)
					(name "TCK")
					(number "42")
				)
				(pin input line
					(at 25.4 -87.63 180)
					(length 2.54)
					(name "TDI")
					(number "43")
				)
				(pin output line
					(at 25.4 -90.17 180)
					(length 2.54)
					(name "TDO")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "MDIO")
					(number "45")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDDO")
					(number "46")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "47")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "MDC")
					(number "48")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 2.54)
					(name "RX_CTRL")
					(number "49")
				)
				(pin output line
					(at 0 -72.39 0)
					(length 2.54)
					(name "RXD[0]")
					(number "50")
				)
				(pin output line
					(at 0 -69.85 0)
					(length 2.54)
					(name "RXD[1]")
					(number "51")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VDDOR")
					(number "52")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 2.54)
					(name "RX_CLK")
					(number "53")
				)
				(pin output line
					(at 0 -67.31 0)
					(length 2.54)
					(name "RXD[2]")
					(number "54")
				)
				(pin output line
					(at 0 -64.77 0)
					(length 2.54)
					(name "RXD[3]")
					(number "55")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VDDOR")
					(number "56")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "VREF")
					(number "57")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 2.54)
					(name "TXD[0]")
					(number "58")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 2.54)
					(name "TXD[1]")
					(number "59")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "TX_CLK")
					(number "60")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "TXD[2]")
					(number "61")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "TXD[3]")
					(number "62")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "TX_CTRL")
					(number "63")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 2.54)
					(name "CONFIG[0]")
					(number "64")
				)
				(pin passive line
					(at 25.4 -93.98 180)
					(length 2.54)
					(name "VSS")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
