(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "93AA66C_SOIC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "93AA66C_SOIC"
				(at 35.56 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "93AA66C_SOIC"
				(at 35.56 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/93AA66X-93LC66X-93C66X-4-Kbit-Microwire-Compatible-Serial-EEPROM-Data-Sheet.pdf"
				(at 35.56 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EEPROM 512x8 Or 256x16"
				(at 35.56 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "93AA66C-I/SN"
				(at 35.56 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, EEPROM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "93AA66C_SOIC_1_1"
				(pin input line
					(at 16.51 0 180)
					(length 2.54)
					(name "CS")
					(number "1")
				)
				(pin input line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "CLK")
					(number "2")
				)
				(pin input line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "DI")
					(number "3")
				)
				(pin tri_state line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "DO")
					(number "4")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "ORG")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
