(footprint "Spacer_Drill2.1mm_H3mm_9774030633R"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Spacer M=1.6 h=3mm fi=3.3mm")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Spacer_Drill2.1mm_H3mm_9774030633R"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -9.6 6.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.6 7.7 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -9.6 8.9 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.06 -1.08)
		(size 0.4 0.4)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.639127 -0.07) (xy 0.639552 -0.689893) (xy 0.3 -0.57) (xy 0.03 -0.42) (xy -0.225884 -0.205558)
					(xy -0.45 0.07) (xy -0.61 0.34) (xy -0.71 0.66) (xy -0.09 0.66) (xy 0 0.46) (xy 0.194348 0.215005)
					(xy 0.41 0.04)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_line
				(start -0.09 0.66)
				(end -0.709999 0.66)
				(width 0.2)
			)
			(gr_line
				(start 0.639127 -0.07)
				(end 0.639552 -0.689892)
				(width 0.2)
			)
			(gr_arc
				(start -0.71 0.66)
				(mid -0.225884 -0.205558)
				(end 0.639552 -0.689893)
				(width 0.2)
			)
			(gr_arc
				(start -0.09 0.66)
				(mid 0.194347 0.215005)
				(end 0.639127 -0.069678)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -1.06 1.08 90)
		(size 0.4 0.4)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.639127 -0.07) (xy 0.639552 -0.689893) (xy 0.3 -0.57) (xy 0.03 -0.42) (xy -0.225884 -0.205558)
					(xy -0.45 0.07) (xy -0.61 0.34) (xy -0.71 0.66) (xy -0.09 0.66) (xy 0 0.46) (xy 0.194348 0.215005)
					(xy 0.41 0.04)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_line
				(start -0.09 0.66)
				(end -0.709999 0.66)
				(width 0.2)
			)
			(gr_line
				(start 0.639127 -0.07)
				(end 0.639552 -0.689892)
				(width 0.2)
			)
			(gr_arc
				(start -0.71 0.66)
				(mid -0.225884 -0.205558)
				(end 0.639552 -0.689893)
				(width 0.2)
			)
			(gr_arc
				(start -0.09 0.66)
				(mid 0.194347 0.215005)
				(end 0.639127 -0.069678)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.06 -1.08 270)
		(size 0.4 0.4)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.639127 -0.07) (xy 0.639552 -0.689893) (xy 0.3 -0.57) (xy 0.03 -0.42) (xy -0.225884 -0.205558)
					(xy -0.45 0.07) (xy -0.61 0.34) (xy -0.71 0.66) (xy -0.09 0.66) (xy 0 0.46) (xy 0.194348 0.215005)
					(xy 0.41 0.04)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_line
				(start -0.09 0.66)
				(end -0.709999 0.66)
				(width 0.2)
			)
			(gr_line
				(start 0.639127 -0.07)
				(end 0.639552 -0.689892)
				(width 0.2)
			)
			(gr_arc
				(start -0.71 0.66)
				(mid -0.225884 -0.205558)
				(end 0.639552 -0.689893)
				(width 0.2)
			)
			(gr_arc
				(start -0.09 0.66)
				(mid 0.194347 0.215005)
				(end 0.639127 -0.069678)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.06 1.08 180)
		(size 0.4 0.4)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.639127 -0.07) (xy 0.639552 -0.689893) (xy 0.3 -0.57) (xy 0.03 -0.42) (xy -0.225884 -0.205558)
					(xy -0.45 0.07) (xy -0.61 0.34) (xy -0.71 0.66) (xy -0.09 0.66) (xy 0 0.46) (xy 0.194348 0.215005)
					(xy 0.41 0.04)
				)
				(width 0.2)
				(fill yes)
			)
			(gr_line
				(start -0.09 0.66)
				(end -0.709999 0.66)
				(width 0.2)
			)
			(gr_line
				(start 0.639127 -0.07)
				(end 0.639552 -0.689892)
				(width 0.2)
			)
			(gr_arc
				(start -0.71 0.66)
				(mid -0.225884 -0.205558)
				(end 0.639552 -0.689893)
				(width 0.2)
			)
			(gr_arc
				(start -0.09 0.66)
				(mid 0.194347 0.215005)
				(end 0.639127 -0.069678)
				(width 0.2)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 4 4)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_9774030633r.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
