(footprint "Spacer_Drill5.4mm_H5mm_9774050482R"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Mounting Hardware, Inside through hole M4, Drill 5.4mm, Height 5mm")
	(property "Reference" "REF**"
		(at 0 -5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Spacer_Drill5.4mm_H5mm_9774050482R"
		(at -4.8 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.95 7.2 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.95 8.4 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.95 9.6 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.55 2.36 180)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -2.031548 -1.093964)
				(mid -0.016573 -0.061893)
				(end 0.94 1.99)
				(width 0.2)
			)
			(gr_arc
				(start -2.047793 -1.257755)
				(mid 0.042712 -0.22974)
				(end 1.084509 1.853931)
				(width 0.2)
			)
			(gr_arc
				(start -2.048223 -1.392653)
				(mid 0.135758 -0.325784)
				(end 1.218959 1.850144)
				(width 0.2)
			)
			(gr_arc
				(start -2.1 -1.549999)
				(mid 0.24845 -0.425477)
				(end 1.378904 1.920123)
				(width 0.2)
			)
			(gr_arc
				(start -2.11 -1.689999)
				(mid 0.384912 -0.549345)
				(end 1.539278 1.939252)
				(width 0.2)
			)
			(gr_arc
				(start -2.16 -1.829999)
				(mid 0.521279 -0.680661)
				(end 1.670957 2.000471)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -1.999999)
				(mid 0.615796 -0.780769)
				(end 1.850984 2.005688)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.682237)
				(mid -0.368932 0.188947)
				(end 0.51059 1.993657)
				(width 0.2)
			)
			(gr_arc
				(start -2.129829 -0.524993)
				(mid -0.47151 0.298492)
				(end 0.354406 1.955602)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.480822)
				(mid -0.509621 0.331098)
				(end 0.309322 1.995722)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.581554)
				(mid -0.438641 0.260655)
				(end 0.410198 1.996469)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.782877)
				(mid -0.30068 0.115791)
				(end 0.610475 1.986763)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.98404)
				(mid -0.154743 -0.021134)
				(end 0.813162 1.999417)
				(width 0.2)
			)
			(gr_line
				(start 0.33 2.007681)
				(end 1.83 2.007681)
				(width 0.2)
			)
			(gr_line
				(start -2.177681 -0.5)
				(end -2.177681 -2)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.883476)
				(mid -0.226005 0.049026)
				(end 0.712402 1.99787)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.4 -2.57 90)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -2.031548 -1.093964)
				(mid -0.016573 -0.061893)
				(end 0.94 1.99)
				(width 0.2)
			)
			(gr_arc
				(start -2.047793 -1.257755)
				(mid 0.042712 -0.22974)
				(end 1.084509 1.853931)
				(width 0.2)
			)
			(gr_arc
				(start -2.048223 -1.392653)
				(mid 0.135758 -0.325784)
				(end 1.218959 1.850144)
				(width 0.2)
			)
			(gr_arc
				(start -2.1 -1.549999)
				(mid 0.24845 -0.425477)
				(end 1.378904 1.920123)
				(width 0.2)
			)
			(gr_arc
				(start -2.11 -1.689999)
				(mid 0.384912 -0.549345)
				(end 1.539278 1.939252)
				(width 0.2)
			)
			(gr_arc
				(start -2.16 -1.829999)
				(mid 0.521279 -0.680661)
				(end 1.670957 2.000471)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -1.999999)
				(mid 0.615796 -0.780769)
				(end 1.850984 2.005688)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.682237)
				(mid -0.368932 0.188947)
				(end 0.51059 1.993657)
				(width 0.2)
			)
			(gr_arc
				(start -2.129829 -0.524993)
				(mid -0.47151 0.298492)
				(end 0.354406 1.955602)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.480822)
				(mid -0.509621 0.331098)
				(end 0.309322 1.995722)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.581554)
				(mid -0.438641 0.260655)
				(end 0.410198 1.996469)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.782877)
				(mid -0.30068 0.115791)
				(end 0.610475 1.986763)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.98404)
				(mid -0.154743 -0.021134)
				(end 0.813162 1.999417)
				(width 0.2)
			)
			(gr_line
				(start 0.33 2.007681)
				(end 1.83 2.007681)
				(width 0.2)
			)
			(gr_line
				(start -2.177681 -0.5)
				(end -2.177681 -2)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.883476)
				(mid -0.226005 0.049026)
				(end 0.712402 1.99787)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.39 2.53 270)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -2.031548 -1.093964)
				(mid -0.016573 -0.061893)
				(end 0.94 1.99)
				(width 0.2)
			)
			(gr_arc
				(start -2.047793 -1.257755)
				(mid 0.042712 -0.22974)
				(end 1.084509 1.853931)
				(width 0.2)
			)
			(gr_arc
				(start -2.048223 -1.392653)
				(mid 0.135758 -0.325784)
				(end 1.218959 1.850144)
				(width 0.2)
			)
			(gr_arc
				(start -2.1 -1.549999)
				(mid 0.24845 -0.425477)
				(end 1.378904 1.920123)
				(width 0.2)
			)
			(gr_arc
				(start -2.11 -1.689999)
				(mid 0.384912 -0.549345)
				(end 1.539278 1.939252)
				(width 0.2)
			)
			(gr_arc
				(start -2.16 -1.829999)
				(mid 0.521279 -0.680661)
				(end 1.670957 2.000471)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -1.999999)
				(mid 0.615796 -0.780769)
				(end 1.850984 2.005688)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.682237)
				(mid -0.368932 0.188947)
				(end 0.51059 1.993657)
				(width 0.2)
			)
			(gr_arc
				(start -2.129829 -0.524993)
				(mid -0.47151 0.298492)
				(end 0.354406 1.955602)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.480822)
				(mid -0.509621 0.331098)
				(end 0.309322 1.995722)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.581554)
				(mid -0.438641 0.260655)
				(end 0.410198 1.996469)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.782877)
				(mid -0.30068 0.115791)
				(end 0.610475 1.986763)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.98404)
				(mid -0.154743 -0.021134)
				(end 0.813162 1.999417)
				(width 0.2)
			)
			(gr_line
				(start 0.33 2.007681)
				(end 1.83 2.007681)
				(width 0.2)
			)
			(gr_line
				(start -2.177681 -0.5)
				(end -2.177681 -2)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.883476)
				(mid -0.226005 0.049026)
				(end 0.712402 1.99787)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.57 -2.4)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -2.031548 -1.093964)
				(mid -0.016573 -0.061893)
				(end 0.94 1.99)
				(width 0.2)
			)
			(gr_arc
				(start -2.047793 -1.257755)
				(mid 0.042712 -0.22974)
				(end 1.084509 1.853931)
				(width 0.2)
			)
			(gr_arc
				(start -2.048223 -1.392653)
				(mid 0.135758 -0.325784)
				(end 1.218959 1.850144)
				(width 0.2)
			)
			(gr_arc
				(start -2.1 -1.549999)
				(mid 0.24845 -0.425477)
				(end 1.378904 1.920123)
				(width 0.2)
			)
			(gr_arc
				(start -2.11 -1.689999)
				(mid 0.384912 -0.549345)
				(end 1.539278 1.939252)
				(width 0.2)
			)
			(gr_arc
				(start -2.16 -1.829999)
				(mid 0.521279 -0.680661)
				(end 1.670957 2.000471)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -1.999999)
				(mid 0.615796 -0.780769)
				(end 1.850984 2.005688)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.682237)
				(mid -0.368932 0.188947)
				(end 0.51059 1.993657)
				(width 0.2)
			)
			(gr_arc
				(start -2.129829 -0.524993)
				(mid -0.47151 0.298492)
				(end 0.354406 1.955602)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.480822)
				(mid -0.509621 0.331098)
				(end 0.309322 1.995722)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.581554)
				(mid -0.438641 0.260655)
				(end 0.410198 1.996469)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.782877)
				(mid -0.30068 0.115791)
				(end 0.610475 1.986763)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.98404)
				(mid -0.154743 -0.021134)
				(end 0.813162 1.999417)
				(width 0.2)
			)
			(gr_line
				(start 0.33 2.007681)
				(end 1.83 2.007681)
				(width 0.2)
			)
			(gr_line
				(start -2.177681 -0.5)
				(end -2.177681 -2)
				(width 0.2)
			)
			(gr_arc
				(start -2.177681 -0.883476)
				(mid -0.226005 0.049026)
				(end 0.712402 1.99787)
				(width 0.2)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 9.4 9.4)
		(drill 5.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_9774050482r.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
