(footprint "Spacer_Drill4.4mm_H9mm_9774090360R"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Mounting Hardware, Inside through hole M3, Drill 4.4mm, Height 9mm")
	(property "Reference" "REF**"
		(at 0 -3.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "Spacer_Drill4.4mm_H9mm_9774090360R"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.95 6.65 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.95 7.85 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.95 9.05 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.1 -2.1)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.377294 1.707681)
				(mid 0.317578 0.318818)
				(end 1.705945 -0.377044)
				(width 0.2)
			)
			(gr_arc
				(start -0.478281 1.707681)
				(mid 0.244583 0.250396)
				(end 1.699539 -0.477144)
				(width 0.2)
			)
			(gr_arc
				(start -0.579192 1.707681)
				(mid 0.173852 0.179706)
				(end 1.699475 -0.57809)
				(width 0.2)
			)
			(gr_arc
				(start -0.680037 1.707681)
				(mid 0.102165 0.109975)
				(end 1.696729 -0.678615)
				(width 0.2)
			)
			(gr_arc
				(start -0.780822 1.707681)
				(mid 0.031098 0.039621)
				(end 1.695722 -0.779322)
				(width 0.2)
			)
			(gr_arc
				(start -0.881554 1.707681)
				(mid -0.041167 -0.029528)
				(end 1.691343 -0.879562)
				(width 0.2)
			)
			(gr_arc
				(start -0.982237 1.707681)
				(mid -0.109168 -0.10296)
				(end 1.69896 -0.98122)
				(width 0.2)
			)
			(gr_arc
				(start -1.082877 1.707681)
				(mid -0.184209 -0.16932)
				(end 1.686763 -1.080475)
				(width 0.2)
			)
			(gr_arc
				(start -1.183476 1.707681)
				(mid -0.252982 -0.241979)
				(end 1.692214 -1.181768)
				(width 0.2)
			)
			(gr_arc
				(start -1.28404 1.707681)
				(mid -0.319065 -0.317332)
				(end 1.705244 -1.283783)
				(width 0.2)
			)
			(gr_line
				(start 1.707681 -0.377294)
				(end 1.707681 -1.28404)
				(width 0.2)
			)
			(gr_line
				(start -0.377294 1.707681)
				(end -1.28404 1.707681)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.1 2.1)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 1.707681 0.377294)
				(mid 0.318818 -0.317578)
				(end -0.377044 -1.705945)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.478281)
				(mid 0.250396 -0.244583)
				(end -0.477144 -1.699539)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.579192)
				(mid 0.179706 -0.173852)
				(end -0.57809 -1.699475)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.680037)
				(mid 0.109975 -0.102165)
				(end -0.678615 -1.696729)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.780822)
				(mid 0.039621 -0.031098)
				(end -0.779322 -1.695722)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.881554)
				(mid -0.029528 0.041167)
				(end -0.879562 -1.691343)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 0.982237)
				(mid -0.10485 0.107282)
				(end -0.981842 -1.704264)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 1.082877)
				(mid -0.169319 0.18421)
				(end -1.080475 -1.686759)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 1.183476)
				(mid -0.241979 0.252982)
				(end -1.181768 -1.692214)
				(width 0.2)
			)
			(gr_arc
				(start 1.707681 1.28404)
				(mid -0.315258 0.321134)
				(end -1.283164 -1.699417)
				(width 0.2)
			)
			(gr_line
				(start -0.377294 -1.707681)
				(end -1.28404 -1.707681)
				(width 0.2)
			)
			(gr_line
				(start 1.707681 0.377294)
				(end 1.707681 1.28404)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.1 -2.1)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -1.707681 -0.377294)
				(mid -0.318817 0.317579)
				(end 0.377044 1.705947)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.478281)
				(mid -0.248815 0.24616)
				(end 0.477764 1.703961)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.579192)
				(mid -0.182997 0.170578)
				(end 0.576824 1.690278)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.680037)
				(mid -0.113388 0.098771)
				(end 0.67734 1.687185)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.780822)
				(mid -0.039621 0.031098)
				(end 0.779322 1.695722)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.881554)
				(mid 0.031359 -0.039345)
				(end 0.880198 1.696469)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -0.982237)
				(mid 0.101068 -0.111053)
				(end 0.98059 1.693657)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -1.082877)
				(mid 0.16932 -0.184209)
				(end 1.080475 1.686763)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -1.183476)
				(mid 0.243995 -0.250974)
				(end 1.182402 1.69787)
				(width 0.2)
			)
			(gr_arc
				(start -1.707681 -1.28404)
				(mid 0.315257 -0.321134)
				(end 1.283162 1.699417)
				(width 0.2)
			)
			(gr_line
				(start 0.377294 1.707681)
				(end 1.28404 1.707681)
				(width 0.2)
			)
			(gr_line
				(start -1.707681 -0.377294)
				(end -1.707681 -1.28404)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.1 2.1)
		(size 0.7 0.7)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.377294 -1.707681)
				(mid -0.317579 -0.318817)
				(end -1.705947 0.377044)
				(width 0.2)
			)
			(gr_arc
				(start 0.478281 -1.707681)
				(mid -0.24616 -0.248815)
				(end -1.703961 0.477764)
				(width 0.2)
			)
			(gr_arc
				(start 0.579192 -1.707681)
				(mid -0.170578 -0.182997)
				(end -1.690278 0.576824)
				(width 0.2)
			)
			(gr_arc
				(start 0.680037 -1.707681)
				(mid -0.098771 -0.113388)
				(end -1.687185 0.67734)
				(width 0.2)
			)
			(gr_arc
				(start 0.780822 -1.707681)
				(mid -0.031098 -0.039621)
				(end -1.695722 0.779322)
				(width 0.2)
			)
			(gr_arc
				(start 0.881554 -1.707681)
				(mid 0.039345 0.031359)
				(end -1.696469 0.880198)
				(width 0.2)
			)
			(gr_arc
				(start 0.982237 -1.707681)
				(mid 0.111053 0.101068)
				(end -1.693657 0.98059)
				(width 0.2)
			)
			(gr_arc
				(start 1.082877 -1.707681)
				(mid 0.184209 0.16932)
				(end -1.686763 1.080475)
				(width 0.2)
			)
			(gr_arc
				(start 1.183476 -1.707681)
				(mid 0.250974 0.243995)
				(end -1.69787 1.182402)
				(width 0.2)
			)
			(gr_arc
				(start 1.28404 -1.707681)
				(mid 0.321134 0.315257)
				(end -1.699417 1.283162)
				(width 0.2)
			)
			(gr_line
				(start -1.707681 0.377294)
				(end -1.707681 1.28404)
				(width 0.2)
			)
			(gr_line
				(start 0.377294 -1.707681)
				(end 1.28404 -1.707681)
				(width 0.2)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 7.4 7.4)
		(drill 4.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_9774090360r.glb"
		(offset
			(xyz 0 0 9)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
