(footprint "VFQFPN-40-1EP_5x5mm_P0.4mm_EP3.5x3.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "UQFN, 40 Pin")
	(tags "UQFN NoLead")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "VFQFPN-40-1EP_5x5mm_P0.4mm_EP3.5x3.5mm"
		(at 0 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.101 5.799 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.101 6.999 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.101 8.198 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.1 -1.1)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at -1.1 0)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at -1.1 1.1)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at 0 -1.1)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at 0 1.1)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at 1.1 -1.1)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at 1.1 0)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "" smd roundrect
		(at 1.1 1.1)
		(size 0.8 0.8)
		(layers "F.Paste")
		(roundrect_rratio 0.245098)
	)
	(pad "1" smd roundrect
		(at -2.476 -1.801)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.476 -1.401)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.476 -1)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.476 -0.6)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.476 -0.202)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.476 0.2)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.476 0.598)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.476 0.998)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.476 1.398)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -2.476 1.8)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -1.801 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -1.401 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -1 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -0.6 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -0.202 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 0.2 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 0.598 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0.998 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.398 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 1.8 2.475)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.475 1.8)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.475 1.398)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.475 0.998)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.475 0.598)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.475 0.2)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.475 -0.202)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 2.475 -0.6)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 2.475 -1)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 2.475 -1.401)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 2.475 -1.801)
		(size 0.75 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 1.8 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 1.398 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 0.998 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 0.598 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 0.2 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -0.202 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -0.6 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -1 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -1.401 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -1.801 -2.476)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd rect
		(at 0 0)
		(size 3.5 3.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_9dbl0651ckilf.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
