(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "9DBL0651CKILF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "9DBL0651CKILF"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "9DBL0651CKILF"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/698/REN_9DBL02x2_9DBL04x2_9DBL06x1_9DBL08x1C_DST_20221-3075841.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Clock Buffer 9DBL0651C 6 O/P 3.3V PCIE ZDB, ZO=85"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "9DBL0651CKILF"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Renesas"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PLL, IC, CLOCK, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "9DBL0651CKILF_1_1"
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "SADR_{TRI}")
					(number "1")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "~{HIBW_BYPM_LOBW}")
					(number "2")
				)
				(pin no_connect line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "FB_DNC+")
					(number "3")
				)
				(pin no_connect line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "FB_DNC-")
					(number "4")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDDR")
					(number "5")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CLK_IN+")
					(number "6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CLK_IN-")
					(number "7")
				)
				(pin power_in line
					(at 30.48 -55.88 180)
					(length 2.54)
					(name "GNDDIG")
					(number "8")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "SCLK")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "SDAT")
					(number "10")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDDIG3V3")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "12")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{OE0}")
					(number "13")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "DIF0+")
					(number "14")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "DIF0-")
					(number "15")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD3V3")
					(number "16")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "17")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "DIF1+")
					(number "18")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "DIF1-")
					(number "19")
				)
				(pin no_connect line
					(at 2.54 -54.61 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "~{OE1}")
					(number "21")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "DIF2+")
					(number "22")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "DIF2-")
					(number "23")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "~{OE2}")
					(number "24")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA3V3")
					(number "25")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "26")
				)
				(pin output line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "DIF3+")
					(number "27")
				)
				(pin output line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "DIF3-")
					(number "28")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "~{OE3}")
					(number "29")
				)
				(pin no_connect line
					(at 2.54 -55.88 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD3V3")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "32")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "DIF4+")
					(number "33")
				)
				(pin output line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "DIF4-")
					(number "34")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{OE4}")
					(number "35")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "DIF5+")
					(number "36")
				)
				(pin output line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "DIF5-")
					(number "37")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "~{OE5}")
					(number "38")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "39")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "~{CKPWRGD_PD}")
					(number "40")
				)
				(pin passive line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "EPAD")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
