(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AD5290"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AD5290"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AD5290"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/AD5290-3118426.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Digital Potentiometer IC +/-15V 8-Bit"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AD5290YRMZ100-R7"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIGITAL, POTENTIOMETER, IC, SPI, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AD5290_1_1"
				(pin input line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin input line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "V_{SS}")
					(number "3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{CS}")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLK")
					(number "6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDI")
					(number "7")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDO")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "9")
				)
				(pin output line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "W")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
