(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AD74412RBCPZ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 72.39 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AD74412RBCPZ"
				(at 72.39 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AD74412RBCPZ"
				(at 72.39 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD74412R.pdf"
				(at 72.39 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Quad-channel software configurable input/output circuit"
				(at 72.39 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 72.39 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AD74412RBCPZ"
				(at 72.39 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 72.39 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 72.39 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "ADC, SPI, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "CP-64-15_ADI CP-64-15_ADI-M CP-64-15_ADI-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AD74412RBCPZ_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SENSEH_A")
					(number "1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SENSEHF_A")
					(number "2")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SENSEL_A")
					(number "3")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "SENSELF_A")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VIOUTP_A")
					(number "5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VIOUTN_A")
					(number "6")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CCOMP_A")
					(number "63")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CASCODE_A")
					(number "64")
				)
			)
			(symbol "AD74412RBCPZ_2_1"
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VIOUTN_B")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VIOUTP_B")
					(number "12")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "SENSELF_B")
					(number "13")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SENSEL_B")
					(number "14")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SENSEHF_B")
					(number "15")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SENSEH_B")
					(number "16")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CASCODE_B")
					(number "17")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CCOMP_B")
					(number "18")
				)
			)
			(symbol "AD74412RBCPZ_3_1"
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CCOMP_C")
					(number "31")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CASCODE_C")
					(number "32")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SENSEH_C")
					(number "33")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SENSEHF_C")
					(number "34")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SENSEL_C")
					(number "35")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "SENSELF_C")
					(number "36")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VIOUTP_C")
					(number "37")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VIOUTN_C")
					(number "38")
				)
			)
			(symbol "AD74412RBCPZ_4_1"
				(pin output line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VIOUTN_D")
					(number "43")
				)
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "VIOUTP_D")
					(number "44")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "SENSELF_D")
					(number "45")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SENSEL_D")
					(number "46")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SENSEHF_D")
					(number "47")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SENSEH_D")
					(number "48")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CASCODE_D")
					(number "49")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CCOMP_D")
					(number "50")
				)
			)
			(symbol "AD74412RBCPZ_5_1"
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "8")
				)
				(pin power_out line
					(at 0 -12.7 0)
					(length 3.81)
					(name "ALDO5V")
					(number "9")
				)
				(pin power_out line
					(at 0 -16.51 0)
					(length 3.81)
					(name "ALDO1V8")
					(number "10")
				)
				(pin power_in line
					(at 31.75 0 180)
					(length 3.81)
					(name "CPUMP_P")
					(number "24")
				)
				(pin power_in line
					(at 31.75 -33.02 180)
					(length 3.81)
					(name "DGND")
					(number "25")
				)
				(pin power_in line
					(at 31.75 -5.08 180)
					(length 3.81)
					(name "CPUMP_N")
					(number "26")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 3.81)
					(name "AVSS")
					(number "27")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 3.81)
					(name "AGND")
					(number "28")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "REFIN")
					(number "29")
				)
				(pin output line
					(at 0 -24.13 0)
					(length 3.81)
					(name "REFOUT")
					(number "30")
				)
				(pin no_connect line
					(at 3.81 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "39")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "40")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "AGND_SENSE")
					(number "41")
				)
				(pin passive line
					(at 31.75 -33.02 180)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "54")
				)
				(pin power_in line
					(at 31.75 -13.97 180)
					(length 3.81)
					(name "IOVDD")
					(number "55")
				)
				(pin power_out line
					(at 31.75 -26.67 180)
					(length 3.81)
					(name "DLDO1V8")
					(number "57")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "AVSS")
					(number "65")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "AVDD")
					(number "[7,42]")
				)
				(pin power_in line
					(at 31.75 -11.43 180)
					(length 3.81)
					(name "DVCC")
					(number "[23,56]")
				)
			)
			(symbol "AD74412RBCPZ_6_1"
				(pin output line
					(at 24.13 0 180)
					(length 3.81)
					(name "GPO_A")
					(number "19")
				)
				(pin output line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "GPO_B")
					(number "20")
				)
				(pin output line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "GPO_C")
					(number "21")
				)
				(pin output line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "GPO_D")
					(number "22")
				)
				(pin output line
					(at 0 -11.43 0)
					(length 3.81)
					(name "SDO")
					(number "51")
				)
				(pin output line
					(at 24.13 -13.97 180)
					(length 3.81)
					(name "~{ADC_RDY}")
					(number "52")
				)
				(pin output line
					(at 24.13 -11.43 180)
					(length 3.81)
					(name "~{ALERT}")
					(number "53")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "~{LDAC}")
					(number "58")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 3.81)
					(name "SCLK")
					(number "59")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 3.81)
					(name "SDI")
					(number "60")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 3.81)
					(name "~{SYNC}")
					(number "61")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "~{RESET}")
					(number "62")
				)
			)
			(embedded_fonts no)
		)
)
