(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AD8604ARUZ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AD8604ARUZ"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AD8604ARUZ"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD8601_8602_8604.pdf"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CMOS Amplifier 4 Circuit Rail-to-Rail 14-TSSOP"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AD8604ARUZ"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "AMP, CMOS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AD8604ARUZ_1_1"
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "-")
					(number "2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "+")
					(number "3")
				)
			)
			(symbol "AD8604ARUZ_2_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "+")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "-")
					(number "6")
				)
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "")
					(number "7")
				)
			)
			(symbol "AD8604ARUZ_3_1"
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "-")
					(number "9")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "+")
					(number "10")
				)
			)
			(symbol "AD8604ARUZ_4_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "+")
					(number "12")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "-")
					(number "13")
				)
				(pin output line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "")
					(number "14")
				)
			)
			(symbol "AD8604ARUZ_5_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V-")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
