(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADC12DJ3200"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADC12DJ3200"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADC12DJ3200"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/adc12dj3200"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "12-bit SAR ADC, dual 3.2-GSPS or single 6.4-GSPS, 1.1 V and 1.9 V supply, FCBGA 144 pin 10x10 mm"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADC12DJ3200AAV"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "BGA, IC, ADC, RF, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "AAV144_TEX"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADC12DJ3200_1_1"
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "A1")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "A2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "A3")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "A6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "A7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "A12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "B2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "B3")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "B4")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "B5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "B6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "B7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "B12")
				)
				(pin output line
					(at 34.29 -25.4 180)
					(length 3.81)
					(name "BG")
					(number "C3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "C4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VA11")
					(number "C5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "C6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "NCOA0")
					(number "C7")
				)
				(pin output line
					(at 34.29 -7.62 180)
					(length 3.81)
					(name "ORA0")
					(number "C8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "C9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VD11")
					(number "C10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "D1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "D2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "D3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "D4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "D5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "D6")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "NCOA1")
					(number "D7")
				)
				(pin output line
					(at 34.29 -10.16 180)
					(length 3.81)
					(name "ORA1")
					(number "D8")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "D9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "D10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "E1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "E2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "E3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "E4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "E5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "E6")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "CALTRIG")
					(number "E7")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 3.81)
					(name "~{SCS}")
					(number "E8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "E9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "E10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "F2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "F3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "F4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "F5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "F6")
				)
				(pin output line
					(at 34.29 -21.59 180)
					(length 3.81)
					(name "CALSTAT")
					(number "F7")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 3.81)
					(name "SCLK")
					(number "F8")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DGND")
					(number "F9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "F10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "G2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "G3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "G4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "G5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "G6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "G7")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 3.81)
					(name "SDI")
					(number "G8")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "G9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "G10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "H1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "H2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "H3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "H4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "H5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "H6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "H7")
				)
				(pin output line
					(at 0 -34.29 0)
					(length 3.81)
					(name "SDO")
					(number "H8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "H9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "H10")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 3.81)
					(name "AGND")
					(number "J1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "J2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "J3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VA19")
					(number "J4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "J5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "J6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "NCOB1")
					(number "J7")
				)
				(pin output line
					(at 34.29 -16.51 180)
					(length 3.81)
					(name "ORB1")
					(number "J8")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "J9")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "J10")
				)
				(pin input line
					(at 34.29 -31.75 180)
					(length 3.81)
					(name "TDIODE+")
					(number "K2")
				)
				(pin input line
					(at 34.29 -34.29 180)
					(length 3.81)
					(name "TDIODE-")
					(number "K3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VA19")
					(number "K4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VA11")
					(number "K5")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PD")
					(number "K6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "NCOB0")
					(number "K7")
				)
				(pin output line
					(at 34.29 -13.97 180)
					(length 3.81)
					(name "ORB0")
					(number "K8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "K9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VD11")
					(number "K10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "L2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "L3")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "L4")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "L5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "L6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "L7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "L12")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "M1")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "M2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "M3")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "M6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "M7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "M12")
				)
			)
			(symbol "ADC12DJ3200_2_1"
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "INA+")
					(number "A4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "INA-")
					(number "A5")
				)
				(pin output line
					(at 38.1 -19.05 180)
					(length 3.81)
					(name "DA3+")
					(number "A8")
				)
				(pin output line
					(at 38.1 -21.59 180)
					(length 3.81)
					(name "DA3-")
					(number "A9")
				)
				(pin output line
					(at 38.1 -12.7 180)
					(length 3.81)
					(name "DA2+")
					(number "A10")
				)
				(pin output line
					(at 38.1 -15.24 180)
					(length 3.81)
					(name "DA2-")
					(number "A11")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "TMSTP+")
					(number "B1")
				)
				(pin output line
					(at 38.1 -44.45 180)
					(length 3.81)
					(name "DA7+")
					(number "B8")
				)
				(pin output line
					(at 38.1 -46.99 180)
					(length 3.81)
					(name "DA7-")
					(number "B9")
				)
				(pin output line
					(at 38.1 -38.1 180)
					(length 3.81)
					(name "DA6+")
					(number "B10")
				)
				(pin output line
					(at 38.1 -40.64 180)
					(length 3.81)
					(name "DA6-")
					(number "B11")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TMSTP-")
					(number "C1")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "~{SYNCSE}")
					(number "C2")
				)
				(pin output line
					(at 38.1 -31.75 180)
					(length 3.81)
					(name "DA5+")
					(number "C11")
				)
				(pin output line
					(at 38.1 -6.35 180)
					(length 3.81)
					(name "DA1+")
					(number "C12")
				)
				(pin output line
					(at 38.1 -34.29 180)
					(length 3.81)
					(name "DA5-")
					(number "D11")
				)
				(pin output line
					(at 38.1 -8.89 180)
					(length 3.81)
					(name "DA1-")
					(number "D12")
				)
				(pin output line
					(at 38.1 -25.4 180)
					(length 3.81)
					(name "DA4+")
					(number "E11")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(name "DA0+")
					(number "E12")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "CLK+")
					(number "F1")
				)
				(pin output line
					(at 38.1 -27.94 180)
					(length 3.81)
					(name "DA4-")
					(number "F11")
				)
				(pin output line
					(at 38.1 -2.54 180)
					(length 3.81)
					(name "DA0-")
					(number "F12")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 3.81)
					(name "CLK-")
					(number "G1")
				)
				(pin output line
					(at 38.1 -81.28 180)
					(length 3.81)
					(name "DB4-")
					(number "G11")
				)
				(pin output line
					(at 38.1 -55.88 180)
					(length 3.81)
					(name "DB0-")
					(number "G12")
				)
				(pin output line
					(at 38.1 -78.74 180)
					(length 3.81)
					(name "DB4+")
					(number "H11")
				)
				(pin output line
					(at 38.1 -53.34 180)
					(length 3.81)
					(name "DB0+")
					(number "H12")
				)
				(pin output line
					(at 38.1 -87.63 180)
					(length 3.81)
					(name "DB5-")
					(number "J11")
				)
				(pin output line
					(at 38.1 -62.23 180)
					(length 3.81)
					(name "DB1-")
					(number "J12")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "SYSREF+")
					(number "K1")
				)
				(pin output line
					(at 38.1 -85.09 180)
					(length 3.81)
					(name "DB5+")
					(number "K11")
				)
				(pin output line
					(at 38.1 -59.69 180)
					(length 3.81)
					(name "DB1+")
					(number "K12")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 3.81)
					(name "SYSREF-")
					(number "L1")
				)
				(pin output line
					(at 38.1 -97.79 180)
					(length 3.81)
					(name "DB7+")
					(number "L8")
				)
				(pin output line
					(at 38.1 -100.33 180)
					(length 3.81)
					(name "DB7-")
					(number "L9")
				)
				(pin output line
					(at 38.1 -91.44 180)
					(length 3.81)
					(name "DB6+")
					(number "L10")
				)
				(pin output line
					(at 38.1 -93.98 180)
					(length 3.81)
					(name "DB6-")
					(number "L11")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 3.81)
					(name "INB+")
					(number "M4")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 3.81)
					(name "INB-")
					(number "M5")
				)
				(pin output line
					(at 38.1 -72.39 180)
					(length 3.81)
					(name "DB3+")
					(number "M8")
				)
				(pin output line
					(at 38.1 -74.93 180)
					(length 3.81)
					(name "DB3-")
					(number "M9")
				)
				(pin output line
					(at 38.1 -66.04 180)
					(length 3.81)
					(name "DB2+")
					(number "M10")
				)
				(pin output line
					(at 38.1 -68.58 180)
					(length 3.81)
					(name "DB2-")
					(number "M11")
				)
			)
			(embedded_fonts no)
		)
)
