(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADM3055E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADM3055E"
				(at 40.64 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADM3055E"
				(at 40.64 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adm3055e-adm3057e.pdf"
				(at 40.64 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CAN FD Transceiver, 5kV rms Signal and Power Isolated, 12Mbps, Vio: 1.7-5.5V, Vcm: +/-25V, Vf: +/-40V, T: -40 to +105°C"
				(at 40.64 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADM3055EBRIZ"
				(at 40.64 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 40.64 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -18.796 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CAN, TRANSCEIVER, IC, ISOLATOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADM3055E_1_1"
				(pin power_out line
					(at 0 -29.21 0)
					(length 2.54)
					(name "GND_{1}")
					(number "1")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 2.54)
					(hide yes)
					(name "GND_{1}")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{IO}")
					(number "4")
				)
				(pin output line
					(at 0 -6.35 0)
					(length 2.54)
					(name "RXD")
					(number "5")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SILENT")
					(number "6")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "TXD")
					(number "7")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "STBY")
					(number "8")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "AUX_{IN}")
					(number "9")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 2.54)
					(hide yes)
					(name "GND_{1}")
					(number "10")
				)
				(pin power_out line
					(at 27.94 -29.21 180)
					(length 2.54)
					(name "GND_{2}")
					(number "11")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 2.54)
					(name "RS")
					(number "12")
				)
				(pin bidirectional line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "CANL")
					(number "13")
				)
				(pin bidirectional line
					(at 27.94 0 180)
					(length 2.54)
					(name "CANH")
					(number "14")
				)
				(pin passive line
					(at 27.94 -29.21 180)
					(length 2.54)
					(hide yes)
					(name "GND_{2}")
					(number "15")
				)
				(pin power_in line
					(at 27.94 -16.51 180)
					(length 2.54)
					(name "V_{ISOIN}")
					(number "16")
				)
				(pin output line
					(at 27.94 -13.97 180)
					(length 2.54)
					(name "AUX_{OUT}")
					(number "17")
				)
				(pin passive line
					(at 27.94 -26.67 180)
					(length 2.54)
					(hide yes)
					(name "GND_{ISO}")
					(number "18")
				)
				(pin output line
					(at 27.94 -19.05 180)
					(length 2.54)
					(name "V_{ISOOUT}")
					(number "19")
				)
				(pin power_out line
					(at 27.94 -26.67 180)
					(length 2.54)
					(name "GND_{ISO}")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
