(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADM3485ARZ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADM3485ARZ"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADM3485ARZ"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM3483_3485_3488_3490_3491.pdf?ADICID=SYND_WW_P682800_PF-spglobal"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RS-485/RS-422 Transceivers, 10Mbit/s Differential, 3.3V, 8-Pin SOIC"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADM3485ARZ"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, DRIVER, TRANSCEIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADM3485ARZ_1_1"
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "RO")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RE}")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DE")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DI")
					(number "4")
				)
				(pin power_in line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "A")
					(number "6")
				)
				(pin input line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "B")
					(number "7")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
