(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADV7282-M"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADV7282-M"
				(at 71.12 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADV7282-M"
				(at 71.12 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/ADV7282-2955931.pdf"
				(at 71.12 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Video decoder"
				(at 71.12 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 71.12 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADV7282WBCPZ-M"
				(at 71.12 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 71.12 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, VIDEO, IC, DECODER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "CP_32_12_ADI CP_32_12_ADI-M CP_32_12_ADI-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADV7282-M_1_1"
				(pin power_in line
					(at 50.8 -50.8 180)
					(length 2.54)
					(name "DGND")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DVDDIO")
					(number "2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DVDD")
					(number "3")
				)
				(pin power_in line
					(at 50.8 -50.8 180)
					(length 2.54)
					(hide yes)
					(name "DGND")
					(number "4")
				)
				(pin output line
					(at 50.8 -43.18 180)
					(length 2.54)
					(name "~{INTRQ}")
					(number "5")
				)
				(pin output line
					(at 50.8 -5.08 180)
					(length 2.54)
					(name "GPO2")
					(number "6")
				)
				(pin output line
					(at 50.8 -2.54 180)
					(length 2.54)
					(name "GPO1")
					(number "7")
				)
				(pin output line
					(at 50.8 0 180)
					(length 2.54)
					(name "GPO0")
					(number "8")
				)
				(pin output line
					(at 50.8 -10.16 180)
					(length 2.54)
					(name "D0_P")
					(number "9")
				)
				(pin output line
					(at 50.8 -12.7 180)
					(length 2.54)
					(name "D0_N")
					(number "10")
				)
				(pin output line
					(at 50.8 -15.24 180)
					(length 2.54)
					(name "CLK_P")
					(number "11")
				)
				(pin output line
					(at 50.8 -17.78 180)
					(length 2.54)
					(name "CLK_N")
					(number "12")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "MVDD")
					(number "13")
				)
				(pin output line
					(at 50.8 -27.94 180)
					(length 2.54)
					(name "XTALP")
					(number "14")
				)
				(pin input line
					(at 50.8 -30.48 180)
					(length 2.54)
					(name "XTALN")
					(number "15")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PVDD")
					(number "16")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AIN1")
					(number "17")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "AIN2")
					(number "18")
				)
				(pin output line
					(at 50.8 -38.1 180)
					(length 2.54)
					(name "VREFP")
					(number "19")
				)
				(pin output line
					(at 50.8 -40.64 180)
					(length 2.54)
					(name "VREFN")
					(number "20")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "AVDD")
					(number "21")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DIAG1")
					(number "22")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "AIN3")
					(number "23")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "AIN4")
					(number "24")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DIAG2")
					(number "25")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "AIN5")
					(number "26")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "AIN6")
					(number "27")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "~{RESET}")
					(number "28")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "ALSB")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SDATA")
					(number "30")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SCLK")
					(number "31")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "~{PWRDWN}")
					(number "32")
				)
				(pin passive line
					(at 50.8 -48.26 180)
					(length 2.54)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
