(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADV7535"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADV7535"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADV7535"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADV7535.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MIPI/DSI Receiver with HDMI Transmitter"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADV7535BCBZ-RL7"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "T_operational" "[-10,85]"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, HDMI, MIPI, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADV7535_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "V3P3")
					(number "B1")
				)
				(pin power_in line
					(at 33.02 0 180)
					(length 3.81)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "GND")
					(number "B3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "AVDD")
					(number "B4")
				)
				(pin power_in line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "GND")
					(number "B5")
				)
				(pin power_in line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "GND")
					(number "B6")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PVDD")
					(number "C6")
				)
				(pin power_in line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "GND")
					(number "C7")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "V1P8")
					(number "D4")
				)
				(pin power_in line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "GND")
					(number "E1")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DVDD")
					(number "E2")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "V1P8")
					(number "E3")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DVDD")
					(number "E4")
				)
				(pin power_in line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "GND")
					(number "E7")
				)
				(pin power_in line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "GND")
					(number "F1")
				)
				(pin power_in line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "GND")
					(number "F7")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DVDD")
					(number "G1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "A2VDD")
					(number "G7")
				)
			)
			(symbol "ADV7535_2_1"
				(pin output line
					(at 33.02 0 180)
					(length 3.81)
					(name "TX2+")
					(number "A1")
				)
				(pin output line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "TX2-")
					(number "A2")
				)
				(pin output line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "TX1+")
					(number "A3")
				)
				(pin output line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "TX1-")
					(number "A4")
				)
				(pin output line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "TX0+")
					(number "A5")
				)
				(pin output line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "TX0-")
					(number "A6")
				)
				(pin output line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "TXC")
					(number "A7")
				)
				(pin output line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "TXC-")
					(number "B7")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "SPDIF")
					(number "C1")
					(alternate "I2S" passive line)
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "SCLK")
					(number "C2")
					(alternate "MCLK" passive line)
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PD")
					(number "C3")
				)
				(pin input line
					(at 33.02 -38.1 180)
					(length 3.81)
					(name "HPD")
					(number "C4")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "R_EXT")
					(number "C5")
				)
				(pin output line
					(at 33.02 -33.02 180)
					(length 3.81)
					(name "DDC_SCL")
					(number "D1")
				)
				(pin bidirectional line
					(at 33.02 -35.56 180)
					(length 3.81)
					(name "DDC_SDA")
					(number "D2")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "LRCLK")
					(number "D3")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 3.81)
					(name "INT")
					(number "D5")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "CEC")
					(number "D6")
				)
				(pin input line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "CEC_CLK")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "SDA")
					(number "E5")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "SCL")
					(number "E6")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DRXC-")
					(number "F2")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DRX0-")
					(number "F3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DRX1-")
					(number "F4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DRX2-")
					(number "F5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DRX3-")
					(number "F6")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DRXC+")
					(number "G2")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DRX0+")
					(number "G3")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DRX1+")
					(number "G4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DRX2+")
					(number "G5")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "DRX3+")
					(number "G6")
				)
			)
			(embedded_fonts no)
		)
)
