(footprint "BGA-156-146_5x5mm_Layout13x12_P0.35mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.925 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-156-146_5x5mm_Layout13x12_P0.35mm"
		(at 0 3.675 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.098 10 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.098 11.2 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.098 12.4 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2.1 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A2" smd circle
		(at -1.75 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A3" smd circle
		(at -1.4 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A4" smd circle
		(at -1.05 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A5" smd circle
		(at -0.7 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A6" smd circle
		(at -0.35 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A7" smd circle
		(at 0 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A8" smd circle
		(at 0.35 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A9" smd circle
		(at 0.7 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A10" smd circle
		(at 1.05 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A11" smd circle
		(at 1.4 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A12" smd circle
		(at 1.75 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "A13" smd circle
		(at 2.1 -1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B1" smd circle
		(at -2.1 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B2" smd circle
		(at -1.75 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B3" smd circle
		(at -1.4 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B4" smd circle
		(at -1.05 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B5" smd circle
		(at -0.7 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B6" smd circle
		(at -0.35 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B7" smd circle
		(at 0 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B8" smd circle
		(at 0.35 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B9" smd circle
		(at 0.7 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B10" smd circle
		(at 1.05 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B11" smd circle
		(at 1.4 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B12" smd circle
		(at 1.75 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "B13" smd circle
		(at 2.1 -1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C1" smd circle
		(at -2.1 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C2" smd circle
		(at -1.75 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C3" smd circle
		(at -1.4 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C4" smd circle
		(at -1.05 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C5" smd circle
		(at -0.7 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C6" smd circle
		(at -0.35 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C7" smd circle
		(at 0 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C8" smd circle
		(at 0.35 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C9" smd circle
		(at 0.7 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C10" smd circle
		(at 1.05 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C11" smd circle
		(at 1.4 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C12" smd circle
		(at 1.75 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "C13" smd circle
		(at 2.1 -1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D1" smd circle
		(at -2.1 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D2" smd circle
		(at -1.75 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D3" smd circle
		(at -1.4 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D4" smd circle
		(at -1.05 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D5" smd circle
		(at -0.7 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D6" smd circle
		(at -0.35 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D7" smd circle
		(at 0 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D8" smd circle
		(at 0.35 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D9" smd circle
		(at 0.7 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D10" smd circle
		(at 1.05 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D11" smd circle
		(at 1.4 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D12" smd circle
		(at 1.75 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "D13" smd circle
		(at 2.1 -0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E1" smd circle
		(at -2.1 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E2" smd circle
		(at -1.75 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E3" smd circle
		(at -1.4 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E4" smd circle
		(at -1.05 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E5" smd circle
		(at -0.7 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E6" smd circle
		(at -0.35 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E7" smd circle
		(at 0 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E8" smd circle
		(at 0.35 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E9" smd circle
		(at 0.7 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E10" smd circle
		(at 1.05 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E11" smd circle
		(at 1.4 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E12" smd circle
		(at 1.75 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "E13" smd circle
		(at 2.1 -0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F1" smd circle
		(at -2.1 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F2" smd circle
		(at -1.75 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F3" smd circle
		(at -1.4 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F4" smd circle
		(at -1.05 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F9" smd circle
		(at 0.7 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F10" smd circle
		(at 1.05 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F11" smd circle
		(at 1.4 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F12" smd circle
		(at 1.75 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "F13" smd circle
		(at 2.1 -0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G1" smd circle
		(at -2.1 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G2" smd circle
		(at -1.75 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G3" smd circle
		(at -1.4 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G4" smd circle
		(at -1.05 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G5" smd circle
		(at -0.7 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G9" smd circle
		(at 0.7 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G10" smd circle
		(at 1.05 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G11" smd circle
		(at 1.4 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G12" smd circle
		(at 1.75 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "G13" smd circle
		(at 2.1 0.175)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H1" smd circle
		(at -2.1 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H2" smd circle
		(at -1.75 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H3" smd circle
		(at -1.4 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H4" smd circle
		(at -1.05 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H5" smd circle
		(at -0.7 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H9" smd circle
		(at 0.7 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H10" smd circle
		(at 1.05 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H11" smd circle
		(at 1.4 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H12" smd circle
		(at 1.75 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "H13" smd circle
		(at 2.1 0.525)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J1" smd circle
		(at -2.1 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J2" smd circle
		(at -1.75 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J3" smd circle
		(at -1.4 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J4" smd circle
		(at -1.05 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J5" smd circle
		(at -0.7 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J6" smd circle
		(at -0.35 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J7" smd circle
		(at 0 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J8" smd circle
		(at 0.35 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J9" smd circle
		(at 0.7 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J10" smd circle
		(at 1.05 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J11" smd circle
		(at 1.4 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J12" smd circle
		(at 1.75 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "J13" smd circle
		(at 2.1 0.875)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K1" smd circle
		(at -2.1 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K2" smd circle
		(at -1.75 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K3" smd circle
		(at -1.4 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K4" smd circle
		(at -1.05 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K5" smd circle
		(at -0.7 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K6" smd circle
		(at -0.35 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K7" smd circle
		(at 0 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K8" smd circle
		(at 0.35 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K9" smd circle
		(at 0.7 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K10" smd circle
		(at 1.05 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K11" smd circle
		(at 1.4 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K12" smd circle
		(at 1.75 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "K13" smd circle
		(at 2.1 1.225)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L1" smd circle
		(at -2.1 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L2" smd circle
		(at -1.75 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L3" smd circle
		(at -1.4 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L4" smd circle
		(at -1.05 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L5" smd circle
		(at -0.7 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L6" smd circle
		(at -0.35 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L7" smd circle
		(at 0 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L8" smd circle
		(at 0.35 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L9" smd circle
		(at 0.7 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L10" smd circle
		(at 1.05 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L11" smd circle
		(at 1.4 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L12" smd circle
		(at 1.75 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "L13" smd circle
		(at 2.1 1.575)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M1" smd circle
		(at -2.1 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M2" smd circle
		(at -1.75 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M3" smd circle
		(at -1.4 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M4" smd circle
		(at -1.05 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M5" smd circle
		(at -0.7 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M6" smd circle
		(at -0.35 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M7" smd circle
		(at 0 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M8" smd circle
		(at 0.35 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M9" smd circle
		(at 0.7 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M10" smd circle
		(at 1.05 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M11" smd circle
		(at 1.4 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M12" smd circle
		(at 1.75 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(pad "M13" smd circle
		(at 2.1 1.925)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.03)
	)
	(embedded_fonts no)
	(model "antmicro_amap42kp_kbr.glb"
		(offset
			(xyz -2.5 -2.5 0.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
