(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AMAP42KP-KBR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 44.45 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AMAP42KP-KBR"
				(at 44.45 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AMAP42KP-KBR"
				(at 44.45 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ambiq.com/apollo4-plus/"
				(at 44.45 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Apollo4 192 MHz Cortex M4F, 141-pin BGA"
				(at 44.45 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AMAP42KP-KBR"
				(at 44.45 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Ambiq"
				(at 44.45 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 44.45 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 44.45 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "VSD class" "Ambiq Apollo 4 plus"
				(at 44.45 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, BGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AMAP42KP-KBR_1_1"
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "SIMOBUCK_SW")
					(number "A1")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "SIMOBUCK_SWSEL")
					(number "A2")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VDDC")
					(number "A3")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "XI")
					(number "A4")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "XO")
					(number "A5")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "RSTN")
					(number "A6")
				)
				(pin passive line
					(at 31.75 -5.08 180)
					(length 3.81)
					(name "LPADCD0NSE0")
					(number "A11")
				)
				(pin passive line
					(at 31.75 -2.54 180)
					(length 3.81)
					(name "LPADCD0PSE1")
					(number "A12")
				)
				(pin passive line
					(at 31.75 0 180)
					(length 3.81)
					(name "LPADC_VREF")
					(number "A13")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VDDP")
					(number "B1")
				)
				(pin passive line
					(at 31.75 -55.88 180)
					(length 3.81)
					(name "VSSP")
					(number "B2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "VDDC_LV")
					(number "B3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VDDA")
					(number "B4")
				)
				(pin passive line
					(at 31.75 -58.42 180)
					(length 3.81)
					(name "VSSA")
					(number "B5")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "LPMICBIAS")
					(number "B11")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDAUDA")
					(number "B12")
				)
				(pin passive line
					(at 31.75 -53.34 180)
					(length 3.81)
					(name "VSSAUDA")
					(number "B13")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDDS")
					(number "C1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VDDF")
					(number "C2")
				)
				(pin passive line
					(at 31.75 -10.16 180)
					(length 3.81)
					(name "LPADCD1NSE2")
					(number "C12")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "XI32M")
					(number "C13")
				)
				(pin passive line
					(at 31.75 -50.8 180)
					(length 3.81)
					(name "VSS")
					(number "D2")
				)
				(pin passive line
					(at 31.75 -7.62 180)
					(length 3.81)
					(name "LPADCD1PSE3")
					(number "D12")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "XO32M")
					(number "D13")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDAUDD")
					(number "E12")
				)
				(pin passive line
					(at 31.75 -48.26 180)
					(length 3.81)
					(name "VSSAUDD")
					(number "E13")
				)
				(pin no_connect line
					(at 27.94 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F5")
				)
				(pin no_connect line
					(at 27.94 -33.02 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F6")
				)
				(pin no_connect line
					(at 27.94 -34.29 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F7")
				)
				(pin no_connect line
					(at 27.94 -35.56 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F8")
				)
				(pin no_connect line
					(at 27.94 -36.83 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G6")
				)
				(pin no_connect line
					(at 27.94 -29.21 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G7")
				)
				(pin no_connect line
					(at 27.94 -31.75 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G8")
				)
				(pin passive line
					(at 31.75 -16.51 180)
					(length 3.81)
					(name "MIPI_CLKN")
					(number "G13")
				)
				(pin no_connect line
					(at 27.94 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H6")
				)
				(pin no_connect line
					(at 27.94 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H7")
				)
				(pin no_connect line
					(at 27.94 -39.37 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H8")
				)
				(pin passive line
					(at 31.75 -13.97 180)
					(length 3.81)
					(name "MIPI_CLKP")
					(number "H13")
				)
				(pin passive line
					(at 31.75 -45.72 180)
					(length 3.81)
					(name "VSS18")
					(number "J10")
				)
				(pin passive line
					(at 31.75 -21.59 180)
					(length 3.81)
					(name "MIPI_D1N")
					(number "J13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VDDUSB33")
					(number "K7")
				)
				(pin passive line
					(at 31.75 -19.05 180)
					(length 3.81)
					(name "MIPI_D1P")
					(number "K13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "VDDUSB0P9")
					(number "L7")
				)
				(pin passive line
					(at 31.75 -43.18 180)
					(length 3.81)
					(name "VSSAUSB")
					(number "L8")
				)
				(pin passive line
					(at 31.75 -26.67 180)
					(length 3.81)
					(name "MIPI_D0N")
					(number "L13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "USB0P_P")
					(number "M7")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "USB0P_N")
					(number "M8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDH2")
					(number "M9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDH")
					(number "M10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD18")
					(number "M12")
				)
				(pin passive line
					(at 31.75 -24.13 180)
					(length 3.81)
					(name "MIPI_D0P")
					(number "M13")
				)
			)
			(symbol "AMAP42KP-KBR_2_1"
				(pin passive line
					(at 24.13 -55.88 180)
					(length 3.81)
					(name "GPIO51")
					(number "A9")
				)
				(pin passive line
					(at 24.13 -53.34 180)
					(length 3.81)
					(name "GPIO50")
					(number "A10")
				)
				(pin passive line
					(at 24.13 -60.96 180)
					(length 3.81)
					(name "GPIO53")
					(number "B9")
				)
				(pin passive line
					(at 24.13 -58.42 180)
					(length 3.81)
					(name "GPIO52")
					(number "B10")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "GPIO19")
					(number "C3")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "GPIO12")
					(number "C4")
				)
				(pin passive line
					(at 24.13 -66.04 180)
					(length 3.81)
					(name "GPIO55")
					(number "C9")
				)
				(pin passive line
					(at 24.13 -63.5 180)
					(length 3.81)
					(name "GPIO54")
					(number "C10")
				)
				(pin passive line
					(at 24.13 -49.53 180)
					(length 3.81)
					(name "GPIO49")
					(number "D1")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "GPIO18")
					(number "D3")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "GPIO17")
					(number "D4")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "GPIO13")
					(number "D5")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "GPIO14")
					(number "D6")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "GPIO16")
					(number "D7")
				)
				(pin passive line
					(at 24.13 -71.12 180)
					(length 3.81)
					(name "GPIO57")
					(number "D9")
				)
				(pin passive line
					(at 24.13 -68.58 180)
					(length 3.81)
					(name "GPIO56")
					(number "D10")
				)
				(pin passive line
					(at 24.13 -39.37 180)
					(length 3.81)
					(name "GPIO45")
					(number "D11")
				)
				(pin passive line
					(at 24.13 -46.99 180)
					(length 3.81)
					(name "GPIO48")
					(number "E1")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "GPIO24")
					(number "E2")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "GPIO28")
					(number "E3")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "GPIO11")
					(number "E4")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "GPIO15")
					(number "E5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "GPIO10")
					(number "E6")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "GPIO09")
					(number "E7")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "GPIO08")
					(number "E8")
				)
				(pin passive line
					(at 24.13 -41.91 180)
					(length 3.81)
					(name "GPIO46")
					(number "E11")
				)
				(pin passive line
					(at 24.13 -44.45 180)
					(length 3.81)
					(name "GPIO47")
					(number "F1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "GPIO23")
					(number "F2")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GPIO22")
					(number "F3")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "GPIO29")
					(number "F4")
				)
				(pin passive line
					(at 24.13 -29.21 180)
					(length 3.81)
					(name "GPIO41")
					(number "F11")
				)
				(pin passive line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "GPIO38")
					(number "F12")
				)
				(pin passive line
					(at 24.13 -26.67 180)
					(length 3.81)
					(name "GPIO40")
					(number "F13")
				)
				(pin passive line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "GPIO36")
					(number "G1")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(name "GPIO30")
					(number "G4")
				)
				(pin passive line
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "GPIO39")
					(number "G11")
				)
				(pin passive line
					(at 24.13 -36.83 180)
					(length 3.81)
					(name "GPIO44")
					(number "G12")
				)
				(pin passive line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "GPIO35")
					(number "H1")
				)
				(pin passive line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "GPIO37")
					(number "H11")
				)
				(pin passive line
					(at 24.13 -31.75 180)
					(length 3.81)
					(name "GPIO42")
					(number "H12")
				)
				(pin passive line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "GPIO34")
					(number "J1")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "GPIO21")
					(number "J3")
				)
				(pin passive line
					(at 24.13 -73.66 180)
					(length 3.81)
					(name "GPIO58")
					(number "J7")
				)
				(pin passive line
					(at 24.13 -76.2 180)
					(length 3.81)
					(name "GPIO59")
					(number "J8")
				)
				(pin passive line
					(at 24.13 -34.29 180)
					(length 3.81)
					(name "GPIO43")
					(number "J11")
				)
				(pin passive line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "GPIO33")
					(number "K1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "GPIO00")
					(number "K2")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "GPIO20")
					(number "K3")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GPIO25")
					(number "K4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "GPIO05")
					(number "K6")
				)
				(pin passive line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "GPIO32")
					(number "L1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "GPIO01")
					(number "L2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "GPIO03")
					(number "L3")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "GPIO26")
					(number "L4")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "GPIO06")
					(number "L6")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "GPIO31")
					(number "M1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "GPIO02")
					(number "M2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "GPIO04")
					(number "M3")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "GPIO27")
					(number "M4")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "GPIO07")
					(number "M6")
				)
			)
			(symbol "AMAP42KP-KBR_3_1"
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "GPIO65")
					(number "A7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "GPIO66")
					(number "A8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "GPIO64")
					(number "B6")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "GPIO68")
					(number "B7")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "GPIO69")
					(number "B8")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "GPIO70")
					(number "C5")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "GPIO67")
					(number "C6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "GPIO71")
					(number "C7")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "GPIO72")
					(number "C8")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(name "GPIO90")
					(number "C11")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "GPIO73")
					(number "D8")
				)
				(pin passive line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "GPIO92")
					(number "E9")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "GPIO91")
					(number "E10")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "GPIO88")
					(number "F9")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "GPIO89")
					(number "F10")
				)
				(pin passive line
					(at 24.13 -31.75 180)
					(length 3.81)
					(name "GPIO102")
					(number "G2")
				)
				(pin passive line
					(at 24.13 -26.67 180)
					(length 3.81)
					(name "GPIO100")
					(number "G3")
				)
				(pin passive line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "GPIO97")
					(number "G5")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "GPIO87")
					(number "G9")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "GPIO86")
					(number "G10")
				)
				(pin passive line
					(at 24.13 -34.29 180)
					(length 3.81)
					(name "GPIO103")
					(number "H2")
				)
				(pin passive line
					(at 24.13 -29.21 180)
					(length 3.81)
					(name "GPIO101")
					(number "H3")
				)
				(pin passive line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "GPIO98")
					(number "H4")
				)
				(pin passive line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "GPIO96")
					(number "H5")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GPIO85")
					(number "H9")
				)
				(pin passive line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "GPIO93")
					(number "H10")
				)
				(pin passive line
					(at 24.13 -36.83 180)
					(length 3.81)
					(name "GPIO104")
					(number "J2")
				)
				(pin passive line
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "GPIO99")
					(number "J4")
				)
				(pin passive line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "GPIO95")
					(number "J5")
				)
				(pin passive line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "GPIO94")
					(number "J6")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "GPIO84")
					(number "J9")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "GPIO74")
					(number "J12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "GPIO61")
					(number "K5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "GPIO60")
					(number "K8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "GPIO83")
					(number "K9")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "GPIO80")
					(number "K10")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "GPIO77")
					(number "K11")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "GPIO75")
					(number "K12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "GPIO62")
					(number "L5")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GPIO82")
					(number "L9")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "GPIO81")
					(number "L10")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "GPIO78")
					(number "L11")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "GPIO76")
					(number "L12")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "GPIO63")
					(number "M5")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "GPIO79")
					(number "M11")
				)
			)
			(embedded_fonts no)
		)
)
