(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AS6C8008-55BIN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AS6C8008-55BIN"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AS6C8008-55BIN"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.alliancememory.com/wp-content/uploads/pdf/lp_sram/AllianceMemory_8M_LPSRAM_AS6C8008_v1.1_May%202021.pdf"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SRAM, Asynchronous SRAM, 8 Mbit, TFBGA, 48 Pins, 2.7 V"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AS6C8008-55BIN"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Alliance Memory"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, ASYNCHRONOUS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "TSOP?I*18.4x12mm*P0.5mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AS6C8008-55BIN_1_1"
				(pin no_connect line
					(at 6.35 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A1")
				)
				(pin input line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "OE#")
					(number "A2")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "A0")
					(number "A3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A1")
					(number "A4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A2")
					(number "A5")
				)
				(pin input line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "CE2")
					(number "A6")
				)
				(pin no_connect line
					(at 8.89 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B1")
				)
				(pin no_connect line
					(at 7.62 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A3")
					(number "B3")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A4")
					(number "B4")
				)
				(pin input line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "CE#")
					(number "B5")
				)
				(pin no_connect line
					(at 11.43 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B6")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "DQ0")
					(number "C1")
				)
				(pin no_connect line
					(at 10.16 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A5")
					(number "C3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A6")
					(number "C4")
				)
				(pin no_connect line
					(at 12.7 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C5")
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "DQ4")
					(number "C6")
				)
				(pin passive line
					(at 25.4 -45.72 180)
					(length 2.54)
					(name "VSS")
					(number "D1")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "DQ1")
					(number "D2")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "A17")
					(number "D3")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A7")
					(number "D4")
				)
				(pin bidirectional line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "DQ5")
					(number "D5")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "VCC")
					(number "D6")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "E1")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "DQ2")
					(number "E2")
				)
				(pin no_connect line
					(at 13.97 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "E3")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "A16")
					(number "E4")
				)
				(pin bidirectional line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "DQ6")
					(number "E5")
				)
				(pin passive line
					(at 25.4 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "DQ3")
					(number "F1")
				)
				(pin no_connect line
					(at 15.24 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "F2")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "A14")
					(number "F3")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "A15")
					(number "F4")
				)
				(pin no_connect line
					(at 16.51 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "F5")
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "DQ7")
					(number "F6")
				)
				(pin no_connect line
					(at 17.78 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "G1")
				)
				(pin no_connect line
					(at 19.05 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "G2")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "A12")
					(number "G3")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A13")
					(number "G4")
				)
				(pin input line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "WE#")
					(number "G5")
				)
				(pin no_connect line
					(at 20.32 -50.8 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "G6")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "A18")
					(number "H1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A8")
					(number "H2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A9")
					(number "H3")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A10")
					(number "H4")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A11")
					(number "H5")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "A19")
					(number "H6")
				)
			)
			(embedded_fonts no)
		)
)
