(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "AT24CS01_SOIC8"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "AT24CS01_SOIC8"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "AT24CS01_SOIC8"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MPD/ProductDocuments/DataSheets/20006330A.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EEPROM, 1 Kbit, 128 x 8bit, Serial I2C (2-Wire), 1 MHz, SOIC-8"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "AT24CS01-SSHM-B"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "AT24CS01_SOIC8_1_1"
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "A0")
					(number "1")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin power_in line
					(at 15.24 -11.43 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "WP")
					(number "7")
				)
				(pin power_in line
					(at 15.24 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
