(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ATA6571RT_SOIC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ATA6571RT_SOIC"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ATA6571RT_SOIC"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/AERO/ProductDocuments/DataSheets/Radiation_Tolerant_CAN_FD_Transceiver_Data_Sheet_DS50003902.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation Tolerant CAN FD Transceiver, 5 Mbps, Vcc: 5V, Vio: 3.3V, -55/+125°C, SOIC-14"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ATA6571D3XRT-HP"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CAN, IC, SMT, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ATA6571RT_SOIC_1_1"
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXD")
					(number "1")
				)
				(pin power_in line
					(at 17.78 -20.32 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RXD")
					(number "4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{IO}")
					(number "5")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EN")
					(number "6")
				)
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "INH")
					(number "7")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "~{ERR}")
					(number "8")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "WAKE")
					(number "9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VS")
					(number "10")
				)
				(pin no_connect line
					(at 15.24 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "11")
				)
				(pin bidirectional line
					(at 17.78 -17.78 180)
					(length 2.54)
					(name "CAN_L")
					(number "12")
				)
				(pin bidirectional line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "CAN_H")
					(number "13")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{STDBY}")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
