(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ATSAMD21G18A-MU"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ATSAMD21G18A-MU"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ATSAMD21G18A-MU"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/268/SAM_D21_DA1_Family_Data_Sheet_DS40001882H-3081333.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "32bit Microcontroller, 48MHz, 256 kB Flash, ARM Cortex-M0+"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ATSAMD21G18A-MU"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ATSAMD21G18A-MU_1_1"
				(pin bidirectional line
					(at 33.02 0 180)
					(length 2.54)
					(name "PA00")
					(number "1")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "PA01")
					(number "2")
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "PA02")
					(number "3")
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 2.54)
					(name "PA03")
					(number "4")
				)
				(pin power_in line
					(at 0 -71.12 0)
					(length 2.54)
					(name "GNDANA")
					(number "5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDANA")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PB08")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PB09")
					(number "8")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 2.54)
					(name "PA04")
					(number "9")
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "PA05")
					(number "10")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "PA06")
					(number "11")
				)
				(pin bidirectional line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "PA07")
					(number "12")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 2.54)
					(name "PA08")
					(number "13")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "PA09")
					(number "14")
				)
				(pin bidirectional line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "PA10")
					(number "15")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "PA11")
					(number "16")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDIO")
					(number "17")
				)
				(pin power_in line
					(at 0 -73.66 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PB10")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PB11")
					(number "20")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "PA12")
					(number "21")
				)
				(pin bidirectional line
					(at 33.02 -33.02 180)
					(length 2.54)
					(name "PA13")
					(number "22")
				)
				(pin bidirectional line
					(at 33.02 -35.56 180)
					(length 2.54)
					(name "PA14")
					(number "23")
				)
				(pin bidirectional line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "PA15")
					(number "24")
				)
				(pin bidirectional line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "PA16")
					(number "25")
				)
				(pin bidirectional line
					(at 33.02 -43.18 180)
					(length 2.54)
					(name "PA17")
					(number "26")
				)
				(pin bidirectional line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "PA18")
					(number "27")
				)
				(pin bidirectional line
					(at 33.02 -48.26 180)
					(length 2.54)
					(name "PA19")
					(number "28")
				)
				(pin bidirectional line
					(at 33.02 -50.8 180)
					(length 2.54)
					(name "PA20")
					(number "29")
				)
				(pin bidirectional line
					(at 33.02 -53.34 180)
					(length 2.54)
					(name "PA21")
					(number "30")
				)
				(pin bidirectional line
					(at 33.02 -55.88 180)
					(length 2.54)
					(name "PA22")
					(number "31")
				)
				(pin bidirectional line
					(at 33.02 -58.42 180)
					(length 2.54)
					(name "PA23")
					(number "32")
				)
				(pin bidirectional line
					(at 33.02 -60.96 180)
					(length 2.54)
					(name "PA24")
					(number "33")
				)
				(pin bidirectional line
					(at 33.02 -63.5 180)
					(length 2.54)
					(name "PA25")
					(number "34")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "35")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PB22")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PB23")
					(number "38")
				)
				(pin bidirectional line
					(at 33.02 -66.04 180)
					(length 2.54)
					(name "PA27")
					(number "39")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "~{RESET}")
					(number "40")
				)
				(pin bidirectional line
					(at 33.02 -68.58 180)
					(length 2.54)
					(name "PA28")
					(number "41")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "42")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDCORE")
					(number "43")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDIN")
					(number "44")
				)
				(pin bidirectional line
					(at 33.02 -71.12 180)
					(length 2.54)
					(name "PA30")
					(number "45")
				)
				(pin bidirectional line
					(at 33.02 -73.66 180)
					(length 2.54)
					(name "PA31")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PB02")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PB03")
					(number "48")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
