(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ATSAMD21J17D-AFT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ATSAMD21J17D-AFT"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ATSAMD21J17D-AFT"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-D21-DA1-Family-Data-Sheet-DS40001882H.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, SAM32 Family SAM D2X Series Microcontrollers, ARM Cortex-M0+, 32 bit, 48 MHz, 128 KB"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ATSAMD21J17D-AFT"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ATSAMD21J17D-AFT_1_1"
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GNDANA")
					(number "7")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDANA")
					(number "8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDIO")
					(number "21")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "22")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "34")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "47")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "48")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{RESET}")
					(number "52")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "54")
				)
				(pin power_out line
					(at 22.86 0 180)
					(length 2.54)
					(name "VDDCORE")
					(number "55")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIN")
					(number "56")
				)
			)
			(symbol "ATSAMD21J17D-AFT_2_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "PA00")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "PA01")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "PA02")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PA03")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PA04")
					(number "13")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PA05")
					(number "14")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PA06")
					(number "15")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PA07")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PA08")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PA09")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PA10")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PA11")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PA12")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PA13")
					(number "30")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PA14")
					(number "31")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PA15")
					(number "32")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "PA16")
					(number "35")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "PA17")
					(number "36")
				)
				(pin bidirectional line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "PA18")
					(number "37")
				)
				(pin bidirectional line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "PA19")
					(number "38")
				)
				(pin bidirectional line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "PA20")
					(number "41")
				)
				(pin bidirectional line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "PA21")
					(number "42")
				)
				(pin bidirectional line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "PA22")
					(number "43")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "PA23")
					(number "44")
				)
				(pin bidirectional line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "PA24")
					(number "45")
				)
				(pin bidirectional line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "PA25")
					(number "46")
				)
				(pin bidirectional line
					(at 22.86 -27.94 180)
					(length 2.54)
					(name "PA27")
					(number "51")
				)
				(pin bidirectional line
					(at 22.86 -30.48 180)
					(length 2.54)
					(name "PA28")
					(number "53")
				)
				(pin bidirectional line
					(at 22.86 -35.56 180)
					(length 2.54)
					(name "PA30")
					(number "57")
				)
				(pin bidirectional line
					(at 22.86 -38.1 180)
					(length 2.54)
					(name "PA31")
					(number "58")
				)
			)
			(symbol "ATSAMD21J17D-AFT_3_1"
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PB04")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PB05")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PB06")
					(number "9")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PB07")
					(number "10")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PB08")
					(number "11")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PB09")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PB10")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PB11")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PB12")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PB13")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PB14")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PB15")
					(number "28")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "PB16")
					(number "39")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "PB17")
					(number "40")
				)
				(pin bidirectional line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "PB22")
					(number "49")
				)
				(pin bidirectional line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "PB23")
					(number "50")
				)
				(pin bidirectional line
					(at 22.86 -35.56 180)
					(length 2.54)
					(name "PB30")
					(number "59")
				)
				(pin bidirectional line
					(at 22.86 -38.1 180)
					(length 2.54)
					(name "PB31")
					(number "60")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "PB00")
					(number "61")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "PB01")
					(number "62")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "PB02")
					(number "63")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PB03")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
)
