(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ATXP032-CCUE-T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ATXP032-CCUE-T"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ATXP032-CCUE-T"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.renesas.com/jp/ja/document/oth/adesto-memory-nxp"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash 32 Mbit, 1.8V, -40 to 85 C, BGA 24-ball (Tape & Reel), High-speed Single"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ATXP032-CCUE-T"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Renesas"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ATXP032-CCUE-T_1_1"
				(pin no_connect line
					(at 17.78 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin no_connect line
					(at 17.78 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A3")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{RESET}")
					(number "A4")
				)
				(pin no_connect line
					(at 17.78 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "A5")
				)
				(pin no_connect line
					(at 17.78 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SCK")
					(number "B2")
				)
				(pin power_in line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "VSS")
					(number "B3")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VCC")
					(number "B4")
				)
				(pin no_connect line
					(at 17.78 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "B5")
				)
				(pin power_in line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "VSSQ")
					(number "C1")
				)
				(pin input line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "~{CS}")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DS")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DQ2")
					(number "C4")
				)
				(pin no_connect line
					(at 17.78 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C5")
				)
				(pin power_in line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "VCCQ")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DQ1")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DQ0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DQ3")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DQ4")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DQ7")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DQ6")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DQ5")
					(number "E3")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "E4")
				)
				(pin passive line
					(at 20.32 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "E5")
				)
			)
			(embedded_fonts no)
		)
)
