(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CC1101RGPR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CC1101RGPR"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CC1101RGPR"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fcc1101"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF Transceiver, Sub 1GHz, 2FSK, 4FSK, ASK, GFSK, MSK, OOK, 600Kbps, 1.8V to 3.6V, QFN-20"
				(at 38.1 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CC1101RGPR"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CC1101RGPR_1_1"
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCLK")
					(number "1")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SO(GDO1)")
					(number "2")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GDO2")
					(number "3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DVDD")
					(number "4")
				)
				(pin passive line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "DCOUPL")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GDO0")
					(number "6")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "~{CS}")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "XOSC_{Q1}")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "XOSC_{Q2}")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "AVDD")
					(number "11")
				)
				(pin bidirectional line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "RF+")
					(number "12")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "RF-")
					(number "13")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "15")
				)
				(pin power_in line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "GND")
					(number "16")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "R_{BIAS}")
					(number "17")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DGUARD")
					(number "18")
				)
				(pin passive line
					(at 25.4 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "19")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SI")
					(number "20")
				)
				(pin power_in line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "GND_{EP}")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
