(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CC1200RHBT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CC1200RHBT"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CC1200RHBT"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fcc1200"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC, low-cost sub-1 GHz transceiver"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CC1200RHBT"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, RF"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CC1200RHBT_1_1"
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VDD_GUARD")
					(number "1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{RESET}")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "GPIO3")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "GPIO4")
					(number "4")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "5")
				)
				(pin power_out line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "DCPL")
					(number "6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SI")
					(number "7")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SCLK")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SO(GPIO1)")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "GPIO0")
					(number "10")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "~{CS}")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DVDD")
					(number "12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD_IF")
					(number "13")
				)
				(pin power_in line
					(at 33.02 -48.26 180)
					(length 2.54)
					(name "RBIAS")
					(number "14")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVDD_RF")
					(number "15")
				)
				(pin no_connect line
					(at 30.48 -50.8 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "PA")
					(number "17")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 2.54)
					(name "TRX_SW")
					(number "18")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "LNA+")
					(number "19")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "LNA-")
					(number "20")
				)
				(pin power_in line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "DCPL_VCO")
					(number "21")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "AVDD_SYNTH1")
					(number "22")
				)
				(pin passive line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "LPF0")
					(number "23")
				)
				(pin passive line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "LPF1")
					(number "24")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "AVDD_PFD_CHP")
					(number "25")
				)
				(pin power_in line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "DCPL_PFD_CHP")
					(number "26")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "AVDD_SYNTH2")
					(number "27")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AVDD_XOSC")
					(number "28")
				)
				(pin power_in line
					(at 33.02 -43.18 180)
					(length 2.54)
					(name "DCPL_XOSC")
					(number "29")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "XOSC_Q1")
					(number "30")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "XOSC_Q2")
					(number "31")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "EXT_XOSC")
					(number "32")
				)
				(pin power_in line
					(at 33.02 -55.88 180)
					(length 2.54)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
