(footprint "VQFN-40-1EP_6x6mm_P0.5mm_EP4.5x4.5mm_H1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Based on: https://www.ti.com/lit/ds/symlink/cc2541.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1760970742770")
	(property "Reference" "REF**"
		(at -3.58 -3.63 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-40-1EP_6x6mm_P0.5mm_EP4.5x4.5mm_H1mm"
		(at -3.57 4.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -3.6 6.5 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.6 7.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.6 8.9 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.46 -1.46)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at -1.46 0)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at -1.46 1.46)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at 0 -1.46)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at 0 1.46)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at 1.46 -1.46)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at 1.46 0)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "" smd roundrect
		(at 1.46 1.46)
		(size 1.26 1.26)
		(layers "F.Paste")
		(roundrect_rratio 0.1075268817)
	)
	(pad "1" smd roundrect
		(at -2.9 -2.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "2" smd roundrect
		(at -2.9 -1.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "3" smd roundrect
		(at -2.9 -1.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "4" smd roundrect
		(at -2.9 -0.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "5" smd roundrect
		(at -2.9 -0.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "6" smd roundrect
		(at -2.9 0.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "7" smd roundrect
		(at -2.9 0.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "8" smd roundrect
		(at -2.9 1.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "9" smd roundrect
		(at -2.9 1.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "10" smd roundrect
		(at -2.9 2.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "11" smd roundrect
		(at -2.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "12" smd roundrect
		(at -1.75 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "13" smd roundrect
		(at -1.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "14" smd roundrect
		(at -0.75 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "15" smd roundrect
		(at -0.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "16" smd roundrect
		(at 0.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "17" smd roundrect
		(at 0.75 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "18" smd roundrect
		(at 1.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "19" smd roundrect
		(at 1.75 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "20" smd roundrect
		(at 2.25 2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "21" smd roundrect
		(at 2.9 2.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "22" smd roundrect
		(at 2.9 1.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "23" smd roundrect
		(at 2.9 1.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "24" smd roundrect
		(at 2.9 0.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "25" smd roundrect
		(at 2.9 0.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "26" smd roundrect
		(at 2.9 -0.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "27" smd roundrect
		(at 2.9 -0.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "28" smd roundrect
		(at 2.9 -1.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "29" smd roundrect
		(at 2.9 -1.75)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "30" smd roundrect
		(at 2.9 -2.25)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "31" smd roundrect
		(at 2.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "32" smd roundrect
		(at 1.75 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "33" smd roundrect
		(at 1.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "34" smd roundrect
		(at 0.75 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "35" smd roundrect
		(at 0.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "36" smd roundrect
		(at -0.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "37" smd roundrect
		(at -0.75 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "38" smd roundrect
		(at -1.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "39" smd roundrect
		(at -1.75 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "40" smd roundrect
		(at -2.25 -2.9 90)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "41" smd rect
		(at 0 0)
		(size 4.5 4.5)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(embedded_fonts no)
	(model "antmicro_cc2541f256rhar.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
