(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CC2541F256RHAR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CC2541F256RHAR"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CC2541F256RHAR"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fcc2541"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC, 2.4-GHz Bluetooth™ low energy and Proprietary System-on-Chip"
				(at 50.8 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CC2541F256RHAR"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CC2541F256RHAR_1_1"
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 2.54)
					(name "SDA")
					(number "3")
				)
				(pin no_connect line
					(at 33.02 -40.64 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "P1_5")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "P1_4")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "P1_3")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "P1_2")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "P1_1")
					(number "9")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DVDD2")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "P1_0")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "P0_7")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "P0_6")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "P0_5")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "P0_4")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "P0_3")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "P0_2")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 2.54)
					(name "P0_1")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 2.54)
					(name "P0_0")
					(number "19")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "RESET_N")
					(number "20")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AVDD5")
					(number "21")
				)
				(pin bidirectional line
					(at 35.56 -68.58 180)
					(length 2.54)
					(name "XOSC_Q1")
					(number "22")
				)
				(pin bidirectional line
					(at 35.56 -73.66 180)
					(length 2.54)
					(name "XOSC_Q2")
					(number "23")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "AVDD3")
					(number "24")
				)
				(pin passive line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "RF_P")
					(number "25")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 2.54)
					(name "RF_N")
					(number "26")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "AVDD2")
					(number "27")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVDD1")
					(number "28")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "AVDD4")
					(number "29")
				)
				(pin passive line
					(at 35.56 -78.74 180)
					(length 2.54)
					(name "RBIAS")
					(number "30")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "AVDD6")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "P2_4/OSC32K_Q1")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "P2_3/OSC32K_Q1")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "P2_2/DC")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "P2_1/DD")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "P2_0")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "P1_7")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "P1_6")
					(number "38")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DVDD1")
					(number "39")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DCOUPL")
					(number "40")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 2.54)
					(name "EP_GND")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
