(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CC2650F128RGZT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CC2650F128RGZT"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CC2650F128RGZT"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fcc2650"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC, SimpleLink™ Multistandard Wireless MCU"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CC2650F128RGZT"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, RF"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CC2650F128RGZT_1_1"
				(pin bidirectional line
					(at 40.64 -22.86 180)
					(length 2.54)
					(name "RF_P")
					(number "1")
				)
				(pin bidirectional line
					(at 40.64 -25.4 180)
					(length 2.54)
					(name "RF_N")
					(number "2")
				)
				(pin bidirectional line
					(at 40.64 -71.12 180)
					(length 2.54)
					(name "X32K_Q1")
					(number "3")
				)
				(pin bidirectional line
					(at 40.64 -76.2 180)
					(length 2.54)
					(name "X32K_Q2")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DIO_0")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DIO_1")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DIO_2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DIO_3")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DIO_4")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "DIO_5")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "DIO_6")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "DIO_7")
					(number "12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDS2")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DIO_8")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "DIO_9")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "DIO_10")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "DIO_11")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "DIO_12")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "DIO_13")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "DIO_14")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "DIO_15")
					(number "21")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDS3")
					(number "22")
				)
				(pin power_in line
					(at 40.64 -88.9 180)
					(length 2.54)
					(name "DCOUPL")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 2.54)
					(name "JTAG_TMSC")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 2.54)
					(name "JTAG_TCKC")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "DIO_16")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "DIO_17")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "DIO_18")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "DIO_19")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "DIO_20")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "DIO_21")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "DIO_22")
					(number "32")
				)
				(pin power_out line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DCDC_SW")
					(number "33")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDS_DCDC")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 2.54)
					(name "RESET_N")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "DIO_23")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 2.54)
					(name "DIO_24")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 2.54)
					(name "DIO_25")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 2.54)
					(name "DIO_26")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 2.54)
					(name "DIO_27")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 2.54)
					(name "DIO_28")
					(number "41")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 2.54)
					(name "DIO_29")
					(number "42")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 2.54)
					(name "DIO_30")
					(number "43")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDS")
					(number "44")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDDR")
					(number "45")
				)
				(pin bidirectional line
					(at 40.64 -63.5 180)
					(length 2.54)
					(name "X24M_N")
					(number "46")
				)
				(pin bidirectional line
					(at 40.64 -58.42 180)
					(length 2.54)
					(name "X24M_P")
					(number "47")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VDDR_RF")
					(number "48")
				)
				(pin power_in line
					(at 40.64 -109.22 180)
					(length 2.54)
					(name "EP_GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
