(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CC3200R1M2RGCR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CC3200R1M2RGCR"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CC3200R1M2RGCR"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fcc3200"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "32 Bit Microcontroller, SimpleLink Family CC32xx Series Microcontrollers, ARM Cortex-M4, 32 bit"
				(at 55.88 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CC3200R1M2RGCR"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CC3200R1M2RGCR_1_1"
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "GPIO10")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "GPIO11")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "GPIO12")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "GPIO13")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "GPIO14")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "GPIO15")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "GPIO16")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "GPIO17")
					(number "8")
				)
				(pin power_in line
					(at 43.18 -43.18 180)
					(length 2.54)
					(name "VDD_DIG1")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN_IO1")
					(number "10")
				)
				(pin output line
					(at 0 -96.52 0)
					(length 2.54)
					(name "FLASH_SPI_CLK")
					(number "11")
				)
				(pin output line
					(at 0 -99.06 0)
					(length 2.54)
					(name "FLASH_SPI_DOUT")
					(number "12")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 2.54)
					(name "FLASH_SPI_DIN")
					(number "13")
				)
				(pin output line
					(at 0 -101.6 0)
					(length 2.54)
					(name "FLASH_SPI_CS")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "GPIO22")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "TDI")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 2.54)
					(name "TDO")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "GPIO28")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 2.54)
					(name "TCK")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 2.54)
					(name "TMS")
					(number "20")
				)
				(pin output line
					(at 0 -106.68 0)
					(length 2.54)
					(name "SOP2")
					(number "21")
				)
				(pin input line
					(at 43.18 -96.52 180)
					(length 2.54)
					(name "WLAN_XTAL_N")
					(number "22")
				)
				(pin input line
					(at 43.18 -88.9 180)
					(length 2.54)
					(name "WLAN_XTAL_P")
					(number "23")
				)
				(pin power_in line
					(at 43.18 -63.5 180)
					(length 2.54)
					(name "VDD_PLL")
					(number "24")
				)
				(pin power_in line
					(at 43.18 -20.32 180)
					(length 2.54)
					(name "LDO_IN2")
					(number "25")
				)
				(pin no_connect line
					(at 40.64 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "26")
				)
				(pin no_connect line
					(at 40.64 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "27")
				)
				(pin no_connect line
					(at 40.64 -71.12 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin output line
					(at 43.18 -104.14 180)
					(length 2.54)
					(name "ANTSEL1")
					(number "29")
				)
				(pin output line
					(at 43.18 -106.68 180)
					(length 2.54)
					(name "ANTSEL2")
					(number "30")
				)
				(pin bidirectional line
					(at 43.18 0 180)
					(length 2.54)
					(name "RF_BG")
					(number "31")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "nRESET")
					(number "32")
				)
				(pin power_in line
					(at 43.18 -35.56 180)
					(length 2.54)
					(name "VDD_PA_IN")
					(number "33")
				)
				(pin output line
					(at 0 -109.22 0)
					(length 2.54)
					(name "SOP1")
					(number "34")
				)
				(pin output line
					(at 0 -111.76 0)
					(length 2.54)
					(name "SOP0")
					(number "35")
				)
				(pin input line
					(at 43.18 -17.78 180)
					(length 2.54)
					(name "LDO_IN1")
					(number "36")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN_DCDC_ANA")
					(number "37")
				)
				(pin input line
					(at 43.18 -5.08 180)
					(length 2.54)
					(name "DCDC_ANA_SW")
					(number "38")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VIN_DCDC_PA")
					(number "39")
				)
				(pin input line
					(at 43.18 -25.4 180)
					(length 2.54)
					(name "DCDC_PA_SW_P")
					(number "40")
				)
				(pin input line
					(at 43.18 -27.94 180)
					(length 2.54)
					(name "DCDC_PA_SW_N")
					(number "41")
				)
				(pin input line
					(at 43.18 -30.48 180)
					(length 2.54)
					(name "DCDC_PA_OUT")
					(number "42")
				)
				(pin input line
					(at 43.18 -40.64 180)
					(length 2.54)
					(name "DCDC_DIG_SW")
					(number "43")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VIN_DCDC_DIG")
					(number "44")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 2.54)
					(name "DCDC_ANA2_SW_P")
					(number "45")
				)
				(pin input line
					(at 43.18 -53.34 180)
					(length 2.54)
					(name "DCDC_ANA2_SW_N")
					(number "46")
				)
				(pin input line
					(at 43.18 -55.88 180)
					(length 2.54)
					(name "VDD_ANA2")
					(number "47")
				)
				(pin input line
					(at 43.18 -10.16 180)
					(length 2.54)
					(name "VDD_ANA1")
					(number "48")
				)
				(pin input line
					(at 43.18 -60.96 180)
					(length 2.54)
					(name "VDD_RAM")
					(number "49")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GPIO0")
					(number "50")
				)
				(pin output line
					(at 43.18 -73.66 180)
					(length 2.54)
					(name "RTC_XTAL_P")
					(number "51")
				)
				(pin output line
					(at 43.18 -81.28 180)
					(length 2.54)
					(name "RTC_XTAL_N")
					(number "52")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "GPIO30")
					(number "53")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VIN_IO2")
					(number "54")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "GPIO1")
					(number "55")
				)
				(pin power_in line
					(at 43.18 -45.72 180)
					(length 2.54)
					(name "VDD_DIG2")
					(number "56")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GPIO2")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GPIO3")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GPIO4")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "GPIO5")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "GPIO6")
					(number "61")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "GPIO7")
					(number "62")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "GPIO8")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GPIO9")
					(number "64")
				)
				(pin power_in line
					(at 43.18 -111.76 180)
					(length 2.54)
					(name "GND/TAB")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
