(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CD575M-A1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CD575M-A1"
				(at 71.12 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CD575M-A1"
				(at 71.12 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://developer.nvidia.com/embedded/tegra-k1-reference"
				(at 71.12 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Tegra K1 processors integrate a power optimized version of  Kepler GPU architecture. It supports OpenGL® 4.4, OpenGL ES 3.1 and CUDA®/GPGPU on mobile and embedded devices."
				(at 71.12 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CD575M-A1"
				(at 71.12 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nvidia"
				(at 71.12 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 71.12 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Displayed name" "Tegra K1 T124"
				(at 71.12 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SOC,MEMORY,HDMI,DSI,BGA,AUDIO,MIPI,MONITOR,PLL,SEMICONDUCTOR,VIDEO"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CD575M-A1_1_1"
				(text "AO"
					(at 25.4 0 900)
				)
				(text "CORE CLOCKS"
					(at 25.4 -13.97 900)
				)
				(text "DIGITAL I/O"
					(at 25.4 -41.91 900)
				)
				(text "DISPLAY/CAMERA"
					(at 25.4 -67.31 900)
				)
				(text "POWER"
					(at 27.94 -27.94 900)
				)
				(text "USB2.0/\nHSIC"
					(at 32.004 -1.778 900)
				)
				(text "USB 3.0+PCIe"
					(at 33.02 -13.97 900)
				)
				(text "SATA"
					(at 33.02 -27.94 900)
				)
				(text "FUSE"
					(at 33.02 -35.56 900)
				)
				(text "DRAM"
					(at 33.02 -43.18 900)
				)
				(text "GPU"
					(at 33.02 -53.34 900)
				)
				(text "CPU"
					(at 33.02 -58.42 900)
				)
				(text "CORE"
					(at 33.02 -63.5 900)
				)
				(text "GND"
					(at 33.02 -73.66 900)
				)
				(text "SENSE"
					(at 40.64 -86.36 0)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "A2")
					(alternate "GPIO3_PX.07" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "VDDIO_DDR_HS")
					(number "A17")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A30")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(hide yes)
					(name "AVDD_HDMI")
					(number "AA9")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "AVDD_HDMI")
					(number "AA10")
					(alternate "GPIO3_PN.01" passive line)
					(alternate "I2S0_SDATA_IN" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "VDD_CORE")
					(number "AA13")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA14")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA15")
					(alternate "GPIO3_PJ.06" passive line)
					(alternate "UB3_RTS" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA16")
					(alternate "GPIO3_PP.06" passive line)
					(alternate "I2S3_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA17")
					(alternate "GPIO3_PEE.00" passive line)
					(alternate "extperiph3_clk" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA18")
					(alternate "GPIO3_PU.03" passive line)
					(alternate "UA3_RTS" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA19")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "AA22")
					(alternate "GPIO3_PC.04" passive line)
					(alternate "I2C1_CLK" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "VDD_GPU")
					(number "AA23")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB2")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB7")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB11")
					(alternate "GPIO3_PA.02" passive line)
					(alternate "I2S1_LRCK" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "VDD_RTC")
					(number "AB12")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB13")
					(alternate "GPIO3_PK.07" passive line)
					(alternate "UD3_RTS" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB14")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "AVDD_PLL_UTMIP")
					(number "AB15")
					(alternate "CLK_32K_IN" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB16")
					(alternate "GPIO3_PI.07" passive line)
					(alternate "tracedata7" passive line)
				)
				(pin passive line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "AVDDIO_PEX")
					(number "AB17")
					(alternate "GPIO3_PZ.07" passive line)
					(alternate "I2CPMU_DAT" passive line)
				)
				(pin passive line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "DVDDIO_PEX")
					(number "AB18")
					(alternate "GPIO3_PY.04" passive line)
					(alternate "SDMMC1_DAT3" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB19")
				)
				(pin passive line
					(at 58.42 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "DVDDIO_PEX")
					(number "AB20")
					(alternate "GPIO3_PA.00" passive line)
					(alternate "soc_therm_oc2_n" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB21")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB25")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB30")
					(alternate "GPIO3_PH.04" passive line)
					(alternate "SDMMC2A_DAT0" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC9")
					(alternate "GPIO3_PJ.00" passive line)
					(alternate "wake33" passive line)
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "VDDIO_CAM")
					(number "AC11")
					(alternate "JTAG_TCK" passive line)
					(alternate "ST" passive line)
				)
				(pin passive line
					(at 58.42 0 180)
					(length 5.08)
					(name "AVDD_USB")
					(number "AC12")
					(alternate "0" passive line)
					(alternate "JTAG_TDO" passive line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VDDIO_BB")
					(number "AC14")
					(alternate "JTAG_TDI" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "VDDIO_HSIC")
					(number "AC15")
					(alternate "RTCK" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 58.42 -7.62 180)
					(length 5.08)
					(hide yes)
					(name "AVDDIO_PEX")
					(number "AC17")
					(alternate "GPIO3_PZ.06" passive line)
					(alternate "I2CPMU_CLK" passive line)
				)
				(pin passive line
					(at 58.42 -7.62 180)
					(length 5.08)
					(hide yes)
					(name "AVDDIO_PEX")
					(number "AC18")
					(alternate "JTAG_TMS" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 58.42 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "DVDDIO_PEX")
					(number "AC20")
					(alternate "SDMMC1_COMP_PU" passive line)
					(alternate "sdio1comp" passive line)
				)
				(pin passive line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "AVDD_PEX_PLL")
					(number "AC21")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD8")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE2")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE7")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE8")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE13")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE16")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE19")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE22")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE23")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE24")
					(alternate "GPIO3_PG.02" passive line)
					(alternate "tracedata0" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE25")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AE30")
				)
				(pin passive line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "VDDIO_PEX_CTL")
					(number "AE31")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "AVDD_LVDS0_PLL")
					(number "AF1")
					(alternate "GPIO3_PAA.03" passive line)
					(alternate "SDMMC4_DAT3" passive line)
				)
				(pin passive line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "HVDD_SATA")
					(number "AF31")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "AVDD_PLL_EREFE")
					(number "AG31")
					(alternate "GPIO3_PCC.04" passive line)
					(alternate "SDMMC4_CLK" passive line)
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "AVDD_HDMI_PLL")
					(number "AH1")
					(alternate "SDMMC4_COMP_PD" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH2")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH7")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH13")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH16")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH19")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH22")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH25")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH30")
				)
				(pin passive line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "AVDD_SATA_PLL")
					(number "AH31")
					(alternate "GPIO3" passive line)
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "AVDD_LVDS0_IO")
					(number "AJ1")
					(alternate "SDMMC4_COMP_PU" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK1")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK2")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK7")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK13")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "AVDD_CSI_DSI")
					(number "AK14")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK16")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK19")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK22")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK25")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK28")
				)
				(pin passive line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "VDDIO_SATA")
					(number "AK30")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK31")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "AVDD_PLL_UD2DPD")
					(number "AL4")
					(alternate "GPIO3_PB.07" passive line)
					(alternate "SDMMC3_DAT0" passive line)
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "AVDD_CSI_DSI")
					(number "AL13")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(hide yes)
					(name "AVDD_CSI_DSI")
					(number "AL14")
				)
				(pin passive line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "HVDD_PEX_PLL_E")
					(number "AL28")
				)
				(pin passive line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "HVDD_PEX")
					(number "AL29")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL30")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B1")
					(alternate "GPIO3_PV.02" passive line)
					(alternate "SDMMC3_CD_N" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B10")
					(alternate "GPIO3_PR.07" passive line)
					(alternate "wake49" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B13")
					(alternate "GPIO3_PI.02" passive line)
					(alternate "SDMMC2A_DAT6" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B16")
					(alternate "0" passive line)
					(alternate "CPU_PWR_REQ" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "AVDD_PLL_APC2C3")
					(number "B17")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B19")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B25")
					(alternate "GPIO3_PG.00" passive line)
					(alternate "boot_select0" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B31")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "AVDD_OSC")
					(number "D1")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D2")
					(alternate "GPIO3_PG.07" passive line)
					(alternate "SPI4C_DIN" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D7")
					(alternate "GPIO3_PR.00" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D13")
					(alternate "GPIO3_PR.05" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D16")
					(alternate "GPIO3_PJ.07" passive line)
					(alternate "UD3_TXD" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D19")
					(alternate "GPIO3_PS.03" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D22")
					(alternate "GPIO3_PK.02" passive line)
					(alternate "wake34" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D25")
					(alternate "0" passive line)
					(alternate "RESET_OUT_N" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D30")
					(alternate "GPIO3_PT.05" passive line)
					(alternate "I2C2_CLK" passive line)
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "VDDIO_SDMMC3")
					(number "E1")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "VDDIO_SDMMC4")
					(number "F31")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G4")
					(alternate "GPIO3_PG.01" passive line)
					(alternate "boot_select1" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G7")
					(alternate "PMICINTR" passive line)
					(alternate "wake18" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G10")
					(alternate "GPIO3_PG.04" passive line)
					(alternate "SPI4C_CS3" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G13")
					(alternate "GPIO3_PS.07" passive line)
					(alternate "soc_therm_oc1_n" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G19")
					(alternate "GPIO3_PI.03" passive line)
					(alternate "SPI4C_CS0" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G22")
					(alternate "GPIO3_PJ.02" passive line)
					(alternate "soc_therm_oc4_n" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G24")
					(alternate "GPIO3_PR.01" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G25")
					(alternate "GPIO3_PH.03" passive line)
					(alternate "PM3_PWM3" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "G30")
					(alternate "GPIO3_PI.00" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H8")
					(alternate "GPIO3_PS.04" passive line)
					(alternate "wake25" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "H24")
					(alternate "GPIO3_PB.01" passive line)
					(alternate "UD3_CTS" passive line)
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J9")
					(alternate "GPIO3_PN.00" passive line)
					(alternate "I2S0_LRCK" passive line)
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "VDDIO_DDR")
					(number "J11")
					(alternate "GPIO3_PW.05" passive line)
					(alternate "extperiph2_clk" passive line)
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J12")
					(alternate "GPIO3_PW.03" passive line)
					(alternate "wake11" passive line)
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J14")
				)
				(pin passive line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "VDDIO_DDR_MCLK")
					(number "J15")
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J17")
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J18")
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J20")
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "J21")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J23")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "AVDD_PLL_CG")
					(number "J31")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K2")
					(alternate "GPIO3_PH.00" passive line)
					(alternate "PM3_PWM0" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K4")
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "K10")
				)
				(pin passive line
					(at 58.42 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_DDR")
					(number "K11")
					(alternate "GPIO3_PA.05" passive line)
					(alternate "I2S1_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K12")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K13")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K14")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K15")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "AVDD_PLL_M")
					(number "K16")
					(alternate "GPIO3_PB.06" passive line)
					(alternate "SDMMC3_DAT1" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K17")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K18")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K19")
					(alternate "1" passive line)
					(alternate "PWRON" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K20")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "K21")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K22")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K28")
					(alternate "GPIO3_PG.06" passive line)
					(alternate "SPI4C_DOUT" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K30")
					(alternate "GPIO3_PR.04" passive line)
					(alternate "wake50" passive line)
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VDDIO_AUDIO")
					(number "K31")
					(alternate "JTAG_TRST_N" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "VDDIO_SYS_2")
					(number "L10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L13")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L15")
					(alternate "GPIO3_PI.04" passive line)
					(alternate "SPI4C_CS1" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L16")
					(alternate "GPIO3_PX.05" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L17")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L18")
					(alternate "GPIO3_PX.01" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L19")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L22")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "VDD_CPU")
					(number "L23")
					(alternate "GPIO3_PA.04" passive line)
					(alternate "I2S1_SDATA_IN" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "L24")
					(alternate "GPIO3_PU.02" passive line)
					(alternate "UA3_CTS" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "L25")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "L26")
					(alternate "GPIO3_PW.02" passive line)
					(alternate "wake12" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "L27")
					(alternate "GPIO3_PX.03" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "AVDD_PLL_X")
					(number "L31")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "M12")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M13")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M14")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M15")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M16")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M17")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M18")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M19")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M20")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M22")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M23")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M24")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M25")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M26")
					(alternate "GPIO3_PA.03" passive line)
					(alternate "I2S1_SCLK" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "M27")
					(alternate "GPIO3_PEE.02" passive line)
					(alternate "SATA_DEV_SLP" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N2")
					(alternate "GPIO3_PK.04" passive line)
					(alternate "SDMMC2A_DAT5" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N10")
					(alternate "CLDVFS_PWM" passive line)
					(alternate "GPIO3_PX.00" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N11")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "N12")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N13")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N14")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N15")
					(alternate "GPIO3_PN.02" passive line)
					(alternate "I2S0_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N16")
					(alternate "GPIO3" passive line)
					(alternate "GPIO3_PW.04" passive line)
					(alternate "extperiph1_clk" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N17")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N18")
					(alternate "GPIO3_PJ.05" passive line)
					(alternate "UB3_CTS" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N19")
					(alternate "GPIO3_PW.06" passive line)
					(alternate "UC3_TXD" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N20")
					(alternate "GPIO3_PW.07" passive line)
					(alternate "UC3_RXD" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N21")
					(alternate "GPIO3_PU.05" passive line)
					(alternate "wake6" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N22")
					(alternate "GPIO3_PU.06" passive line)
					(alternate "wake7" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "N25")
					(alternate "GPIO3_PC.05" passive line)
					(alternate "I2C1_DAT" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N30")
					(alternate "GPIO3_PN.03" passive line)
					(alternate "I2S0_SCLK" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "VDDIO_SDMMC1")
					(number "P9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "AVDD_PLL_C4")
					(number "P10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P11")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "P12")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P13")
					(alternate "GPIO3_PEE.01" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P14")
					(alternate "GPIO3_PC.02" passive line)
					(alternate "IR3_TXD" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P15")
					(alternate "GPIO3_PU.04" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P16")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P17")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P18")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P19")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P20")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P21")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P22")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "P23")
					(alternate "GPIO3_PP.07" passive line)
					(alternate "I2S3_SCLK" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P24")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "VDD_CORE_SENSE")
					(number "P25")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "GND_CORE_SENSE")
					(number "P26")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "VVDD_CORE_PROBE")
					(number "P27")
				)
				(pin passive line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "VPP_FUSE")
					(number "R10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R11")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "R12")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R13")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R14")
					(alternate "GPIO3_PI.06" passive line)
					(alternate "SDMMC2A_DAT7" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R15")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R16")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R17")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R18")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R19")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R20")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R21")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R22")
				)
				(pin passive line
					(at 58.42 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "R23")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R24")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "VVDD_CPU_PROBE")
					(number "R25")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "VDD_CPU_SENSE")
					(number "R26")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "GND_CPU_SENSE")
					(number "R27")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T2")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T7")
					(alternate "GPIO3_PK.03" passive line)
					(alternate "SDMMC2A_DAT4" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T11")
					(alternate "GPIO3_PC.07" passive line)
					(alternate "wake8" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "T12")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T13")
					(alternate "GPIO3_PK.01" passive line)
					(alternate "SDMMC2A_CLK" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T14")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T15")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T16")
					(alternate "GPIO3_PH.07" passive line)
					(alternate "SDMMC2A_CMD" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T17")
					(alternate "GPIO3_PH.05" passive line)
					(alternate "SDMMC2A_DAT2" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T18")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T19")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T20")
					(alternate "GPIO3_PH.01" passive line)
					(alternate "PM3_PWM1" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T21")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T22")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T25")
					(alternate "GPIO3_PB.00" passive line)
					(alternate "UD3_RXD" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T28")
					(alternate "SDMMC2_COMP_PD" passive line)
					(alternate "sdio2comp" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T30")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T31")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VDDIO_GMI")
					(number "U9")
					(alternate "ST" passive line)
					(alternate "TEST_MODE_" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "VDDIO_UART")
					(number "U10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U11")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "U12")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U13")
					(alternate "SDMMC2_COMP_PU" passive line)
					(alternate "sdio2comp" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U14")
					(alternate "GPIO3_PU.00" passive line)
					(alternate "UA3_TXD" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U15")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U16")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "U17")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "U18")
					(alternate "GPIO3_PZ.01" passive line)
					(alternate "SDMMC1_CMD" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "U19")
					(alternate "GPIO3_PC.03" passive line)
					(alternate "IR3_RXD" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "U20")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "U21")
					(alternate "SDMMC1_COMP_PD" passive line)
					(alternate "sdio1comp" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U22")
					(alternate "GPIO3_PA.01" passive line)
					(alternate "UC3_CTS" passive line)
				)
				(pin passive line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "VVDD_GPU_PROBE")
					(number "U25")
				)
				(pin passive line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "VDD_GPU_SENSE")
					(number "U26")
				)
				(pin passive line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "GND_GPU_SENSE")
					(number "U27")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(hide yes)
					(name "VDDIO_GMI")
					(number "V10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "V12")
					(alternate "GPIO3_PX.06" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V13")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V14")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V15")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V16")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V17")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V18")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V19")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V20")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "V21")
					(alternate "GPIO3_PZ.00" passive line)
					(alternate "SDMMC1_CLK" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V22")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "VDDIO_SYS")
					(number "V23")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V27")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W2")
					(alternate "GPIO3_PI.05" passive line)
					(alternate "SDMMC2A_DAT1" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W4")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W7")
					(alternate "GPIO3_PC.00" passive line)
					(alternate "UC3_RTS" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W10")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W11")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "W12")
					(alternate "GPIO3_PP.04" passive line)
					(alternate "I2S3_LRCK" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W13")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W14")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W15")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W16")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W17")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W18")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W19")
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W20")
					(alternate "GPIO3_PY.05" passive line)
					(alternate "SDMMC1_DAT2" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "W21")
					(alternate "GPIO3_PY.07" passive line)
					(alternate "SDMMC1_DAT0" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
					(alternate "GPIO3_PH.06" passive line)
					(alternate "SDMMC2A_DAT3" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W25")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W28")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W30")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VDDIO_HV")
					(number "Y10")
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "Y12")
					(alternate "GPIO3_PU.01" passive line)
					(alternate "UA3_RXD" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y13")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y14")
					(alternate "GPIO3_PX.04" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y15")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y16")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y17")
				)
				(pin passive line
					(at 58.42 -73.66 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y18")
					(alternate "CLDVFS_CLK" passive line)
					(alternate "GPIO3_PX.02" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "Y19")
					(alternate "GPIO3_PY.06" passive line)
					(alternate "SDMMC1_DAT1" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "Y20")
					(alternate "GPIO3_PCC.05" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 58.42 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "Y22")
					(alternate "GPIO3_PP.05" passive line)
					(alternate "I2S3_SDATA_IN" passive line)
				)
				(pin passive line
					(at 58.42 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDD_GPU")
					(number "Y23")
					(alternate "GPIO3_PV.03" passive line)
					(alternate "SDMMC1_WP_N" passive line)
				)
			)
			(symbol "CD575M-A1_2_1"
				(text "SYS"
					(at 22.86 -35.56 900)
				)
				(text "HV"
					(at 22.86 -88.9 900)
				)
				(text "UART"
					(at 22.86 -124.46 900)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "OWR")
					(number "AA7")
					(alternate "GPIO3_PBB.04" passive line)
					(alternate "OWR" passive line)
					(alternate "VGP4" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "SPDIF_IN")
					(number "AA8")
					(alternate "GPIO3_PK.06" passive line)
					(alternate "SPDIF_IN" passive line)
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "KB_COL7")
					(number "AA25")
					(alternate "GPIO3_PQ.07" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -63.5 180)
					(length 5.08)
					(name "KB_ROW16")
					(number "AA26")
					(alternate "GPIO3_PT.00" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "KB_COL5")
					(number "AA27")
					(alternate "GPIO3_PQ.05" passive line)
					(alternate "wake54" passive line)
				)
				(pin passive line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "KB_ROW9")
					(number "AA28")
					(alternate "GPIO3_PO.01" passive line)
					(alternate "GPIO3_PS.01" passive line)
					(alternate "UA3_TXD" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "KB_ROW8")
					(number "AA29")
					(alternate "GPIO3_PS.00" passive line)
					(alternate "wake27" passive line)
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SYS_RESET_N")
					(number "AA30")
					(alternate "SYS_RESET_N" passive line)
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "KB_ROW10")
					(number "AA31")
					(alternate "GPIO3_PS.02" passive line)
					(alternate "UA3_RXD" passive line)
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "USB_VBUS_EN0")
					(number "AB1")
					(alternate "GPIO3_PN.04" passive line)
					(alternate "usb_vbus_en0" passive line)
				)
				(pin passive line
					(at 45.72 -38.1 180)
					(length 5.08)
					(name "KB_ROW6")
					(number "AB31")
					(alternate "DCA_LSPII" passive line)
					(alternate "GPIO3_PR.06" passive line)
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "USB_VBUS_EN1")
					(number "AC1")
					(alternate "GPIO3_PN.05" passive line)
					(alternate "usb_vbus_en1" passive line)
				)
				(pin passive line
					(at 45.72 -78.74 180)
					(length 5.08)
					(name "DP_HPD")
					(number "AC2")
					(alternate "DP_HPD" passive line)
					(alternate "GPIO3_PFF.00" passive line)
					(alternate "GPIO3_PO.06" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "HDMI_INT")
					(number "AC3")
					(alternate "GPIO3_PN.07" passive line)
					(alternate "wake4" passive line)
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "SPDIF_OUT")
					(number "AC4")
					(alternate "GPIO3_PK.05" passive line)
					(alternate "SPDIF_OUT" passive line)
				)
				(pin passive line
					(at 45.72 -90.17 180)
					(length 5.08)
					(name "DP_AUX_CH0_N")
					(number "AC5")
					(alternate "I2C6_DAT" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 45.72 -87.63 180)
					(length 5.08)
					(name "DP_AUX_CH0_P")
					(number "AC6")
					(alternate "GPIO3_PO.02" passive line)
					(alternate "I2C6_CLK" passive line)
					(alternate "pu" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 45.72 -99.06 180)
					(length 5.08)
					(name "DDC_SCL")
					(number "AC7")
					(alternate "GPIO3_PV.04" passive line)
					(alternate "I2C4_CLK" passive line)
				)
				(pin passive line
					(at 45.72 -101.6 180)
					(length 5.08)
					(name "DDC_SDA")
					(number "AC8")
					(alternate "GPIO3_PV.05" passive line)
					(alternate "I2C4_DAT" passive line)
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "KB_COL1")
					(number "AC28")
					(alternate "GPIO3_PQ.01" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -66.04 180)
					(length 5.08)
					(name "KB_ROW17")
					(number "AC29")
					(alternate "GPIO3_PT.01" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "KB_ROW14")
					(number "AC30")
					(alternate "GPIO3_PS.06" passive line)
					(alternate "wake28" passive line)
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "KB_ROW3")
					(number "AC31")
					(alternate "GPIO3_PR.03" passive line)
					(alternate "SYS_CLK_REQ" passive line)
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "HDMI_CEC")
					(number "AD7")
					(alternate "CEC" passive line)
					(alternate "GPIO3_PEE.03" passive line)
				)
				(pin passive line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "KB_COL2")
					(number "AD28")
					(alternate "GPIO3_PP.02" passive line)
					(alternate "GPIO3_PQ.02" passive line)
					(alternate "I2S2_SDATA_OUT" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "KB_COL6")
					(number "AD29")
					(alternate "GPIO3_PQ.06" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 0 180)
					(length 5.08)
					(name "KB_COL0")
					(number "AD30")
					(alternate "GPIO3_PP.00" passive line)
					(alternate "GPIO3_PQ.00" passive line)
					(alternate "I2S2_LRCK" passive line)
					(alternate "wake51" passive line)
				)
				(pin passive line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "KB_COL3")
					(number "AD31")
					(alternate "GPIO3_PQ.03" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "KB_COL4")
					(number "AF28")
					(alternate "GPIO3_PQ.04" passive line)
					(alternate "SDMMC3_WP_N" passive line)
				)
				(pin passive line
					(at 45.72 -55.88 180)
					(length 5.08)
					(name "KB_ROW13")
					(number "AF29")
					(alternate "GPIO3_PS.05" passive line)
					(alternate "wake26" passive line)
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "KB_ROW2")
					(number "AF30")
					(alternate "GPIO3_PR.02" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "XTAL_IN")
					(number "E3")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "XTAL_OUT")
					(number "E4")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "CLK_32K_IN")
					(number "H3")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "JTAG_TRST_N")
					(number "H4")
					(alternate "JTAG_TRST_N" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "JTAG_TDI")
					(number "H5")
					(alternate "GPIO3_PS.05" passive line)
					(alternate "JTAG_TDI" passive line)
					(alternate "pu" passive line)
					(alternate "wake26" passive line)
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "JTAG_TCK")
					(number "H6")
					(alternate "GPIO3_PQ.04" passive line)
					(alternate "JTAG_TCK" passive line)
					(alternate "SDMMC3_WP_N" passive line)
					(alternate "ST" passive line)
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "TEST_MODE_EN")
					(number "H7")
					(alternate "GPIO3_PR.02" passive line)
					(alternate "ST" passive line)
					(alternate "TEST_MODE_" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "JTAG_TDO")
					(number "J1")
					(alternate "0" passive line)
					(alternate "JTAG_TDO" passive line)
					(alternate "PEX_CLK_OUT_1_P" passive line)
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "JTAG_RTCK")
					(number "J2")
					(alternate "RTCK" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PWR_I2C_SDA")
					(number "J3")
					(alternate "GPIO3_PZ.07" passive line)
					(alternate "I2CPMU_DAT" passive line)
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PWR_I2C_SCL")
					(number "J4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "JTAG_TMS")
					(number "J5")
					(alternate "JTAG_TMS" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "CLK_32K_OUT")
					(number "J6")
					(alternate "GPIO3_PA.00" passive line)
					(alternate "soc_therm_oc2_n" passive line)
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "UART2_RXD")
					(number "L9")
					(alternate "GPIO3_PC.03" passive line)
					(alternate "GPIO3_PFF.02" passive line)
					(alternate "IR3_RXD" passive line)
					(alternate "SATA_DA" passive line)
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "UART2_CTS_N")
					(number "M1")
					(alternate "GPIO3_PDD.03" passive line)
					(alternate "GPIO3_PJ.05" passive line)
					(alternate "UB3_CTS" passive line)
					(alternate "pe_wake_l" passive line)
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "UART3_TXD")
					(number "M2")
					(alternate "GPIO3_PBB.05" passive line)
					(alternate "GPIO3_PW.06" passive line)
					(alternate "UC3_TXD" passive line)
					(alternate "VGP5" passive line)
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "UART3_RXD")
					(number "M3")
					(alternate "GPIO3_PW.07" passive line)
					(alternate "UC3_RXD" passive line)
				)
				(pin passive line
					(at 45.72 -134.62 180)
					(length 5.08)
					(name "GPIO_PU5")
					(number "M4")
					(alternate "0" passive line)
					(alternate "GPIO3_PU.05" passive line)
					(alternate "PEX_CLK_OUT_1_N" passive line)
					(alternate "wake6" passive line)
				)
				(pin passive line
					(at 45.72 -137.16 180)
					(length 5.08)
					(name "GPIO_PU6")
					(number "M5")
					(alternate "GPIO3_PU.06" passive line)
					(alternate "wake7" passive line)
				)
				(pin passive line
					(at 0 -147.32 0)
					(length 5.08)
					(name "GEN1_I2C_SDA")
					(number "M6")
					(alternate "GPIO3_PC.05" passive line)
					(alternate "GPIO3_PV.00" passive line)
					(alternate "I2C1_DAT" passive line)
					(alternate "wake24" passive line)
				)
				(pin passive line
					(at 45.72 -144.78 180)
					(length 5.08)
					(name "CLK3_REQ")
					(number "M7")
					(alternate "GPIO3_PBB.02" passive line)
					(alternate "GPIO3_PEE.01" passive line)
					(alternate "I2C3_DAT" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "UART2_TXD")
					(number "M8")
					(alternate "GPIO3_PC.02" passive line)
					(alternate "IR3_TXD" passive line)
				)
				(pin passive line
					(at 45.72 -132.08 180)
					(length 5.08)
					(name "GPIO_PU4")
					(number "M9")
					(alternate "GPIO3_PU.04" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 45.72 -127 180)
					(length 5.08)
					(name "GPIO_PU2")
					(number "M10")
					(alternate "GPIO3_PU.02" passive line)
					(alternate "UA3_CTS" passive line)
				)
				(pin passive line
					(at 45.72 -114.3 180)
					(length 5.08)
					(name "DAP4_SCLK")
					(number "N1")
					(alternate "GPIO3_PP.07" passive line)
					(alternate "I2S3_SCLK" passive line)
				)
				(pin passive line
					(at 45.72 -109.22 180)
					(length 5.08)
					(name "DAP4_FS")
					(number "P1")
					(alternate "GPIO3_PP.04" passive line)
					(alternate "I2S3_LRCK" passive line)
				)
				(pin passive line
					(at 45.72 -124.46 180)
					(length 5.08)
					(name "GPIO_PU1")
					(number "P2")
					(alternate "GPIO3_PU.01" passive line)
					(alternate "UA3_RXD" passive line)
				)
				(pin passive line
					(at 45.72 -111.76 180)
					(length 5.08)
					(name "DAP4_DIN")
					(number "P3")
					(alternate "GPIO3_PP.05" passive line)
					(alternate "I2S3_SDATA_IN" passive line)
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "UART2_RTS_N")
					(number "P4")
					(alternate "GPIO3_PFF.01" passive line)
					(alternate "GPIO3_PJ.06" passive line)
					(alternate "UB3_RTS" passive line)
					(alternate "usb_vbus_en2" passive line)
				)
				(pin passive line
					(at 45.72 -106.68 180)
					(length 5.08)
					(name "DAP4_DOUT")
					(number "P5")
					(alternate "GPIO3_PP.06" passive line)
					(alternate "I2S3_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 0 -144.78 0)
					(length 5.08)
					(name "GEN1_I2C_SCL")
					(number "P6")
					(alternate "GPIO3_PC.04" passive line)
					(alternate "GPIO3_PY.02" passive line)
					(alternate "I2C1_CLK" passive line)
					(alternate "SPI1A_SCK" passive line)
				)
				(pin passive line
					(at 45.72 -147.32 180)
					(length 5.08)
					(name "CLK3_OUT")
					(number "P7")
					(alternate "GPIO3_PEE.00" passive line)
					(alternate "extperiph3_clk" passive line)
				)
				(pin passive line
					(at 45.72 -129.54 180)
					(length 5.08)
					(name "GPIO_PU3")
					(number "P8")
					(alternate "GPIO3_PU.03" passive line)
					(alternate "UA3_RTS" passive line)
				)
				(pin passive line
					(at 45.72 -121.92 180)
					(length 5.08)
					(name "GPIO_PU0")
					(number "R7")
					(alternate "GPIO3_PU.00" passive line)
					(alternate "UA3_TXD" passive line)
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "UART3_CTS_N")
					(number "R8")
					(alternate "GPIO3_PA.01" passive line)
					(alternate "UC3_CTS" passive line)
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "UART3_RTS_N")
					(number "R9")
					(alternate "GPIO3_PC.00" passive line)
					(alternate "UC3_RTS" passive line)
				)
				(pin passive line
					(at 45.72 -71.12 180)
					(length 5.08)
					(name "THERM_DP")
					(number "U28")
				)
				(pin passive line
					(at 45.72 -73.66 180)
					(length 5.08)
					(name "THERM_DN")
					(number "U29")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "SDMMC3_CD_N")
					(number "V24")
					(alternate "GPIO3_PP.01" passive line)
					(alternate "GPIO3_PV.02" passive line)
					(alternate "I2S2_SDATA_IN" passive line)
					(alternate "SDMMC3_CD_N" passive line)
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "CPU_PWR_REQ")
					(number "V25")
					(alternate "0" passive line)
					(alternate "CPU_PWR_REQ" passive line)
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "KB_ROW11")
					(number "V28")
					(alternate "GPIO3_PS.03" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "PWR_INT_N")
					(number "V30")
				)
				(pin passive line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "KB_ROW0")
					(number "W31")
					(alternate "GPIO3_PR.00" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "RESET_OUT_N")
					(number "Y24")
				)
				(pin passive line
					(at 45.72 -60.96 180)
					(length 5.08)
					(name "KB_ROW15")
					(number "Y25")
					(alternate "GPIO3_PS.07" passive line)
					(alternate "soc_therm_oc1_n" passive line)
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "KB_ROW1")
					(number "Y26")
					(alternate "GPIO3_PR.01" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 45.72 -53.34 180)
					(length 5.08)
					(name "KB_ROW12")
					(number "Y27")
					(alternate "GPIO3_PS.04" passive line)
					(alternate "wake25" passive line)
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "CORE_PWR_REQ")
					(number "Y28")
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "KB_ROW4")
					(number "Y29")
					(alternate "GPIO3_PBB.01" passive line)
					(alternate "GPIO3_PR.04" passive line)
					(alternate "I2C3_CLK" passive line)
					(alternate "wake50" passive line)
				)
				(pin passive line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "KB_ROW7")
					(number "Y30")
					(alternate "GPIO3_PR.07" passive line)
					(alternate "wake49" passive line)
				)
				(pin passive line
					(at 45.72 -35.56 180)
					(length 5.08)
					(name "KB_ROW5")
					(number "Y31")
					(alternate "GPIO3_PR.05" passive line)
					(alternate "pd" passive line)
				)
			)
			(symbol "CD575M-A1_3_1"
				(text "USB 2.0"
					(at 22.86 -7.62 900)
				)
				(text "USB 3.0+PEX"
					(at 22.86 -40.64 900)
				)
				(text "BB"
					(at 22.86 -116.84 900)
				)
				(text "HSIC"
					(at 22.86 -139.7 900)
				)
				(text "PCIE Express CTRL"
					(at 25.4 -86.36 900)
				)
				(pin passive line
					(at 45.72 -96.52 180)
					(length 5.08)
					(name "PEX_CLK2P")
					(number "AC26")
					(alternate "0" passive line)
					(alternate "GPIO3_PT.01" passive line)
					(alternate "PEX_CLK_OUT_2_P" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 45.72 -99.06 180)
					(length 5.08)
					(name "PEX_CLK2N")
					(number "AC27")
					(alternate "0" passive line)
					(alternate "GPIO3_PS.06" passive line)
					(alternate "PEX_CLK_OUT_2_N" passive line)
					(alternate "wake28" passive line)
				)
				(pin passive line
					(at 45.72 -132.08 180)
					(length 5.08)
					(name "GPIO_PV1")
					(number "AD15")
					(alternate "GPIO3_PV.01" passive line)
					(alternate "wake1" passive line)
				)
				(pin passive line
					(at 45.72 -109.22 180)
					(length 5.08)
					(name "ULPI_DATA2")
					(number "AD17")
					(alternate "GPIO3_PO.03" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -144.78 180)
					(length 5.08)
					(name "HSIC2_STROBE")
					(number "AD18")
				)
				(pin passive line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "USB2_DP")
					(number "AD20")
					(alternate "GPIO3_PEE.05" passive line)
					(alternate "SDMMC3_CLK_LB_IN" passive line)
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "PEX_RX2P")
					(number "AD21")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "DAP3_FS")
					(number "AE15")
					(alternate "GPIO3_PP.00" passive line)
					(alternate "I2S2_LRCK" passive line)
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "DAP3_DOUT")
					(number "AE17")
					(alternate "GPIO3_PP.02" passive line)
					(alternate "I2S2_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 5.08)
					(name "HSIC1_STROBE")
					(number "AE18")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "USB2_DN")
					(number "AE20")
					(alternate "GPIO3_PA.07" passive line)
					(alternate "SDMMC3_CMD" passive line)
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "PEX_RX2N")
					(number "AE21")
				)
				(pin passive line
					(at 45.72 -104.14 180)
					(length 5.08)
					(name "ULPI_DATA0")
					(number "AF15")
					(alternate "GPIO3_PO.01" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "DAP3_DIN")
					(number "AF17")
					(alternate "GPIO3_PP.01" passive line)
					(alternate "I2S2_SDATA_IN" passive line)
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(name "HSIC1_DATA")
					(number "AF18")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "USB1_DN")
					(number "AF20")
					(alternate "GPIO3_PT.07" passive line)
					(alternate "SDMMC4_CMD" passive line)
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PEX_USB3_TX1P")
					(number "AF21")
				)
				(pin passive line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "PEX_TX3P")
					(number "AF23")
					(alternate "GPIO3_PAA.00" passive line)
					(alternate "SDMMC4_DAT0" passive line)
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PEX_TESTCLKN")
					(number "AF24")
				)
				(pin passive line
					(at 45.72 -73.66 180)
					(length 5.08)
					(name "PEX_CLK1P")
					(number "AF26")
					(alternate "0" passive line)
					(alternate "PEX_CLK_OUT_1_P" passive line)
					(alternate "PEX_CLK_OUT_2_N" passive line)
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "ULPI_NXT")
					(number "AG15")
					(alternate "GPIO3_PI.01" passive line)
					(alternate "GPIO3_PY.02" passive line)
					(alternate "SPI1A_SCK" passive line)
					(alternate "force_recovery" passive line)
				)
				(pin passive line
					(at 45.72 -129.54 180)
					(length 5.08)
					(name "GPIO_PV0")
					(number "AG17")
					(alternate "GPIO3_PV.00" passive line)
					(alternate "wake24" passive line)
				)
				(pin passive line
					(at 45.72 -142.24 180)
					(length 5.08)
					(name "HSIC2_DATA")
					(number "AG18")
				)
				(pin passive line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "USB1_DP")
					(number "AG20")
					(alternate "GPIO3_PB.05" passive line)
					(alternate "SDMMC3_DAT2" passive line)
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PEX_USB3_TX1N")
					(number "AG21")
				)
				(pin passive line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "PEX_TX3N")
					(number "AG23")
					(alternate "GPIO3_PAA.07" passive line)
					(alternate "SDMMC4_DAT7" passive line)
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PEX_TESTCLKP")
					(number "AG24")
				)
				(pin passive line
					(at 45.72 -76.2 180)
					(length 5.08)
					(name "PEX_CLK1N")
					(number "AG26")
					(alternate "0" passive line)
					(alternate "GPIO3_PQ.01" passive line)
					(alternate "PEX_CLK_OUT_1_N" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PEX_WAKE_N")
					(number "AG28")
					(alternate "GPIO3_PDD.03" passive line)
					(alternate "pe_wake_l" passive line)
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "USB_VBUS_EN2")
					(number "AG29")
					(alternate "GPIO3_PFF.01" passive line)
					(alternate "usb_vbus_en2" passive line)
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "GPIO_PFF2")
					(number "AG30")
					(alternate "GPIO3_PFF.02" passive line)
					(alternate "PEX_CLK_OUT_2_P" passive line)
					(alternate "SATA_DA" passive line)
				)
				(pin passive line
					(at 45.72 -106.68 180)
					(length 5.08)
					(name "ULPI_DATA1")
					(number "AH15")
					(alternate "GPIO3_PO.02" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 45.72 -116.84 180)
					(length 5.08)
					(name "ULPI_DATA5")
					(number "AH17")
					(alternate "GPIO3_PO.06" passive line)
					(alternate "GPIO3_PT.06" passive line)
					(alternate "I2C2_DAT" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -144.78 0)
					(length 5.08)
					(name "HSIC_REXT")
					(number "AH18")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "USB0_DN")
					(number "AH20")
					(alternate "GPIO3_PAA.06" passive line)
					(alternate "SDMMC4_DAT6" passive line)
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "USB3_TX0P")
					(number "AH21")
				)
				(pin passive line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "PEX_TX2P")
					(number "AH23")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PEX_REFCLKP")
					(number "AH24")
				)
				(pin passive line
					(at 45.72 -60.96 180)
					(length 5.08)
					(name "PEX_TX4N")
					(number "AH26")
					(alternate "GPIO3_PB.04" passive line)
					(alternate "SDMMC3_DAT3" passive line)
				)
				(pin passive line
					(at 45.72 -111.76 180)
					(length 5.08)
					(name "ULPI_DATA3")
					(number "AJ15")
					(alternate "GPIO3_PO.04" passive line)
					(alternate "wake32" passive line)
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "DAP3_SCLK")
					(number "AJ17")
					(alternate "GPIO3_PP.03" passive line)
					(alternate "I2S2_SCLK" passive line)
				)
				(pin passive line
					(at 45.72 -114.3 180)
					(length 5.08)
					(name "ULPI_DATA4")
					(number "AJ18")
					(alternate "GPIO3_PK.00" passive line)
					(alternate "GPIO3_PO.05" passive line)
					(alternate "soc_therm_oc3_n" passive line)
					(alternate "wake0" passive line)
				)
				(pin passive line
					(at 45.72 0 180)
					(length 5.08)
					(name "USB0_DP")
					(number "AJ20")
					(alternate "GPIO3_PAA.05" passive line)
					(alternate "SDMMC4_DAT5" passive line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "USB3_TX0N")
					(number "AJ21")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "PEX_TX2N")
					(number "AJ23")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PEX_REFCLKN")
					(number "AJ24")
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "PEX_TX4P")
					(number "AJ26")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PEX_L0_RST_N")
					(number "AJ29")
					(alternate "GPIO3_PDD.01" passive line)
					(alternate "pe0_rst_l" passive line)
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PEX_L1_CLKREQ_N")
					(number "AJ30")
					(alternate "GPIO3_PDD.06" passive line)
					(alternate "pe1_clkreq_l" passive line)
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PEX_L1_RST_N")
					(number "AJ31")
					(alternate "GPIO3_PDD.05" passive line)
					(alternate "pe1_rst_l" passive line)
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "ULPI_CLK")
					(number "AK17")
					(alternate "GPIO3_PY.00" passive line)
					(alternate "SPI1A_DOUT" passive line)
				)
				(pin passive line
					(at 45.72 -119.38 180)
					(length 5.08)
					(name "ULPI_DATA6")
					(number "AK18")
					(alternate "GPIO3_PG.05" passive line)
					(alternate "GPIO3_PO.07" passive line)
					(alternate "SPI4C_SCK" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "USB0_ID")
					(number "AK20")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "USB3_RX0P")
					(number "AK21")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PEX_USB3_RX1P")
					(number "AK23")
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "PEX_RX3N")
					(number "AK24")
				)
				(pin passive line
					(at 45.72 -66.04 180)
					(length 5.08)
					(name "PEX_RX4P")
					(number "AK26")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PEX_L0_CLKREQ_N")
					(number "AK29")
					(alternate "GPIO3_PDD.02" passive line)
					(alternate "pe0_clkreq_l" passive line)
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "ULPI_STP")
					(number "AL16")
					(alternate "GPIO3_PY.03" passive line)
					(alternate "OWR" passive line)
					(alternate "SPI1A_CS0" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 45.72 -121.92 180)
					(length 5.08)
					(name "ULPI_DATA7")
					(number "AL17")
					(alternate "GPIO3_PH.02" passive line)
					(alternate "GPIO3_PO.00" passive line)
					(alternate "PM3_PWM2" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "ULPI_DIR")
					(number "AL18")
					(alternate "GPIO3_PG.03" passive line)
					(alternate "GPIO3_PY.01" passive line)
					(alternate "SPI1A_DIN" passive line)
					(alternate "tracedata1" passive line)
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "USB_REXT")
					(number "AL19")
					(alternate "GPIO3_PEE.04" passive line)
					(alternate "SDMMC3_CLK_LB_OUT" passive line)
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(name "USB0_VBUS")
					(number "AL20")
					(alternate "GPIO3_PAA.02" passive line)
					(alternate "SDMMC4_DAT2" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "USB3_RX0N")
					(number "AL21")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PEX_TERMP")
					(number "AL22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PEX_USB3_RX1N")
					(number "AL23")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "PEX_RX3P")
					(number "AL24")
				)
				(pin passive line
					(at 45.72 -68.58 180)
					(length 5.08)
					(name "PEX_RX4N")
					(number "AL26")
					(alternate "GPIO3_PAA.01" passive line)
					(alternate "SDMMC4_DAT1" passive line)
				)
			)
			(symbol "CD575M-A1_4_1"
				(text "DSI_CSI"
					(at 22.86 -35.56 900)
				)
				(text "LVDS/eDP"
					(at 22.86 -86.36 900)
				)
				(text "HDMI"
					(at 22.86 -109.22 900)
				)
				(text "CAM"
					(at 22.86 -132.08 900)
				)
				(text "Audio"
					(at 22.86 -162.56 900)
				)
				(pin passive line
					(at 45.72 -116.84 180)
					(length 5.08)
					(name "HDMI_TXD2P")
					(number "AD1")
				)
				(pin passive line
					(at 45.72 -119.38 180)
					(length 5.08)
					(name "HDMI_TXD2N")
					(number "AD2")
				)
				(pin passive line
					(at 45.72 -109.22 180)
					(length 5.08)
					(name "HDMI_TXD1P")
					(number "AD3")
				)
				(pin passive line
					(at 45.72 -111.76 180)
					(length 5.08)
					(name "HDMI_TXD1N")
					(number "AD4")
				)
				(pin passive line
					(at 45.72 -104.14 180)
					(length 5.08)
					(name "HDMI_TXD0N")
					(number "AD5")
				)
				(pin passive line
					(at 45.72 -101.6 180)
					(length 5.08)
					(name "HDMI_TXD0P")
					(number "AD6")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "CSI_A_D1_P")
					(number "AD9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "CSI_A_CLK_P")
					(number "AD11")
				)
				(pin passive line
					(at 45.72 -55.88 180)
					(length 5.08)
					(name "DSI_B_D1_P")
					(number "AD12")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "DSI_A_D1_N")
					(number "AD14")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "HDMI_PROBE")
					(number "AE1")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "CSI_A_D1_N")
					(number "AE9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "CSI_A_CLK_N")
					(number "AE11")
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "DSI_B_D1_N")
					(number "AE12")
				)
				(pin passive line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "DSI_A_D1_P")
					(number "AE14")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "HDMI_RSET")
					(number "AF2")
				)
				(pin passive line
					(at 45.72 -96.52 180)
					(length 5.08)
					(name "LVDS0_TXD4N")
					(number "AF3")
				)
				(pin passive line
					(at 45.72 -93.98 180)
					(length 5.08)
					(name "LVDS0_TXD4P")
					(number "AF4")
					(alternate "SDMMC3_COMP_PU" passive line)
					(alternate "sdio3comp" passive line)
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "HDMI_TXCN")
					(number "AF5")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 5.08)
					(name "HDMI_TXCP")
					(number "AF6")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 5.08)
					(name "CAM_I2C_SCL")
					(number "AF8")
					(alternate "GPIO3_PBB.01" passive line)
					(alternate "GPIO3_PK.06" passive line)
					(alternate "I2C3_CLK" passive line)
					(alternate "SPDIF_IN" passive line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "CSI_E_D0_N")
					(number "AF9")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "CSI_DSI_RUP")
					(number "AF11")
				)
				(pin passive line
					(at 45.72 -73.66 180)
					(length 5.08)
					(name "DSI_B_D3_N")
					(number "AF12")
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "DSI_A_D3_P")
					(number "AF14")
				)
				(pin passive line
					(at 45.72 -88.9 180)
					(length 5.08)
					(name "LVDS0_TXD3N")
					(number "AG1")
				)
				(pin passive line
					(at 45.72 -86.36 180)
					(length 5.08)
					(name "LVDS0_TXD3P")
					(number "AG2")
					(alternate "GPIO3_PAA.04" passive line)
					(alternate "SDMMC4_DAT4" passive line)
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "LVDS0_TXD1N")
					(number "AG3")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "LVDS0_TXD1P")
					(number "AG4")
				)
				(pin passive line
					(at 45.72 -81.28 180)
					(length 5.08)
					(name "LVDS0_TXD2N")
					(number "AG5")
				)
				(pin passive line
					(at 45.72 -78.74 180)
					(length 5.08)
					(name "LVDS0_TXD2P")
					(number "AG6")
				)
				(pin passive line
					(at 0 -142.24 0)
					(length 5.08)
					(name "CAM_I2C_SDA")
					(number "AG8")
					(alternate "GPIO3_PBB.02" passive line)
					(alternate "I2C3_DAT" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "CSI_E_D0_P")
					(number "AG9")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "CSI_DSI_RDN")
					(number "AG11")
				)
				(pin passive line
					(at 45.72 -71.12 180)
					(length 5.08)
					(name "DSI_B_D3_P")
					(number "AG12")
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "DSI_A_D3_N")
					(number "AG14")
				)
				(pin passive line
					(at 45.72 -132.08 180)
					(length 5.08)
					(name "GPIO_PBB5")
					(number "AH5")
					(alternate "GPIO3_PBB.05" passive line)
					(alternate "VGP5" passive line)
				)
				(pin passive line
					(at 45.72 -129.54 180)
					(length 5.08)
					(name "GPIO_PBB4")
					(number "AH6")
					(alternate "GPIO3_PBB.04" passive line)
					(alternate "VGP4" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "CSI_E_CLK_P")
					(number "AH8")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "CSI_B_D1_P")
					(number "AH9")
				)
				(pin passive line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "DSI_B_CLK_P")
					(number "AH11")
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "DSI_B_D0_N")
					(number "AH12")
				)
				(pin passive line
					(at 45.72 0 180)
					(length 5.08)
					(name "DSI_A_CLK_P")
					(number "AH14")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "LVDS0_TXD0N")
					(number "AJ2")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "LVDS0_TXD0P")
					(number "AJ3")
				)
				(pin passive line
					(at 45.72 -137.16 180)
					(length 5.08)
					(name "GPIO_PBB7")
					(number "AJ5")
					(alternate "GPIO3_PBB.07" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 45.72 -139.7 180)
					(length 5.08)
					(name "GPIO_PCC1")
					(number "AJ6")
					(alternate "GPIO3_PCC.01" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "CSI_E_CLK_N")
					(number "AJ8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "CSI_B_D1_N")
					(number "AJ9")
				)
				(pin passive line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "DSI_B_CLK_N")
					(number "AJ11")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "DSI_B_D0_P")
					(number "AJ12")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "DSI_A_CLK_N")
					(number "AJ14")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "LVDS0_RSET")
					(number "AK3")
				)
				(pin passive line
					(at 45.72 -124.46 180)
					(length 5.08)
					(name "GPIO_PBB0")
					(number "AK5")
					(alternate "GPIO3_PBB.00" passive line)
					(alternate "vimclk2_alt3" passive line)
				)
				(pin passive line
					(at 45.72 -127 180)
					(length 5.08)
					(name "GPIO_PBB3")
					(number "AK6")
					(alternate "GPIO3_PBB.03" passive line)
					(alternate "VGP3" passive line)
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "CSI_B_D0_N")
					(number "AK8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "CSI_A_D0_N")
					(number "AK9")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "DSI_A_D0_N")
					(number "AK11")
				)
				(pin passive line
					(at 45.72 -63.5 180)
					(length 5.08)
					(name "DSI_B_D2_P")
					(number "AK12")
				)
				(pin passive line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "DSI_A_D2_P")
					(number "AK15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "LVDS0_PROBE")
					(number "AL3")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "CAM_MCLK")
					(number "AL5")
					(alternate "GPIO3_PCC.00" passive line)
					(alternate "vimclk_alt3" passive line)
				)
				(pin passive line
					(at 45.72 -134.62 180)
					(length 5.08)
					(name "GPIO_PBB6")
					(number "AL6")
					(alternate "GPIO3_PBB.06" passive line)
					(alternate "wake45" passive line)
				)
				(pin passive line
					(at 45.72 -142.24 180)
					(length 5.08)
					(name "GPIO_PCC2")
					(number "AL7")
					(alternate "GPIO3_PCC.02" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "CSI_B_D0_P")
					(number "AL8")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "CSI_A_D0_P")
					(number "AL9")
				)
				(pin passive line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "DSI_A_D0_P")
					(number "AL11")
				)
				(pin passive line
					(at 45.72 -66.04 180)
					(length 5.08)
					(name "DSI_B_D2_N")
					(number "AL12")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "DSI_A_D2_N")
					(number "AL15")
				)
				(pin passive line
					(at 0 -172.72 0)
					(length 5.08)
					(name "DAP1_DIN")
					(number "H28")
					(alternate "GPIO3_PN.01" passive line)
					(alternate "I2S0_SDATA_IN" passive line)
				)
				(pin passive line
					(at 0 -177.8 0)
					(length 5.08)
					(name "DAP1_FS")
					(number "J28")
					(alternate "GPIO3_PN.00" passive line)
					(alternate "I2S0_LRCK" passive line)
				)
				(pin passive line
					(at 45.72 -175.26 180)
					(length 5.08)
					(name "DAP2_DOUT")
					(number "J29")
					(alternate "GPIO3_PA.05" passive line)
					(alternate "I2S1_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 45.72 -165.1 180)
					(length 5.08)
					(name "GPIO_W3_AUD")
					(number "J30")
					(alternate "GPIO3_PW.03" passive line)
					(alternate "wake11" passive line)
				)
				(pin passive line
					(at 0 -175.26 0)
					(length 5.08)
					(name "DAP1_DOUT")
					(number "L28")
					(alternate "GPIO3_PN.02" passive line)
					(alternate "I2S0_SDATA_OUT" passive line)
				)
				(pin passive line
					(at 0 -162.56 0)
					(length 5.08)
					(name "DAP_MCLK1")
					(number "L29")
					(alternate "GPIO3_PW.04" passive line)
					(alternate "extperiph1_clk" passive line)
				)
				(pin passive line
					(at 45.72 -172.72 180)
					(length 5.08)
					(name "DAP2_DIN")
					(number "L30")
					(alternate "GPIO3_PA.04" passive line)
					(alternate "I2S1_SDATA_IN" passive line)
				)
				(pin passive line
					(at 45.72 -162.56 180)
					(length 5.08)
					(name "GPIO_W2_AUD")
					(number "M28")
					(alternate "GPIO3_PW.02" passive line)
					(alternate "wake12" passive line)
				)
				(pin passive line
					(at 45.72 -180.34 180)
					(length 5.08)
					(name "DAP2_SCLK")
					(number "M29")
					(alternate "GPIO3_PA.03" passive line)
					(alternate "I2S1_SCLK" passive line)
				)
				(pin passive line
					(at 45.72 -149.86 180)
					(length 5.08)
					(name "GPIO_X3_AUD")
					(number "M30")
					(alternate "GPIO3_PX.03" passive line)
				)
				(pin passive line
					(at 0 -165.1 0)
					(length 5.08)
					(name "DAP_MCLK1_REQ")
					(number "M31")
					(alternate "GPIO3_PEE.02" passive line)
					(alternate "SATA_DEV_SLP" passive line)
				)
				(pin passive line
					(at 45.72 -157.48 180)
					(length 5.08)
					(name "GPIO_X6_AUD")
					(number "N31")
					(alternate "GPIO3_PX.06" passive line)
				)
				(pin passive line
					(at 45.72 -160.02 180)
					(length 5.08)
					(name "GPIO_X7_AUD")
					(number "P28")
					(alternate "GPIO3_PX.07" passive line)
				)
				(pin passive line
					(at 45.72 -147.32 180)
					(length 5.08)
					(name "GPIO_X1_AUD")
					(number "P29")
					(alternate "GPIO3_PX.01" passive line)
				)
				(pin passive line
					(at 0 -149.86 0)
					(length 5.08)
					(name "DVFS_PWM")
					(number "P30")
					(alternate "CLDVFS_PWM" passive line)
					(alternate "GPIO3_PX.00" passive line)
				)
				(pin passive line
					(at 0 -180.34 0)
					(length 5.08)
					(name "DAP1_SCLK")
					(number "P31")
					(alternate "GPIO3_PN.03" passive line)
					(alternate "I2S0_SCLK" passive line)
				)
				(pin passive line
					(at 45.72 -152.4 180)
					(length 5.08)
					(name "GPIO_X4_AUD")
					(number "R28")
					(alternate "GPIO3_PX.04" passive line)
				)
				(pin passive line
					(at 0 -147.32 0)
					(length 5.08)
					(name "DVFS_CLK")
					(number "R29")
					(alternate "CLDVFS_CLK" passive line)
					(alternate "GPIO3_PX.02" passive line)
				)
				(pin passive line
					(at 45.72 -177.8 180)
					(length 5.08)
					(name "DAP2_FS")
					(number "R30")
					(alternate "GPIO3_PA.02" passive line)
					(alternate "I2S1_LRCK" passive line)
				)
				(pin passive line
					(at 45.72 -154.94 180)
					(length 5.08)
					(name "GPIO_X5_AUD")
					(number "R31")
					(alternate "GPIO3_PX.05" passive line)
				)
			)
			(symbol "CD575M-A1_5_1"
				(text "SDMMC1\n"
					(at 22.86 -17.78 900)
				)
				(text "SATA"
					(at 22.86 -58.42 900)
				)
				(text "GMI (Sync-NOR)"
					(at 27.94 -106.68 900)
				)
				(text "SDMMC3\n"
					(at 30.48 -17.78 900)
				)
				(text "SDMMC4\n"
					(at 30.48 -55.88 900)
				)
				(pin passive line
					(at 53.34 -124.46 180)
					(length 5.08)
					(name "GPIO_PK0")
					(number "AA1")
					(alternate "GPIO3_PK.00" passive line)
					(alternate "soc_therm_oc3_n" passive line)
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "GEN2_I2C_SDA")
					(number "AA2")
					(alternate "GPIO3_PQ.07" passive line)
					(alternate "GPIO3_PT.06" passive line)
					(alternate "I2C2_DAT" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 5.08)
					(name "GPIO_PG5")
					(number "AA3")
					(alternate "GPIO3_PG.05" passive line)
					(alternate "SPI4C_SCK" passive line)
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 5.08)
					(name "GPIO_PH2")
					(number "AA4")
					(alternate "GPIO3_PH.02" passive line)
					(alternate "GPIO3_PS.02" passive line)
					(alternate "PM3_PWM2" passive line)
					(alternate "UA3_RXD" passive line)
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "GPIO_PG3")
					(number "AA5")
					(alternate "GPIO3_PG.03" passive line)
					(alternate "tracedata1" passive line)
				)
				(pin passive line
					(at 53.34 -93.98 180)
					(length 5.08)
					(name "GPIO_PI1")
					(number "AA6")
					(alternate "GPIO3_PI.01" passive line)
					(alternate "I2C6_DAT" passive line)
					(alternate "force_recovery" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "SATA_TESTCLKN")
					(number "AF27")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "SATA_TESTCLKP")
					(number "AG27")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "SATA_L0_RXN")
					(number "AH27")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "SATA_L0_RXP")
					(number "AJ27")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "SATA_L0_TXN")
					(number "AK27")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "SATA_TERMP")
					(number "AL25")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "SATA_L0_TXP")
					(number "AL27")
				)
				(pin passive line
					(at 53.34 -66.04 180)
					(length 5.08)
					(name "SDMMC4_DAT4")
					(number "D31")
					(alternate "GPIO3_PAA.04" passive line)
					(alternate "SDMMC4_DAT4" passive line)
				)
				(pin passive line
					(at 53.34 -30.48 180)
					(length 5.08)
					(name "SDMMC3_COMP_PU")
					(number "E2")
					(alternate "GPIO3_PQ.00" passive line)
					(alternate "SDMMC3_COMP_PU" passive line)
					(alternate "sdio3comp" passive line)
					(alternate "wake51" passive line)
				)
				(pin passive line
					(at 53.34 -27.94 180)
					(length 5.08)
					(name "SDMMC3_COMP_PD")
					(number "E5")
					(alternate "GPIO3_PQ.06" passive line)
					(alternate "SDMMC3_COMP_PD" passive line)
					(alternate "pu" passive line)
					(alternate "sdio3comp" passive line)
				)
				(pin passive line
					(at 53.34 -60.96 180)
					(length 5.08)
					(name "SDMMC4_DAT2")
					(number "E28")
					(alternate "GPIO3_PAA.02" passive line)
					(alternate "SDMMC4_DAT2" passive line)
				)
				(pin passive line
					(at 53.34 -71.12 180)
					(length 5.08)
					(name "SDMMC4_DAT6")
					(number "E29")
					(alternate "GPIO3_PAA.06" passive line)
					(alternate "SDMMC4_DAT6" passive line)
				)
				(pin passive line
					(at 53.34 -68.58 180)
					(length 5.08)
					(name "SDMMC4_DAT5")
					(number "E30")
					(alternate "GPIO3_PAA.05" passive line)
					(alternate "SDMMC4_DAT5" passive line)
				)
				(pin passive line
					(at 53.34 -50.8 180)
					(length 5.08)
					(name "SDMMC4_CMD")
					(number "E31")
					(alternate "GPIO3_PT.07" passive line)
					(alternate "SDMMC4_CMD" passive line)
				)
				(pin passive line
					(at 53.34 -20.32 180)
					(length 5.08)
					(name "SDMMC3_DAT2")
					(number "F1")
					(alternate "GPIO3_PB.05" passive line)
					(alternate "SDMMC3_DAT2" passive line)
				)
				(pin passive line
					(at 53.34 -10.16 180)
					(length 5.08)
					(name "SDMMC3_CMD")
					(number "F2")
					(alternate "GPIO3_PA.07" passive line)
					(alternate "SDMMC3_CMD" passive line)
				)
				(pin passive line
					(at 53.34 -2.54 180)
					(length 5.08)
					(name "SDMMC3_CLK_LB_IN")
					(number "F3")
					(alternate "GPIO3_PEE.05" passive line)
					(alternate "GPIO3_PQ.02" passive line)
					(alternate "SDMMC3_CLK_LB_IN" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 53.34 0 180)
					(length 5.08)
					(name "SDMMC3_CLK_LB_OUT")
					(number "F4")
					(alternate "GPIO3_PEE.04" passive line)
					(alternate "SDMMC3_CLK_LB_OUT" passive line)
				)
				(pin passive line
					(at 53.34 -7.62 180)
					(length 5.08)
					(name "SDMMC3_CLK")
					(number "F5")
					(alternate "GPIO3_PA.06" passive line)
					(alternate "SDMMC3_CLK" passive line)
				)
				(pin passive line
					(at 53.34 -73.66 180)
					(length 5.08)
					(name "SDMMC4_DAT7")
					(number "F28")
					(alternate "GPIO3_PAA.07" passive line)
					(alternate "SDMMC4_DAT7" passive line)
				)
				(pin passive line
					(at 53.34 -55.88 180)
					(length 5.08)
					(name "SDMMC4_DAT0")
					(number "F29")
					(alternate "GPIO3_PAA.00" passive line)
					(alternate "SDMMC4_DAT0" passive line)
				)
				(pin passive line
					(at 53.34 -58.42 180)
					(length 5.08)
					(name "SDMMC4_DAT1")
					(number "F30")
					(alternate "GPIO3_PAA.01" passive line)
					(alternate "SDMMC4_DAT1" passive line)
				)
				(pin passive line
					(at 53.34 -22.86 180)
					(length 5.08)
					(name "SDMMC3_DAT3")
					(number "G1")
					(alternate "GPIO3_PB.04" passive line)
					(alternate "SDMMC3_DAT3" passive line)
				)
				(pin passive line
					(at 53.34 -48.26 180)
					(length 5.08)
					(name "SDMMC4_CLK")
					(number "G31")
					(alternate "GPIO3_PCC.04" passive line)
					(alternate "GPIO3_PQ.03" passive line)
					(alternate "SDMMC4_CLK" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 53.34 -17.78 180)
					(length 5.08)
					(name "SDMMC3_DAT1")
					(number "H1")
					(alternate "GPIO3_PB.06" passive line)
					(alternate "GPIO3_PO.03" passive line)
					(alternate "SDMMC3_DAT1" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 53.34 -15.24 180)
					(length 5.08)
					(name "SDMMC3_DAT0")
					(number "H2")
					(alternate "GPIO3_PB.07" passive line)
					(alternate "GPIO3_PV.01" passive line)
					(alternate "SDMMC3_DAT0" passive line)
					(alternate "wake1" passive line)
				)
				(pin passive line
					(at 53.34 -40.64 180)
					(length 5.08)
					(name "SDMMC4_COMP_PD")
					(number "H29")
					(alternate "SDMMC4_COMP_PD" passive line)
				)
				(pin passive line
					(at 53.34 -43.18 180)
					(length 5.08)
					(name "SDMMC4_COMP_PU")
					(number "H30")
					(alternate "SDMMC4_COMP_PU" passive line)
				)
				(pin passive line
					(at 53.34 -63.5 180)
					(length 5.08)
					(name "SDMMC4_DAT3")
					(number "H31")
					(alternate "GPIO3_PAA.03" passive line)
					(alternate "SDMMC4_DAT3" passive line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SDMMC1_COMP_PU")
					(number "J7")
					(alternate "SDMMC1_COMP_PU" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "SDMMC1_DAT3")
					(number "J8")
					(alternate "GPIO3_PY.04" passive line)
					(alternate "SDMMC1_DAT3" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "CLK2_OUT")
					(number "K1")
					(alternate "GPIO3_PR.03" passive line)
					(alternate "GPIO3_PW.05" passive line)
					(alternate "SYS_CLK_REQ" passive line)
					(alternate "extperiph2_clk" passive line)
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "SDMMC1_DAT2")
					(number "L1")
					(alternate "CEC" passive line)
					(alternate "GPIO3_PEE.03" passive line)
					(alternate "GPIO3_PY.05" passive line)
					(alternate "SDMMC1_DAT2" passive line)
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SDMMC1_DAT0")
					(number "L2")
					(alternate "GPIO3_PY.07" passive line)
					(alternate "SDMMC1_DAT0" passive line)
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SDMMC1_DAT1")
					(number "L3")
					(alternate "GPIO3_PY.06" passive line)
					(alternate "SDMMC1_DAT1" passive line)
					(alternate "wake13" passive line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "CLK2_REQ")
					(number "L4")
					(alternate "GPIO3_PCC.05" passive line)
					(alternate "z" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SDMMC1_WP_N")
					(number "L5")
					(alternate "GPIO3_PV.03" passive line)
					(alternate "SDMMC1_WP_N" passive line)
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SDMMC1_COMP_PD")
					(number "L6")
					(alternate "SDMMC1_COMP_PD" passive line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SDMMC1_CLK")
					(number "L7")
					(alternate "GPIO3_PZ.00" passive line)
					(alternate "SDMMC1_CLK" passive line)
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SDMMC1_CMD")
					(number "L8")
					(alternate "GPIO3_PZ.01" passive line)
					(alternate "SDMMC1_CMD" passive line)
				)
				(pin passive line
					(at 53.34 -106.68 180)
					(length 5.08)
					(name "GPIO_PI6")
					(number "R1")
					(alternate "DP_HPD" passive line)
					(alternate "GPIO3_PFF.00" passive line)
					(alternate "GPIO3_PI.06" passive line)
					(alternate "SDMMC2A_DAT7" passive line)
				)
				(pin passive line
					(at 53.34 -132.08 180)
					(length 5.08)
					(name "GPIO_PK3")
					(number "R2")
					(alternate "GPIO3_PK.03" passive line)
					(alternate "SDMMC2A_DAT4" passive line)
				)
				(pin passive line
					(at 53.34 -127 180)
					(length 5.08)
					(name "GPIO_PK1")
					(number "R3")
					(alternate "GPIO3_PK.01" passive line)
					(alternate "SDMMC2A_CLK" passive line)
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 5.08)
					(name "GPIO_PH5")
					(number "R4")
					(alternate "GPIO3_PH.05" passive line)
					(alternate "SDMMC2A_DAT2" passive line)
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "GPIO_PH4")
					(number "R5")
					(alternate "GPIO3_PH.04" passive line)
					(alternate "SDMMC2A_DAT0" passive line)
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 5.08)
					(name "SDMMC2_COMP_PD")
					(number "R6")
					(alternate "SDMMC2_COMP_PD" passive line)
					(alternate "sdio2comp" passive line)
				)
				(pin passive line
					(at 53.34 -134.62 180)
					(length 5.08)
					(name "GPIO_PK4")
					(number "T1")
					(alternate "GPIO3_PK.04" passive line)
					(alternate "SDMMC2A_DAT5" passive line)
				)
				(pin passive line
					(at 53.34 -86.36 180)
					(length 5.08)
					(name "GPIO_PC7")
					(number "U1")
					(alternate "GPIO3_PC.07" passive line)
					(alternate "GPIO3_PV.05" passive line)
					(alternate "I2C4_DAT" passive line)
					(alternate "wake8" passive line)
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(name "GPIO_PH7")
					(number "U2")
					(alternate "GPIO3_PH.07" passive line)
					(alternate "SDMMC2A_CMD" passive line)
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "GPIO_PH1")
					(number "U3")
					(alternate "GPIO3_PH.01" passive line)
					(alternate "PM3_PWM1" passive line)
				)
				(pin passive line
					(at 53.34 -78.74 180)
					(length 5.08)
					(name "GPIO_PB0")
					(number "U4")
					(alternate "GPIO3_PB.00" passive line)
					(alternate "GPIO3_PQ.05" passive line)
					(alternate "UD3_RXD" passive line)
					(alternate "wake54" passive line)
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "SDMMC2_COMP_PU")
					(number "U5")
					(alternate "SDMMC2_COMP_PU" passive line)
					(alternate "sdio2comp" passive line)
				)
				(pin passive line
					(at 53.34 -114.3 180)
					(length 5.08)
					(name "GPIO_PJ0")
					(number "U6")
					(alternate "GPIO3_PJ.00" passive line)
					(alternate "wake33" passive line)
				)
				(pin passive line
					(at 53.34 -104.14 180)
					(length 5.08)
					(name "GPIO_PI5")
					(number "U7")
					(alternate "GPIO3_PI.05" passive line)
					(alternate "GPIO3_PK.05" passive line)
					(alternate "SDMMC2A_DAT1" passive line)
					(alternate "SPDIF_OUT" passive line)
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "GPIO_PH6")
					(number "U8")
					(alternate "GPIO3_PH.06" passive line)
					(alternate "SDMMC2A_DAT3" passive line)
				)
				(pin passive line
					(at 53.34 -96.52 180)
					(length 5.08)
					(name "GPIO_PI2")
					(number "V1")
					(alternate "GPIO3_PI.02" passive line)
					(alternate "GPIO3_PN.07" passive line)
					(alternate "SDMMC2A_DAT6" passive line)
					(alternate "wake4" passive line)
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "GPIO_PG0")
					(number "V2")
					(alternate "GPIO3_PG.00" passive line)
					(alternate "SYS_RESET_N" passive line)
					(alternate "boot_select0" passive line)
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "GPIO_PG7")
					(number "V3")
					(alternate "GPIO3_PG.07" passive line)
					(alternate "SPI4C_DIN" passive line)
				)
				(pin passive line
					(at 53.34 -116.84 180)
					(length 5.08)
					(name "GPIO_PJ7")
					(number "V4")
					(alternate "GPIO3_PJ.07" passive line)
					(alternate "GPIO3_PT.00" passive line)
					(alternate "UD3_TXD" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 53.34 -137.16 180)
					(length 5.08)
					(name "GPIO_PK7")
					(number "V5")
					(alternate "GPIO3_PK.07" passive line)
					(alternate "GPIO3_PS.00" passive line)
					(alternate "UD3_RTS" passive line)
					(alternate "wake27" passive line)
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "GPIO_PG1")
					(number "V6")
					(alternate "GPIO3_PG.01" passive line)
					(alternate "boot_select1" passive line)
				)
				(pin passive line
					(at 53.34 -99.06 180)
					(length 5.08)
					(name "GPIO_PI3")
					(number "V7")
					(alternate "GPIO3_PI.03" passive line)
					(alternate "GPIO3_PN.05" passive line)
					(alternate "SPI4C_CS0" passive line)
					(alternate "usb_vbus_en1" passive line)
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "GPIO_PH3")
					(number "V8")
					(alternate "GPIO3_PH.03" passive line)
					(alternate "GPIO3_PN.04" passive line)
					(alternate "PM3_PWM3" passive line)
					(alternate "usb_vbus_en0" passive line)
				)
				(pin passive line
					(at 53.34 -81.28 180)
					(length 5.08)
					(name "GPIO_PB1")
					(number "V9")
					(alternate "GPIO3_PB.01" passive line)
					(alternate "GPIO3_PS.01" passive line)
					(alternate "UA3_TXD" passive line)
					(alternate "UD3_CTS" passive line)
				)
				(pin passive line
					(at 53.34 -119.38 180)
					(length 5.08)
					(name "GPIO_PJ2")
					(number "W1")
					(alternate "GPIO3_PJ.02" passive line)
					(alternate "soc_therm_oc4_n" passive line)
				)
				(pin passive line
					(at 53.34 -129.54 180)
					(length 5.08)
					(name "GPIO_PK2")
					(number "Y1")
					(alternate "DCA_LSPII" passive line)
					(alternate "GPIO3_PK.02" passive line)
					(alternate "GPIO3_PR.06" passive line)
					(alternate "wake34" passive line)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "GEN2_I2C_SCL")
					(number "Y2")
					(alternate "GPIO3_PT.05" passive line)
					(alternate "I2C2_CLK" passive line)
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "GPIO_PG4")
					(number "Y3")
					(alternate "GPIO3_PG.04" passive line)
					(alternate "SPI4C_CS3" passive line)
				)
				(pin passive line
					(at 53.34 -109.22 180)
					(length 5.08)
					(name "GPIO_PI7")
					(number "Y4")
					(alternate "GPIO3_PI.07" passive line)
					(alternate "GPIO3_PV.04" passive line)
					(alternate "I2C4_CLK" passive line)
					(alternate "tracedata7" passive line)
				)
				(pin passive line
					(at 53.34 -91.44 180)
					(length 5.08)
					(name "GPIO_PI0")
					(number "Y5")
					(alternate "GPIO3_PI.00" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "GPIO_PH0")
					(number "Y6")
					(alternate "GPIO3_PH.00" passive line)
					(alternate "PM3_PWM0" passive line)
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 5.08)
					(name "GPIO_PG2")
					(number "Y7")
					(alternate "GPIO3_PG.02" passive line)
					(alternate "tracedata0" passive line)
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "GPIO_PG6")
					(number "Y8")
					(alternate "GPIO3_PG.06" passive line)
					(alternate "SPI4C_DOUT" passive line)
				)
				(pin passive line
					(at 53.34 -101.6 180)
					(length 5.08)
					(name "GPIO_PI4")
					(number "Y9")
					(alternate "GPIO3_PI.04" passive line)
					(alternate "I2C6_CLK" passive line)
					(alternate "SPI4C_CS1" passive line)
					(alternate "z" passive line)
				)
			)
			(symbol "CD575M-A1_6_1"
				(text "DDR"
					(at 22.86 -99.06 900)
				)
				(pin passive line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "DDR_DQ0")
					(number "A3")
				)
				(pin passive line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "DDR_DQ1")
					(number "A4")
					(alternate "GPIO3_PDD.01" passive line)
					(alternate "pe0_rst_l" passive line)
				)
				(pin passive line
					(at 43.18 -63.5 180)
					(length 5.08)
					(name "DDR_DQ7")
					(number "A5")
				)
				(pin passive line
					(at 43.18 -99.06 180)
					(length 5.08)
					(name "DDR_DQ21")
					(number "A6")
				)
				(pin passive line
					(at 43.18 -96.52 180)
					(length 5.08)
					(name "DDR_DQ20")
					(number "A7")
				)
				(pin passive line
					(at 43.18 -86.36 180)
					(length 5.08)
					(name "DDR_DQ16")
					(number "A8")
				)
				(pin passive line
					(at 43.18 -78.74 180)
					(length 5.08)
					(name "DDR_DQ13")
					(number "A9")
				)
				(pin passive line
					(at 43.18 -116.84 180)
					(length 5.08)
					(name "DDR_DQ28")
					(number "A10")
				)
				(pin passive line
					(at 43.18 -111.76 180)
					(length 5.08)
					(name "DDR_DQ26")
					(number "A11")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 5.08)
					(name "DDR_CS1_N")
					(number "A12")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "DDR_CKE0")
					(number "A13")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DDR_CKE1")
					(number "A14")
				)
				(pin passive line
					(at 0 -198.12 0)
					(length 5.08)
					(name "DDR_ODT0")
					(number "A15")
				)
				(pin passive line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "DDR_A12")
					(number "A16")
				)
				(pin passive line
					(at 0 -205.74 0)
					(length 5.08)
					(name "DDR_ODT_B1")
					(number "A18")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 5.08)
					(name "DDR_CS_B1_N")
					(number "A19")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DDR_CKE_B0")
					(number "A20")
				)
				(pin passive line
					(at 43.18 -129.54 180)
					(length 5.08)
					(name "DDR_DQ33")
					(number "A21")
				)
				(pin passive line
					(at 43.18 -167.64 180)
					(length 5.08)
					(name "DDR_DQ48")
					(number "A22")
				)
				(pin passive line
					(at 43.18 -172.72 180)
					(length 5.08)
					(name "DDR_DQ50")
					(number "A23")
				)
				(pin passive line
					(at 43.18 -154.94 180)
					(length 5.08)
					(name "DDR_DQ43")
					(number "A24")
				)
				(pin passive line
					(at 43.18 -162.56 180)
					(length 5.08)
					(name "DDR_DQ46")
					(number "A25")
				)
				(pin passive line
					(at 43.18 -165.1 180)
					(length 5.08)
					(name "DDR_DQ47")
					(number "A26")
				)
				(pin passive line
					(at 43.18 -200.66 180)
					(length 5.08)
					(name "DDR_DQ61")
					(number "A27")
				)
				(pin passive line
					(at 43.18 -205.74 180)
					(length 5.08)
					(name "DDR_DQ63")
					(number "A28")
				)
				(pin passive line
					(at 43.18 -195.58 180)
					(length 5.08)
					(name "DDR_DQ59")
					(number "A29")
				)
				(pin passive line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "DDR_DQ5")
					(number "B2")
				)
				(pin passive line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "DDR_DQ4")
					(number "B3")
				)
				(pin passive line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "DDR_DQ2")
					(number "B5")
					(alternate "GPIO3_PDD.06" passive line)
					(alternate "pe1_clkreq_l" passive line)
				)
				(pin passive line
					(at 0 -175.26 0)
					(length 5.08)
					(name "DDR_DM2")
					(number "B6")
				)
				(pin passive line
					(at 43.18 -88.9 180)
					(length 5.08)
					(name "DDR_DQ17")
					(number "B8")
				)
				(pin passive line
					(at 0 -172.72 0)
					(length 5.08)
					(name "DDR_DM1")
					(number "B9")
					(alternate "GPIO3_PBB.00" passive line)
					(alternate "vimclk2_alt3" passive line)
				)
				(pin passive line
					(at 43.18 -119.38 180)
					(length 5.08)
					(name "DDR_DQ29")
					(number "B11")
					(alternate "GPIO3_PCC.00" passive line)
					(alternate "vimclk_alt3" passive line)
				)
				(pin passive line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "DDR_A9")
					(number "B12")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 5.08)
					(name "DDR_CS0_N")
					(number "B14")
				)
				(pin passive line
					(at 0 -200.66 0)
					(length 5.08)
					(name "DDR_ODT1")
					(number "B15")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "DDR_CS_B0_N")
					(number "B18")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DDR_CKE_B1")
					(number "B20")
				)
				(pin passive line
					(at 43.18 -142.24 180)
					(length 5.08)
					(name "DDR_DQ38")
					(number "B21")
					(alternate "GPIO3_PY.01" passive line)
					(alternate "SPI1A_DIN" passive line)
				)
				(pin passive line
					(at 43.18 -177.8 180)
					(length 5.08)
					(name "DDR_DQ52")
					(number "B23")
				)
				(pin passive line
					(at 0 -182.88 0)
					(length 5.08)
					(name "DDR_DM5")
					(number "B24")
				)
				(pin passive line
					(at 43.18 -160.02 180)
					(length 5.08)
					(name "DDR_DQ45")
					(number "B26")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 5.08)
					(name "DDR_DM7")
					(number "B27")
				)
				(pin passive line
					(at 0 -160.02 0)
					(length 5.08)
					(name "DDR_DQS7N")
					(number "B29")
				)
				(pin passive line
					(at 0 -157.48 0)
					(length 5.08)
					(name "DDR_DQS7P")
					(number "B30")
				)
				(pin passive line
					(at 0 -170.18 0)
					(length 5.08)
					(name "DDR_DM0")
					(number "C1")
				)
				(pin passive line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "DDR_DQ3")
					(number "C2")
					(alternate "GPIO3_PDD.05" passive line)
					(alternate "pe1_rst_l" passive line)
				)
				(pin passive line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "DDR_DQ6")
					(number "C3")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "DDR_DQS0P")
					(number "C5")
				)
				(pin passive line
					(at 43.18 -91.44 180)
					(length 5.08)
					(name "DDR_DQ18")
					(number "C6")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 5.08)
					(name "DDR_DQS2P")
					(number "C8")
					(alternate "GPIO3_PO.07" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 43.18 -66.04 180)
					(length 5.08)
					(name "DDR_DQ8")
					(number "C9")
				)
				(pin passive line
					(at 0 -177.8 0)
					(length 5.08)
					(name "DDR_DM3")
					(number "C11")
				)
				(pin passive line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "DDR_A6")
					(number "C12")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "DDR_CAS_N")
					(number "C14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "DDR_WE_N")
					(number "C15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DDR_COMP_PU")
					(number "C17")
				)
				(pin passive line
					(at 0 -203.2 0)
					(length 5.08)
					(name "DDR_ODT_B0")
					(number "C18")
				)
				(pin passive line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "DDR_A13")
					(number "C20")
				)
				(pin passive line
					(at 43.18 -144.78 180)
					(length 5.08)
					(name "DDR_DQ39")
					(number "C21")
				)
				(pin passive line
					(at 43.18 -175.26 180)
					(length 5.08)
					(name "DDR_DQ51")
					(number "C23")
				)
				(pin passive line
					(at 43.18 -149.86 180)
					(length 5.08)
					(name "DDR_DQ41")
					(number "C24")
				)
				(pin passive line
					(at 0 -142.24 0)
					(length 5.08)
					(name "DDR_DQS5P")
					(number "C26")
				)
				(pin passive line
					(at 43.18 -193.04 180)
					(length 5.08)
					(name "DDR_DQ58")
					(number "C27")
				)
				(pin passive line
					(at 43.18 -190.5 180)
					(length 5.08)
					(name "DDR_DQ57")
					(number "C29")
				)
				(pin passive line
					(at 43.18 -203.2 180)
					(length 5.08)
					(name "DDR_DQ62")
					(number "C30")
				)
				(pin passive line
					(at 43.18 -198.12 180)
					(length 5.08)
					(name "DDR_DQ60")
					(number "C31")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 5.08)
					(name "DDR_DQS0N")
					(number "D5")
				)
				(pin passive line
					(at 43.18 -101.6 180)
					(length 5.08)
					(name "DDR_DQ22")
					(number "D6")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 5.08)
					(name "DDR_DQS2N")
					(number "D8")
					(alternate "GPIO3_PY.00" passive line)
					(alternate "SPI1A_DOUT" passive line)
				)
				(pin passive line
					(at 43.18 -81.28 180)
					(length 5.08)
					(name "DDR_DQ14")
					(number "D9")
				)
				(pin passive line
					(at 43.18 -124.46 180)
					(length 5.08)
					(name "DDR_DQ31")
					(number "D11")
					(alternate "GPIO3_PCC.02" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "DDR_A4")
					(number "D12")
				)
				(pin passive line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "DDR_A1")
					(number "D14")
				)
				(pin passive line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "DDR_A8")
					(number "D15")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DDR_COMP_PD")
					(number "D17")
				)
				(pin passive line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "DDR_A10")
					(number "D18")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "DDR_BA1")
					(number "D20")
					(alternate "GPIO3_PCC.01" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 43.18 -139.7 180)
					(length 5.08)
					(name "DDR_DQ37")
					(number "D21")
					(alternate "GPIO3_PO.00" passive line)
					(alternate "pu" passive line)
				)
				(pin passive line
					(at 0 -152.4 0)
					(length 5.08)
					(name "DDR_DQS6N")
					(number "D23")
				)
				(pin passive line
					(at 43.18 -147.32 180)
					(length 5.08)
					(name "DDR_DQ40")
					(number "D24")
				)
				(pin passive line
					(at 0 -144.78 0)
					(length 5.08)
					(name "DDR_DQS5N")
					(number "D26")
				)
				(pin passive line
					(at 43.18 -187.96 180)
					(length 5.08)
					(name "DDR_DQ56")
					(number "D27")
				)
				(pin passive line
					(at 43.18 -93.98 180)
					(length 5.08)
					(name "DDR_DQ19")
					(number "E6")
				)
				(pin passive line
					(at 43.18 -83.82 180)
					(length 5.08)
					(name "DDR_DQ15")
					(number "E8")
				)
				(pin passive line
					(at 43.18 -76.2 180)
					(length 5.08)
					(name "DDR_DQ12")
					(number "E9")
				)
				(pin passive line
					(at 43.18 -114.3 180)
					(length 5.08)
					(name "DDR_DQ27")
					(number "E11")
				)
				(pin passive line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "DDR_A3")
					(number "E12")
				)
				(pin passive line
					(at 43.18 0 180)
					(length 5.08)
					(name "DDR_A0")
					(number "E14")
				)
				(pin passive line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "DDR_A2")
					(number "E15")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "DDR_A14")
					(number "E17")
				)
				(pin passive line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "DDR_A15")
					(number "E18")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "DDR_A_B4")
					(number "E20")
				)
				(pin passive line
					(at 43.18 -132.08 180)
					(length 5.08)
					(name "DDR_DQ34")
					(number "E21")
				)
				(pin passive line
					(at 0 -149.86 0)
					(length 5.08)
					(name "DDR_DQS6P")
					(number "E23")
				)
				(pin passive line
					(at 43.18 -170.18 180)
					(length 5.08)
					(name "DDR_DQ49")
					(number "E24")
				)
				(pin passive line
					(at 43.18 -157.48 180)
					(length 5.08)
					(name "DDR_DQ44")
					(number "E26")
				)
				(pin passive line
					(at 43.18 -152.4 180)
					(length 5.08)
					(name "DDR_DQ42")
					(number "E27")
				)
				(pin passive line
					(at 43.18 -104.14 180)
					(length 5.08)
					(name "DDR_DQ23")
					(number "F6")
				)
				(pin passive line
					(at 43.18 -73.66 180)
					(length 5.08)
					(name "DDR_DQ11")
					(number "F8")
				)
				(pin passive line
					(at 43.18 -68.58 180)
					(length 5.08)
					(name "DDR_DQ9")
					(number "F9")
				)
				(pin passive line
					(at 43.18 -121.92 180)
					(length 5.08)
					(name "DDR_DQ30")
					(number "F11")
					(alternate "GPIO3_PBB.06" passive line)
					(alternate "wake45" passive line)
				)
				(pin passive line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "DDR_A5")
					(number "F12")
				)
				(pin passive line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "DDR_A7")
					(number "F14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "DDR_RESET_N")
					(number "F15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "DDR_A_B5")
					(number "F17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "DDR_BA0")
					(number "F18")
					(alternate "GPIO3_PBB.07" passive line)
					(alternate "pd" passive line)
				)
				(pin passive line
					(at 43.18 -134.62 180)
					(length 5.08)
					(name "DDR_DQ35")
					(number "F20")
				)
				(pin passive line
					(at 0 -180.34 0)
					(length 5.08)
					(name "DDR_DM4")
					(number "F21")
				)
				(pin passive line
					(at 0 -185.42 0)
					(length 5.08)
					(name "DDR_DM6")
					(number "F23")
				)
				(pin passive line
					(at 43.18 -182.88 180)
					(length 5.08)
					(name "DDR_DQ54")
					(number "F24")
				)
				(pin passive line
					(at 43.18 -71.12 180)
					(length 5.08)
					(name "DDR_DQ10")
					(number "G8")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "DDR_DQS1P")
					(number "G9")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 5.08)
					(name "DDR_DQS3N")
					(number "G11")
				)
				(pin passive line
					(at 43.18 -106.68 180)
					(length 5.08)
					(name "DDR_DQ24")
					(number "G12")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "DDR_CLK")
					(number "G14")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "DDR_RAS_N")
					(number "G15")
				)
				(pin passive line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "DDR_A11")
					(number "G17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "DDR_CLKB_N")
					(number "G18")
					(alternate "GPIO3_PO.05" passive line)
					(alternate "wake0" passive line)
				)
				(pin passive line
					(at 43.18 -137.16 180)
					(length 5.08)
					(name "DDR_DQ36")
					(number "G20")
					(alternate "GPIO3_PY.03" passive line)
					(alternate "SPI1A_CS0" passive line)
				)
				(pin passive line
					(at 43.18 -127 180)
					(length 5.08)
					(name "DDR_DQ32")
					(number "G21")
				)
				(pin passive line
					(at 43.18 -180.34 180)
					(length 5.08)
					(name "DDR_DQ53")
					(number "G23")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "DDR_DQS1N")
					(number "H9")
					(alternate "GPIO3_PBB.03" passive line)
					(alternate "VGP3" passive line)
				)
				(pin passive line
					(at 0 -127 0)
					(length 5.08)
					(name "DDR_DQS3P")
					(number "H11")
					(alternate "GPIO3_PDD.02" passive line)
					(alternate "pe0_clkreq_l" passive line)
				)
				(pin passive line
					(at 43.18 -109.22 180)
					(length 5.08)
					(name "DDR_DQ25")
					(number "H12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "DDR_CLK_N")
					(number "H14")
					(alternate "GPIO3_PO.04" passive line)
					(alternate "wake32" passive line)
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "DDR_BA2")
					(number "H15")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "DDR_A_B3")
					(number "H17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "DDR_CLKB")
					(number "H18")
					(alternate "GPIO3_PP.03" passive line)
					(alternate "I2S2_SCLK" passive line)
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 5.08)
					(name "DDR_DQS4N")
					(number "H20")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 5.08)
					(name "DDR_DQS4P")
					(number "H21")
				)
				(pin passive line
					(at 43.18 -185.42 180)
					(length 5.08)
					(name "DDR_DQ55")
					(number "H23")
				)
			)
			(embedded_fonts no)
		)
)
