(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CDCE906PWR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CDCE906PWR"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CDCE906PWR"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cdce906.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&ts=1672406494449&ref_url=https%253A%252F%252Feu.mouser.com%252F"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Clock generator/frequency synthesizer (PLL)"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CDCE906PWR"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PLL, IC, CLOCK, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CDCE906PWR_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "S0/A0/CLK_SEL")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "S1/A1")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin passive line
					(at 12.7 -25.4 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "CLK_IN0")
					(number "5")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "CLK_IN1")
					(number "6")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "7")
				)
				(pin passive line
					(at 12.7 -25.4 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SDA")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SCK")
					(number "10")
				)
				(pin tri_state line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "Y0")
					(number "11")
				)
				(pin tri_state line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "Y1")
					(number "12")
				)
				(pin passive line
					(at 12.7 -25.4 90)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "VCCOUT1")
					(number "14")
				)
				(pin tri_state line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "Y2")
					(number "15")
				)
				(pin tri_state line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "Y3")
					(number "16")
				)
				(pin passive line
					(at 12.7 -25.4 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "17")
				)
				(pin power_in line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "VCCOUT2")
					(number "18")
				)
				(pin tri_state line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "Y4")
					(number "19")
				)
				(pin tri_state line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "Y5")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
