(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CSR1010A05-IQQM-R"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CSR1010A05-IQQM-R"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CSR1010A05-IQQM-R"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.qualcomm.com/products/technology/bluetooth/csr101x-series/csr1010?classification=Datasheet#Documentation"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Qualcomm"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CSR1010A05-IQQM-R"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CSR1010A05-IQQM-R_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_BAT")
					(number "1")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 2.54)
					(name "XTAL_32K_OUT")
					(number "2")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 2.54)
					(name "XTAL_32K_IN")
					(number "3")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 2.54)
					(name "WAKE")
					(number "4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(hide yes)
					(name "VDD_CORE")
					(number "5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD_REG_IN")
					(number "6")
				)
				(pin output line
					(at 40.64 0 180)
					(length 2.54)
					(name "RF")
					(number "7")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD_XTAL")
					(number "8")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 2.54)
					(name "XTAL_16M_OUT")
					(number "9")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 2.54)
					(name "XTAL_16M_IN")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "AIO2")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "AIO1")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "AIO0")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "PIO0")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "PIO1")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PIO3")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PIO4")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "PIO5")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PIO6")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PIO7")
					(number "20")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDD_PADS")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PIO8")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PIO9")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PIO10")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PIO11")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SPI_PIO")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PIO2")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "I2C_SCL")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "I2C_SDA")
					(number "29")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VDD_CORE")
					(number "30")
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 2.54)
					(name "SMPS_LX")
					(number "31")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VDD_BAT_SMPS")
					(number "32")
				)
				(pin power_in line
					(at 40.64 -73.66 180)
					(length 2.54)
					(name "VSS/PAD")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
