(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CY15B108QN-40SXI"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CY15B108QN-40SXI"
				(at 33.02 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CY15B108QN-40SXI"
				(at 33.02 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/cms/en/product/memories/f-ram-ferroelectric-ram/excelon-f-ram/cy15b108qn-40sxi/"
				(at 33.02 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8Mb 3.3V Industrial 40MHz SPI EXCELON™ F-RAM in 8-pin SOIC"
				(at 33.02 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CY15B108QN-40SXI"
				(at 33.02 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 33.02 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, SPI, MEMORY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CY15B108QN-40SXI_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SO")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{WP}")
					(number "3")
				)
				(pin power_in line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "SI")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "DNU")
					(number "7")
				)
				(pin power_in line
					(at 17.78 0 180)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
