(footprint "TQFP-100_14x20mm_P0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.infineon.com/package/PG-TQFP-100-800")
	(property "Reference" "REF**"
		(at -8.8 -12 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "TQFP-100_14x20mm_P0.65mm"
		(at -8.8 12.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.8 14.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.8 15.3 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.8 16.5 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "1" smd roundrect
		(at -7.725 -9.425 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "2" smd roundrect
		(at -7.725 -8.775 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "3" smd roundrect
		(at -7.725 -8.125 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "4" smd roundrect
		(at -7.725 -7.475 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "5" smd roundrect
		(at -7.725 -6.825 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "6" smd roundrect
		(at -7.725 -6.175 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "7" smd roundrect
		(at -7.725 -5.525 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "8" smd roundrect
		(at -7.725 -4.875 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "9" smd roundrect
		(at -7.725 -4.225 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "10" smd roundrect
		(at -7.725 -3.575 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "11" smd roundrect
		(at -7.725 -2.925 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "12" smd roundrect
		(at -7.725 -2.275 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "13" smd roundrect
		(at -7.725 -1.625 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "14" smd roundrect
		(at -7.725 -0.975 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "15" smd roundrect
		(at -7.725 -0.325 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "16" smd roundrect
		(at -7.725 0.325 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "17" smd roundrect
		(at -7.725 0.975 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "18" smd roundrect
		(at -7.725 1.625 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "19" smd roundrect
		(at -7.725 2.275 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "20" smd roundrect
		(at -7.725 2.925 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "21" smd roundrect
		(at -7.725 3.575 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "22" smd roundrect
		(at -7.725 4.225 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "23" smd roundrect
		(at -7.725 4.875 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "24" smd roundrect
		(at -7.725 5.525 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "25" smd roundrect
		(at -7.725 6.175 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "26" smd roundrect
		(at -7.725 6.825 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "27" smd roundrect
		(at -7.725 7.475 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "28" smd roundrect
		(at -7.725 8.125 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "29" smd roundrect
		(at -7.725 8.775 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "30" smd roundrect
		(at -7.725 9.425 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "31" smd roundrect
		(at -6.175 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "32" smd roundrect
		(at -5.525 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "33" smd roundrect
		(at -4.875 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "34" smd roundrect
		(at -4.225 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "35" smd roundrect
		(at -3.575 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "36" smd roundrect
		(at -2.925 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "37" smd roundrect
		(at -2.275 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "38" smd roundrect
		(at -1.625 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "39" smd roundrect
		(at -0.975 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "40" smd roundrect
		(at -0.325 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "41" smd roundrect
		(at 0.325 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "42" smd roundrect
		(at 0.975 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "43" smd roundrect
		(at 1.625 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "44" smd roundrect
		(at 2.275 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "45" smd roundrect
		(at 2.925 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "46" smd roundrect
		(at 3.575 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "47" smd roundrect
		(at 4.225 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "48" smd roundrect
		(at 4.875 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "49" smd roundrect
		(at 5.525 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "50" smd roundrect
		(at 6.175 10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "51" smd roundrect
		(at 7.725 9.425 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "52" smd roundrect
		(at 7.725 8.775 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "53" smd roundrect
		(at 7.725 8.125 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "54" smd roundrect
		(at 7.725 7.475 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "55" smd roundrect
		(at 7.725 6.825 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "56" smd roundrect
		(at 7.725 6.175 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "57" smd roundrect
		(at 7.725 5.525 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "58" smd roundrect
		(at 7.725 4.875 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "59" smd roundrect
		(at 7.725 4.225 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "60" smd roundrect
		(at 7.725 3.575 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "61" smd roundrect
		(at 7.725 2.925 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "62" smd roundrect
		(at 7.725 2.275 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "63" smd roundrect
		(at 7.725 1.625 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "64" smd roundrect
		(at 7.725 0.975 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "65" smd roundrect
		(at 7.725 0.325 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "66" smd roundrect
		(at 7.725 -0.325 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "67" smd roundrect
		(at 7.725 -0.975 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "68" smd roundrect
		(at 7.725 -1.625 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "69" smd roundrect
		(at 7.725 -2.275 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "70" smd roundrect
		(at 7.725 -2.925 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "71" smd roundrect
		(at 7.725 -3.575 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "72" smd roundrect
		(at 7.725 -4.225 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "73" smd roundrect
		(at 7.725 -4.875 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "74" smd roundrect
		(at 7.725 -5.525 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "75" smd roundrect
		(at 7.725 -6.175 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "76" smd roundrect
		(at 7.725 -6.825 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "77" smd roundrect
		(at 7.725 -7.475 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "78" smd roundrect
		(at 7.725 -8.125 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "79" smd roundrect
		(at 7.725 -8.775 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "80" smd roundrect
		(at 7.725 -9.425 90)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "81" smd roundrect
		(at 6.175 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "82" smd roundrect
		(at 5.525 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "83" smd roundrect
		(at 4.875 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "84" smd roundrect
		(at 4.225 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "85" smd roundrect
		(at 3.575 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "86" smd roundrect
		(at 2.925 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "87" smd roundrect
		(at 2.275 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "88" smd roundrect
		(at 1.625 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "89" smd roundrect
		(at 0.975 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "90" smd roundrect
		(at 0.325 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "91" smd roundrect
		(at -0.325 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "92" smd roundrect
		(at -0.975 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "93" smd roundrect
		(at -1.625 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "94" smd roundrect
		(at -2.275 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "95" smd roundrect
		(at -2.925 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "96" smd roundrect
		(at -3.575 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "97" smd roundrect
		(at -4.225 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "98" smd roundrect
		(at -4.875 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "99" smd roundrect
		(at -5.525 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(pad "100" smd roundrect
		(at -6.175 -10.725)
		(size 0.45 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.02)
	)
	(embedded_fonts no)
	(model "antmicro_cyrs17b512_133azmb.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
