(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CYRS17B512-133AZMB"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CYRS17B512-133AZMB"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CYRS17B512-133AZMB"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/assets/row/public/documents/10/49/infineon-cyrs17b512-512-mb-64-mb-serial-nor-flash-spi-qspi-3-datasheet-en.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation hardened FLASH - NOR Memory IC, 512Mbit SPI - Quad I/O, 133 MHz, TQFP-100 (14x20)"
				(at 40.64 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "CYRS17B512-133AZMB"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, SPI, FLASH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CYRS17B512-133AZMB_1_1"
				(pin power_in line
					(at 26.67 -2.54 180)
					(length 3.81)
					(name "VDDIO")
					(number "1")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "~{RESET}")
					(number "7")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "~{CS}")
					(number "8")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "9")
				)
				(pin power_in line
					(at 26.67 0 180)
					(length 3.81)
					(name "VDD")
					(number "10")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "11")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "SI")
					(number "12")
					(alternate "IO0" passive line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "SO")
					(number "13")
					(alternate "IO1" passive line)
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "14")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "15")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SCK")
					(number "16")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "17")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "~{WP}")
					(number "19")
					(alternate "IO2" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "IO3")
					(number "20")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "21")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "22")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "23")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 3.81)
					(name "~{INT}")
					(number "24")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "25")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "26")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "27")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "29")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VDDIO")
					(number "30")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "31")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "32")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "33")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "34")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "39")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "40")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "41")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "42")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "43")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "44")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "47")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "49")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "50")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "51")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "52")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "53")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "54")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "55")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "56")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "57")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "58")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "59")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "60")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "61")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "62")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "63")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "64")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "65")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "66")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "67")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "68")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "69")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "70")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "71")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "72")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "73")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "74")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "75")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "76")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "77")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "78")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "79")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "80")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "81")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "82")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "83")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "84")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "85")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "86")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "87")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "88")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "89")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "90")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "91")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "92")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "93")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "94")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "95")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "96")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "97")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "98")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "DNU")
					(number "99")
				)
				(pin passive line
					(at 26.67 -17.78 180)
					(length 3.81)
					(name "VSS")
					(number "100")
				)
			)
			(embedded_fonts no)
		)
)
