(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DP83848JSQ_NOPB"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 49.53 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DP83848JSQ_NOPB"
				(at 49.53 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DP83848JSQ_NOPB"
				(at 49.53 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dp83848j.pdf?ts=1730717224532&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FDP83848J%252Fpart-details%252FDP83848JSQ%252FNOPB%253Futm_source%253Dgoogle%2526utm_medium%253Dcpc%2526utm_campaign%253Docb-tistore-promo-asc_opn_en-cpc-storeic-google-wwe%2526utm_content%253DDevice%2526ds_k%253DDP83848JSQ%252FNOPB%2526DCM%253Dyes%2526gad_source%253D1%2526gclid%253DCj0KCQiA_qG5BhDTARIsAA0UHSL9ea5GSgyVbQyTSXRIZYE0ABJYc6_W5Zf9Ukm4C-26GJoRYGjZcvIaAnmDEALw_wcB%2526gclsrc%253Daw.ds"
				(at 49.53 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Robust, High Immunity 10/100/1000 Ethernet Physical Layer Transceiver"
				(at 49.53 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DP83848JSQ_NOPB"
				(at 49.53 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 49.53 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 49.53 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 49.53 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, ETHERNET, IC, TRANSCEIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DP83848JSQ_NOPB_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IOVDD33")
					(number "1")
				)
				(pin output clock
					(at 0 -50.8 0)
					(length 2.54)
					(name "TX_CLK")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "TX_EN")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "TXD_0")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "TXD_1")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "TXD_2")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "TXD_3")
					(number "7")
				)
				(pin no_connect line
					(at 33.02 -52.07 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "8")
				)
				(pin no_connect line
					(at 33.02 -50.8 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "9")
				)
				(pin no_connect line
					(at 33.02 -49.53 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "10")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 2.54)
					(name "RD–")
					(number "11")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 2.54)
					(name "RD+")
					(number "12")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 2.54)
					(name "AGND")
					(number "13")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 2.54)
					(name "TD-")
					(number "14")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 2.54)
					(name "TD+")
					(number "15")
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "PFBIN1")
					(number "16")
				)
				(pin passive line
					(at 35.56 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "17")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "AVDD33")
					(number "18")
				)
				(pin output line
					(at 35.56 0 180)
					(length 2.54)
					(name "PFBOUT")
					(number "19")
				)
				(pin input line
					(at 35.56 -45.72 180)
					(length 2.54)
					(name "RBIAS")
					(number "20")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "LED_SPEED")
					(number "21")
					(alternate "AN1" passive line)
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 2.54)
					(name "LED_LINK")
					(number "22")
					(alternate "AN0" passive line)
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RESET_N")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "MDIO")
					(number "24")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MDC")
					(number "25")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IOVDD33")
					(number "26")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "X2")
					(number "27")
				)
				(pin input line
					(at 35.56 -35.56 180)
					(length 2.54)
					(name "X1")
					(number "28")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 2.54)
					(name "DGND")
					(number "29")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "PFBIN2")
					(number "30")
				)
				(pin output clock
					(at 0 -30.48 0)
					(length 2.54)
					(name "RX_CLK")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RX_DV")
					(number "32")
					(alternate "MII_MODE" passive line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "CRS")
					(number "33")
					(alternate "CRS_DV" passive line)
					(alternate "LED_CFG" passive line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RX_ER")
					(number "34")
					(alternate "MDIX_EN" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "COL")
					(number "35")
					(alternate "PHYAD0" passive line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RXD_0")
					(number "36")
					(alternate "PHYAD1" passive line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "RXD_1")
					(number "37")
					(alternate "PHYAD2" passive line)
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "RXD_2")
					(number "38")
					(alternate "PHYAD3" passive line)
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "RXD_3")
					(number "39")
					(alternate "PHYAD4" passive line)
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 2.54)
					(name "IOGND")
					(number "40")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 2.54)
					(name "EP")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
