(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DP83867CR_VQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DP83867CR_VQFN"
				(at 71.12 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DP83867CR_VQFN"
				(at 71.12 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dp83867ir.pdf?ts=1647232328899&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FDP83867IR"
				(at 71.12 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Robust, High Immunity 10/100/1000 Ethernet Physical Layer Transceiver"
				(at 71.12 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 71.12 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DP83867CRRGZR"
				(at 71.12 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 71.12 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, ETHERNET, IC, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "RGZ0048B RGZ0048B_NV"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DP83867CR_VQFN_1_1"
				(text "10/100/1000"
					(at 21.59 0 0)
				)
				(text "Ethernet PHY"
					(at 21.59 -2.54 0)
				)
				(pin bidirectional line
					(at 44.45 -10.16 180)
					(length 2.54)
					(name "TD_P_A")
					(number "1")
				)
				(pin bidirectional line
					(at 44.45 -12.7 180)
					(length 2.54)
					(name "TD_M_A")
					(number "2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDA2P5")
					(number "3")
				)
				(pin bidirectional line
					(at 44.45 -17.78 180)
					(length 2.54)
					(name "TD_P_B")
					(number "4")
				)
				(pin bidirectional line
					(at 44.45 -20.32 180)
					(length 2.54)
					(name "TD_M_B")
					(number "5")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "VDD1P0")
					(number "6")
				)
				(pin bidirectional line
					(at 44.45 -25.4 180)
					(length 2.54)
					(name "TD_P_C")
					(number "7")
				)
				(pin bidirectional line
					(at 44.45 -27.94 180)
					(length 2.54)
					(name "TD_M_C")
					(number "8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDA2P5")
					(number "9")
				)
				(pin bidirectional line
					(at 44.45 -33.02 180)
					(length 2.54)
					(name "TD_P_D")
					(number "10")
				)
				(pin bidirectional line
					(at 44.45 -35.56 180)
					(length 2.54)
					(name "TD_M_D")
					(number "11")
				)
				(pin passive line
					(at 44.45 -59.69 180)
					(length 2.54)
					(name "RBIAS")
					(number "12")
				)
				(pin power_in line
					(at 44.45 -2.54 180)
					(length 2.54)
					(name "VDDA1P8")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 2.54)
					(name "X_O")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 2.54)
					(name "X_I")
					(number "15")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MDC")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MDIO")
					(number "17")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "CLK_OUT")
					(number "18")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "19")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 2.54)
					(name "JTAG_CLK")
					(number "20")
				)
				(pin output line
					(at 0 -57.15 0)
					(length 2.54)
					(name "JTAG_TDO")
					(number "21")
				)
				(pin input line
					(at 0 -62.23 0)
					(length 2.54)
					(name "JTAG_TMS")
					(number "22")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 2.54)
					(name "JTAG_TDI")
					(number "23")
				)
				(pin power_in line
					(at 44.45 0 180)
					(length 2.54)
					(name "VDD1P0")
					(number "24")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "TX_D3")
					(number "25")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TX_D2")
					(number "26")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "TX_D1")
					(number "27")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TX_D0")
					(number "28")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GTX_CLK")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "30")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "VDD1P0")
					(number "31")
				)
				(pin output line
					(at 0 -46.99 0)
					(length 2.54)
					(name "RX_CLK")
					(number "32")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 2.54)
					(name "RX_D0")
					(number "33")
				)
				(pin output line
					(at 0 -39.37 0)
					(length 2.54)
					(name "RX_D1")
					(number "34")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 2.54)
					(name "RX_D2")
					(number "35")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 2.54)
					(name "RX_D3")
					(number "36")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "TX_EN_TX_CTRL")
					(number "37")
				)
				(pin output line
					(at 0 -34.29 0)
					(length 2.54)
					(name "RX_DV_RX_CTRL")
					(number "38")
				)
				(pin output line
					(at 44.45 -52.07 180)
					(length 2.54)
					(name "GPIO_0")
					(number "39")
				)
				(pin output line
					(at 44.45 -54.61 180)
					(length 2.54)
					(name "GPIO_1")
					(number "40")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "41")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "VDD1P0")
					(number "42")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "RESET_N")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "INT_PWDN")
					(number "44")
				)
				(pin bidirectional line
					(at 44.45 -46.99 180)
					(length 2.54)
					(name "LED_2")
					(number "45")
				)
				(pin bidirectional line
					(at 44.45 -44.45 180)
					(length 2.54)
					(name "LED_1")
					(number "46")
				)
				(pin bidirectional line
					(at 44.45 -41.91 180)
					(length 2.54)
					(name "LED_0")
					(number "47")
				)
				(pin power_in line
					(at 44.45 -5.08 180)
					(length 2.54)
					(name "VDDA1P8")
					(number "48")
				)
				(pin power_in line
					(at 44.45 -72.39 180)
					(length 2.54)
					(name "PAD")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
