(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DP83867ERGZR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 64.77 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DP83867ERGZR"
				(at 64.77 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DP83867ERGZR"
				(at 64.77 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dp83867is.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1704962980288&ref_url=https%253A%252F%252Fwww.ti.com%252Fgeneral%252Fdocs%252Fsuppproductinfo.tsp%253FdistId%253D10%2526gotoUrl%253Dhttps%253A%252F%252Fwww.ti.com%252Flit%252Fgpn%252Fdp83867is"
				(at 64.77 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Robust, High Immunity, Small Form Factor 10/100/1000 Ethernet, Physical Layer Transceiver, SGMII/RGMII"
				(at 64.77 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DP83867ERGZR"
				(at 64.77 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 64.77 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 64.77 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 64.77 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, ETHERNET, IC, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "RGZ0048B RGZ0048B_NV"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DP83867ERGZR_1_1"
				(pin bidirectional line
					(at 34.29 0 180)
					(length 2.54)
					(name "TD_P_A")
					(number "1")
				)
				(pin bidirectional line
					(at 34.29 -2.54 180)
					(length 2.54)
					(name "TD_M_A")
					(number "2")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 2.54)
					(name "VDDA2P5")
					(number "3")
				)
				(pin bidirectional line
					(at 34.29 -6.35 180)
					(length 2.54)
					(name "TD_P_B")
					(number "4")
				)
				(pin bidirectional line
					(at 34.29 -8.89 180)
					(length 2.54)
					(name "TD_M_B")
					(number "5")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "VDD1P0")
					(number "6")
				)
				(pin bidirectional line
					(at 34.29 -12.7 180)
					(length 2.54)
					(name "TD_P_C")
					(number "7")
				)
				(pin bidirectional line
					(at 34.29 -15.24 180)
					(length 2.54)
					(name "TD_M_C")
					(number "8")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "VDDA2P5")
					(number "9")
				)
				(pin bidirectional line
					(at 34.29 -19.05 180)
					(length 2.54)
					(name "TD_P_D")
					(number "10")
				)
				(pin bidirectional line
					(at 34.29 -21.59 180)
					(length 2.54)
					(name "TD_M_D")
					(number "11")
				)
				(pin passive line
					(at 34.29 -26.67 180)
					(length 2.54)
					(name "RBIAS")
					(number "12")
				)
				(pin power_in line
					(at 0 -6.35 0)
					(length 2.54)
					(name "VDDA1P8")
					(number "13")
				)
				(pin output line
					(at 0 -64.77 0)
					(length 2.54)
					(name "X_O")
					(number "14")
				)
				(pin input line
					(at 0 -62.23 0)
					(length 2.54)
					(name "X_I")
					(number "15")
				)
				(pin input line
					(at 34.29 -54.61 180)
					(length 2.54)
					(name "MDC")
					(number "16")
				)
				(pin bidirectional line
					(at 34.29 -57.15 180)
					(length 2.54)
					(name "MDIO")
					(number "17")
				)
				(pin output line
					(at 0 -68.58 0)
					(length 2.54)
					(name "CLK_OUT")
					(number "18")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "19")
				)
				(pin input line
					(at 34.29 -36.83 180)
					(length 2.54)
					(name "JTAG_CLK")
					(number "20")
				)
				(pin output line
					(at 34.29 -34.29 180)
					(length 2.54)
					(name "JTAG_TDO")
					(number "21")
				)
				(pin input line
					(at 34.29 -39.37 180)
					(length 2.54)
					(name "JTAG_TMS")
					(number "22")
				)
				(pin input line
					(at 34.29 -31.75 180)
					(length 2.54)
					(name "JTAG_TDI")
					(number "23")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 2.54)
					(name "VDD1P0")
					(number "24")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "TX_D3")
					(number "25")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "TX_D2")
					(number "26")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "TX_D1/SGMII_SIP")
					(number "27")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "TX_D0/SGMII_SIN")
					(number "28")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GTX_CLK")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "30")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "VDD1P0")
					(number "31")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RX_CLK")
					(number "32")
				)
				(pin output line
					(at 0 -36.83 0)
					(length 2.54)
					(name "RX_D0/SGMII_COP")
					(number "33")
				)
				(pin output line
					(at 0 -39.37 0)
					(length 2.54)
					(name "RX_D1/SGMII_CON")
					(number "34")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 2.54)
					(name "RX_D2/SGMII_SOP")
					(number "35")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 2.54)
					(name "RX_D3/SGMII_SON")
					(number "36")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TX_CTRL")
					(number "37")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "RX_CTRL")
					(number "38")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 2.54)
					(name "GPIO_0")
					(number "39")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "GPIO_1")
					(number "40")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "41")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "VDD1P0")
					(number "42")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "~{RESET}")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 2.54)
					(name "~{INT}/~{PWDN}")
					(number "44")
				)
				(pin bidirectional line
					(at 34.29 -49.53 180)
					(length 2.54)
					(name "LED_2")
					(number "45")
				)
				(pin bidirectional line
					(at 34.29 -46.99 180)
					(length 2.54)
					(name "LED_1")
					(number "46")
				)
				(pin bidirectional line
					(at 34.29 -44.45 180)
					(length 2.54)
					(name "LED_0")
					(number "47")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "VDDA1P8")
					(number "48")
				)
				(pin power_in line
					(at 34.29 -68.58 180)
					(length 2.54)
					(name "GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
