(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DS2003CM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DS2003CM"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DS2003CM"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/1158/DS2003.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "IC driver 6/0 16SOIC"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DS2003CM"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DS2003CM_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "In_1")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "In_2")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "In_3")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "In_4")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "In_5")
					(number "5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "In_6")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "In_7")
					(number "7")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at 16.51 -17.78 180)
					(length 2.54)
					(name "Com")
					(number "9")
				)
				(pin input line
					(at 16.51 -15.24 180)
					(length 2.54)
					(name "Out_1")
					(number "10")
				)
				(pin input line
					(at 16.51 -12.7 180)
					(length 2.54)
					(name "Out_6")
					(number "11")
				)
				(pin input line
					(at 16.51 -10.16 180)
					(length 2.54)
					(name "Out_5")
					(number "12")
				)
				(pin input line
					(at 16.51 -7.62 180)
					(length 2.54)
					(name "Out_4")
					(number "13")
				)
				(pin input line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "Out_3")
					(number "14")
				)
				(pin input line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "Out_2")
					(number "15")
				)
				(pin input line
					(at 16.51 0 180)
					(length 2.54)
					(name "Out_1")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
