(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DS90LV028ATM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.322 -2.286 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DS90LV028ATM"
				(at 36.322 -7.366 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DS90LV028ATM"
				(at 36.322 -9.906 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ds90lv028a.pdf?ts=1754038864407&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 36.322 -12.446 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LVDS Dual CMOS Differential Line Receiver, 3.3V, SOIC-8, 400Mbps"
				(at 36.322 -25.146 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 36.322 -17.526 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DS90LV028ATM/NOPB"
				(at 36.322 -4.826 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 36.322 -20.066 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.322 -22.606 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, LVDS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DS90LV028ATM_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RIN1-")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "RIN1+")
					(number "2")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "RIN2+")
					(number "3")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "RIN2-")
					(number "4")
				)
				(pin power_in line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin output line
					(at 20.32 -6.35 180)
					(length 2.54)
					(name "ROUT2")
					(number "6")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "ROUT1")
					(number "7")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
